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MODEL : 8채널 AI Box (AIB-800)

1. 개 요
AIB-800은 8채널 AI Box 입니다.
2. 제 원 
1) 비디오 입력  : 8채널, CIF ~ 32MP, 프로토콜 : SUNAPI, ONVIF
2) AI 분석 기능
Classified object type : Person/Vehicle
Attributes : Vehicle
(Type:car/bus/truck/motorcycle/bicycle)
Support Bestshot
Analytics events based on AI engine:
- Motion Detection*, Object detection, Virtual line*
(Crossing/Direction),
Virtual area* (Loitering/Intrusion/Enter/Exit)
* Some of the video analytics only works with
people/vehicle detection
Analytics events : Virtual area(Appear/Disappear)
Business Intelligence :
- Based on AI engine: People counting, Vehicle counting,
Queuemanagement, Heatmap
3) 프로토콜     : TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP, HTTP, DHCP (Server, Client), 
SMTP, ICMP, IGMP, ARP, DNS, DDNS, uPnP, HTTPS, SNMP, ONVIF (Profile-S), 
SUNAPI(Server, Client), SRTP
4) DDNS         : Hanwha DDNS
5) 최대 조작 스트림 : 80 Streams ( 10 Streams per 1CH)
6) 지원언어    : English, French, German, Italian, Spanish, Russian, Turkish, Polish, Dutch,
Czech, Portuguese, Hungarian, Greek, Korean, Chinese, Japanese
7) 운영체제    : Windows 11/10, macOS 10.13
8) 지원 웹브라우저 : Google Chrome, Microsoft Edge, Mac Safari 
9) 뷰어 SW       : WebViewer, WAVE, SSM, Genetec, Milestone
10) CMS 지원   : Support SDK/CGI(SUNAPI) for interworking with 3'rd party VMS
11) 인터페이스
· 인디케이터  : LED(Status indicator) : - Alarm(1), Power(1), Network(1)
· 이더넷      : RJ-45 1ea (1Gbps)
· 알람        : (1) In(8EA, Terminal Block)
(2) Alarm Reset(1EA)
(3) Out(4EA, Terminal Block)
-> Relay Out1(NO/NC/COM)
-> Relay Out2~4(NO/COM)
        - USB           : 1EA( Rear 1 x USB 3.0) for DEBUG
        - Serial          : Not Supported (internal Debug)
        - Reset          : Factory Reset
        - 전원코드       : DIN 4P 12V, 4A
   12) CPU            : NVIDIA ORIN NX 8GB (SOM)
   13) 작동 온도/습도  : +0°C to +40°C(+32℉ to +104℉) / 20% ~ 85% RH
   14) 전원            : 100 ~ 240 VAC ±10%; 50/60 Hz, 12V, 4A Adaptor, 28W
   15) 사이즈/무게     : 300 x 47.6 x 240.9 mm (11.81 x 1.87 x 9.48 inch) / 1.39kg

http://www.hanwhavision.com/
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