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MODEL : Dual lens BCR camera (TNS-9060IBC)

1. 개 요
TNS-9060IBC은 4K (COLOR&MONO) 해상도, 35mm 렌즈 Wide FoV, AI 기반 바코드 인식을 하는 Dual lens BCR 카메라 입니다.

2. 제 원 

 1) 촬상소자    : Global Shutter Mono 1" CMOS, Global Shutter Color 1" CMOS
 2) 해상도      : Mono: Max 4096x2160, Color: Max 4096x2160
 3) 최대 프레임레이트 : Mono: Max 20fps, Color: Max 20fps
 4) 픽셀사이즈  : 3.45μm(H)×3.45μm(V)
 5) 렌즈        : 35mm, Mono: F8.0, Color: F8.0, C Mount
 6) 화각        : Mono: H21.5° / V11.5° / D24.2°, Color: H21.5° / V11.5° / D24.2°
 7) 최소 지근거리 : 0.2m (0.66ft)
 8) 보정        : Gain Control (Manual, 0~48dB), 노이즈 제거(SSNR V), 화이트발란스(AWC, 
수동), 영상회전(Flip, Mirror)
 9) 전자셔터    : Manual, 1/10,000~1/30s (100us ~ 33.33ms)
 10) 지능형 분석
     Barcode 인식
 Barcode type: Barcode type: 1D Code, Code128 / CODE39 / CODE93 / Codabar / 
ITF(Interleaved 2 of 5) / UPC / EAN
 11) 이더넷 : M12 8pin connector (10/100/1000BASE-T)
 12) 보안
OS/펌웨어 보호 : Secure boot, Signed firmware, Firmware encryption
사용자 인증     : Digest Authentication, Privent brute-force attack
네트워크 인증   : 802.1X Authentication(EAP-TLS, EAP-LEAP, EAP-PEAP MSCHAPv2)
암호통신        : HTTPS, SRTP, WSS(Websocket secure)
접근제어        : IP address filtering
데이터 보호     : Authentication information encryption, ZIP compression encryption
감사(audit)      : User Access/System/Event log
Device ID       : Device Certificate(Hanwha Techwin Root CA, pre-installed)
Secure Storage  : HTPM (Hanwha Trusted Platform Module)
보안인증       : Secure by default
 13) 프로토콜      : IPv4, IPv6, TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP, RTSP, NTP, HTTP, 
HTTPS, SSL/TLS, DHCP, FTP, SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), 
ARP, DNS, DDNS, QoS, UPnP, Bonjour, SRTP (TCP, UDP Unicast)
 14) 응용인터페이스 : SUNAPI(HTTP API), Wisenet Open Platform
 15) 동작 온/습도  : -40°C~+55°C(-40°F ~ +131°F) / 0~95% RH, 
* Start up should be done at above -30°C, 
NEMA TS-2: 74°C - / 0~95% RH
 16) 규격인증  : IP67, IP66, IK10(Exclude Window), NAME 4X
17) 전원       : 24VDC, M12 12pin connector, Max 35.4W, Typical 13.7W, 
* Max: LED On / Typical: LED Off
18) 외관        : Black / Aluminum, Camera: 218x104.1x127.1mm, 1897g
LED: 255.8x73.8x49.8mm, 996g
Total: 255.8x181x127.1mm, 3438g(with install bracket)

http://www.hanwha-security.com/
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