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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com
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PART  1  PRODUCTS
1.01 EQUIPMENT
A. Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
B. Model: HCB-6001
C. Alternates: None
1.02 GENERAL DESCRIPTION
A. [bookmark: _Toc173721624]Video – 2MP (1920x1080) resolution at 30 fps(N), 25 fps(P)
B. Camera – The 2MP analog camera device shall have the following physical and performance properties:
1. Auto day/night operation with removable IR cut filter
a. Low light level operation to 0.09 lux (color) and 0.009 lux (black and white)
2. Digital Wide Dynamic Range, providing a wide range between dark and light areas visible at the same time
3. Digital noise reduction
4. Digital zoom
5. 4 privacy masking regions utilizing a 4 point polygon
6. Digital image stabilization
C. Intelligence and Analytics – The camera shall have a suite of integral intelligent operations and analytic functions to include:
1. Motion detection with four definable detection areas, minimum / maximum object size definition and a learning algorithm that ignores false alarms such as trees and waves on water.
1.03 DETAILED SPECIFICATIONS
A. Video
1. Imager
a. Sensor: 1/2.8" 2 MP CMOS
1) pixels per sensor: 1,945 (H) x 1,109 (V) total, 1,945 (H) x 1,097 (V) effective
2) scanning: progressive
b. Minimum illumination
1) Color mode: 0.09Lux (F1.2, 1/30sec)
2) Black & white mode: 0.009Lux (F1.2, 1/30sec)
c. Scanning System: Progressive Scan
d. Signal: Noise ratio: 52 dB
e. Video Output: BNC(AHD, CVBS, TVI, CVI selectable)
f. Resolution: 1920 x 1080
g. Maximum Frame rate: 30fps at 1920x1080
h. The following features with control settings shall be available:
1) On Screen Display: English, Spanish, French, Portuguese, German, Italian, Russian, Polish, Czech, Romanian, Serbian, Swedish, Danish, Turkish
2) Camera Title: On / Off (up to 15 characters)
3) Day / Night: Auto (ICR) / Color / BW
4) Backlight compensation (BLC): Off / User BLC / HLC
5) Wide Dynamic Range: 120dB
6) Digital Noise Reduction (DNR): On / Off (SSNR IV)
7) Motion detection: 4 zones with 4 sided polygon
8) Privacy masking: 4 zones with 4 sided polygon
9) Gain control: 4 levels or Off
10) White Balance: ATW / Outdoor / Indoor / Manual / AWC (1,800K° ~ 10,500K°)
11) Electronic shutter speed: NTSC:1 - 1/12,000 sec
12) Reverse: Off / H-Rev / V-Rev / HV-Rev
i. Lens: Not included
1) Mount Type: C / CS
2. Video Transmission Distance: 500m (1640.42 ft.) (5C2V coaxial cable)
B. Protocol
1. Remote Control Interface: Coaxial control
2. Protocols
a. AHD:ACP(AHD Coax Protocol)
b. CVBS: Pelco-C(Coaxitron), CCP(CVI Coax Protocol), TCP(TVI Coax Protocol)
3. Serial Interface: RS-485(Samsung-T, Pelco-D/P, Panasonic, Bosch, AD, GE, Vicon, Honeywell)
C. Alarm: (MD) output 1
D. Electrical
a. Input Voltage and Current: Dual (24V AC & 12V DC +-10%)
b. Power Consumption: Maximum 6W
E. Mechanical And Environmental
1. Material: Housing(Plastic)
2. Dimensions (W x H x D): 73.1 x 67.2.6 x 130.9 mm (2.88 x 2.65 x 5.15 in.)
3. Weight: 287g (0.63 lb.)
4. Operating Temperature: -10° C to 55° C (14° F to 131° F)
5. Humidity: 0 - 90%, non-condensing
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