GUIDE SPECIFICATION

MasterFormat 2014: Section 28 23 29

MasterFormat 2016: Section 28 2x xx
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Hanwha Techwin is a leading supplier of advanced video surveillance solutions for IP-video, analog and hybrid systems. Building on the company's history of innovation, Hanwha Techwin is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-efficiency. Hanwha Techwin is committed to the continued development of innovative systems products for professional security applications.

For additional information, visit http://security.hanwhatechwin.com/ 

1080p ANALOG HD 32x PTZ DOME CAMERA
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
Notes to Specifier:

1.  Where several alternative parameters or specifications exist, or where, the specifier has the option of inserting text, such choices are presented in <bold text>.
2.  Explanatory notes and comments are presented in colored text.

Important:  See further notes on the following page.

Important Note to Security Systems Specifiers

CSI MasterFormat 2016 incorporates numerous significant changes affecting electronic safety and security. This document is written to provide flexibility in using either format, although adoption of MasterFormat 2016 is encouraged. The following is a guide to the MasterFormat numbers relevant to the product referenced in this specification.

Primary Specification Area:

MasterFormat 2014:

28 20 00 
Electronic Surveillance

28 23 00 
Video Surveillance




28 23 29
Video Surveillance Remote Devices and Sensors

MasterFormat 2016:

28 20 00
Video Surveillance



28 2x xx
Surveillance Cameras




28 2x xx
IP Cameras

Related Requirements:

MasterFormat 2014:


27 20 00 Data Communications 


28 23 13 Video Surveillance Control and Management Systems


28 23 16 Video Surveillance Monitoring and Supervisory Interfaces


28 23 19 Digital Video Recorders and Analog Recording Devices


28 23 23 Video Surveillance Systems Infrastructure
MasterFormat 2016


27 15 01.xx
Video Surveillance Communications Conductors and Cables 

27 20 00 
Data Communications 

28 05 xx.xx
PoE Power Sources for Electronic Safety and Security 

28 05 xx
Storage Appliances for Electronic Safety and Security 


28 05 xx.xx
Network Video Recorders 

28 05 xx
Cyber Requirements for Electronic Safety and Security


28 05 xx
Safety and Security Network Communications Equipment 

28 2x 00
Video Management System
1080p ANALOG HD 32x PTZ DOME CAMERA
PART  1   GENERAL

1.01 SUMMARY
A. Section includes a 1080p analog HD PTZ camera with 32x zoom ratio. 
B. Product – An analog PTZ camera in an IP66 and IK10 housing.
C. Related Requirements
Refer to MasterFormat notes at the beginning of this document to select requirements specific to the MasterFormat version being used in the specification.

1.02 REFERENCES
A. Abbreviations
1. AGC - Automatic Gain Control
2. ARP – Address Resolution Protocol
3. AWB  - Automatic White Balance
4. BLC – Back light compression
5. CBR – Constant Bit Rate

6. CVBS – Color, Video, Blanking, Sync
7. DHCP - Dynamic Host Configuration Protocol
8. DNR – Digital Noise Reduction
9. DNS - Domain Name Server
10. DDNS – Dynamic Domain Name Server
11. DSCP – Differentiated Services Code Point
12. fps - frames per second
13. FTP - File Transfer Protocol
14. GOV – Group of Video
15. GUI – Graphical User Interface
16. HD – High Definition
17. HTTP - Hypertext Transfer Protocol
18. ICMP – Internet Control Message Protocol
19. IGMP - Internet Group Management Protocol
20. IP - Internet Protocol
21. JPEG - Joint Photographic Experts Group
22. MJPEG - Motion JPEG
23. MP - Megapixel
24. MPEG - Moving Pictures Experts Group
25. NAS – Network Attached Storage
26. NTP - Network Time Protocol
27. PIM-SM - Protocol Independent Multicast-Sparse Mode

28. PoE - Power over Ethernet
29. PPPoE – Point to Point Protocol over Ethernet
30. RTP - Real-Time Transport Protocol
31. RTCP – Real-Time Control Protocol
32. RTSP - Real-Time Streaming Protocol
33. SDK – Software Development Kit
34. SMTP - Simple Mail Transfer Protocol
35. SNMP – Simple Network Management Protocol
36. SSL – Secure Sockets Layer
37. TCP - Transmission Control Protocol
38. UDP - User Datagram Protocol
39. UPnP – Universal Plug and Play
40. VBR – Variable Bit Rate
41. VMS - Video Management System
42. WDR – Wide Dynamic Range
43. DWDR – Digital Wide Dynamic Range
B. Reference Standards
1. Emissions
a. FCC-47 CFR Part 15 Subpart B Class B
b. CE EN 55022:2010
2. Immunity - CE

a. EN 50130-4:2011 

b. EN 61000-3-3:2014 

c. EN 61000-4-2:2009

d. EN 61000-4-3:2006+A2:2010

e. EN 61000-4-4:2012

f. EN 61000-4-5:2014

g. EN 61000-4-6:2009

3. Safety

a. CE EN 50581:2012 (hazardous substances)
1.03 SUBMITTALS
A. Product Data
1. Manufacturer’s printed or electronic data sheets
2. Manufacturer’s installation and operation manuals
3. Warranty documentation

1.04 QUALIFICATIONS
A. Manufacturer shall have a minimum of five years’ experience in producing video surveillance equipment.
B. Installers shall be trained and authorized by the Manufacturer to install, integrate, test, and commission the system.
1.05 DELIVERY, STORAGE AND HANDLING

A. Deliver the camera in the manufacturer’s original, unopened, undamaged container with identification labels intact. 
1.06 WARRANTY, LICENSING AND SUPPORT
A. Manufacturer shall provide a limited 3 year warranty for the product to be free of defects in material and workmanship.
B. Manufacturer shall provide video analytics embedded in the camera free of license charges.

END OF SECTION

PART  2  PRODUCTS

2.01 EQUIPMENT
A. Manufacturer: 
Hanwha Techwin 
http://security.hanwhatechwin.com/
B. Model

HCP-6320H
C. Alternates: 

None

2.02 GENERAL DESCRIPTION

A. Video Output – BNC (AHD)
1. Resolution


1080p (1920 x 1080)
B. Camera – The 1080p analog PTZ camera device shall have the following physical and performance properties:
1. Auto day/night operation with removable IR cut filter
2. Low light level operation up to 0.0001 lux. 
3. 2D/3D Digital noise reduction

4. 32x zoom ratio
5. 16x digital zoom
6. 120dB WDR
7. Defog
8. 32 rectangular privacy masking regions 
9. Azimuth feature (east, west, south, north, north east, south east, northwest, southwest)
10. RS-485 and PTZ camera control protocol for remote control. (compatible with Techwin’s controllers)
C. Intelligence and Analytics – The camera shall have a suite of integral intelligent operations and analytic functions to include:

1. Tampering
2. Virtual line
3. Enter/Exit
4. Appear/Disappear
2.03 DETAILED SPECIFICATIONS

A. Video
1. Imager
a. Sensor


1/2.8" 2.38M CMOS
1.) pixels per sensor
1952(H) x 1116(V) total; 1944(H) x 1104(V) effective
2.) scanning

progressive
2. Min. illumination


Color: 0.3Lux (1/30sec, F1.6, 50IRE) 
0.005Lux (2sec, F1.6, 50IRE)

B/W:   0.03Lux (1/30sec, F1.6, 50IRE), 
0.0005Lux (2sec, F1.6, 50IRE)

Color: 0.2Lux (1/30sec, F1.6, 30IRE)
0.003Lux (2sec, F1.6, 30IRE)

B/W:  0.01Lux (1/30sec, F1.6, 30IRE)
3. S/N ratio




50dB
a. Video Output



BNC (CVBS / AHD)
1.) Resolution



1920 x 1080
B. Lens

4.44 – 142.6 mm 
1. Optical zoom ratio



32x
2. Maximum aperture ratio   


F1.6 (Wide) / F4.4 (Tele)
3. Angle of view




H: 62.8°(Wide) ~ 2.23°(Tele) 
V: 36.8°(Wide) ~ 1.26˚ (Tele)
4. Minimum Object Distance 


Wide 1.4m (4.59ft.), Tele: 1.9m (6.23ft)
5. Focus control




Auto/Manual/One push
6. Lens/Mount type



DC auto iris / Board-in type
C. Pan/Tilt
1. Pan range




360° endless
2. Pan speed




preset: 700°/sec, manual: 0.024°/sec ~ 200°/sec
3. Tilt range




210° (-15° ~ 195°)
4. Tilt speed




preset: 700°/sec, manual: 0.024°/sec ~ 200°/sec
5. Preset





255 presets
6. Preset accuracy




+-0.2°
7. Azimuth




Yes (E / W / S / N / NE / SE / NW / SW OSD)
D. Operational
1. Camera Title




Off / On (Displayed up to 15 characters)
2. Day / Night




Auto (ICR) / Color / Black and white
3. Backlight compensation (BLC)


Off / BLC / HLC
4. Wide Dynamic Range



120dB
5. Contrast Enhancement



SSDR (Off/On)
6. Digital Noise Reduction (DNR)


SSNRIII (Samsung Super Noise Reduction III)
2D+3D noise filter (Off/On)

7. Digital Image Stabilization


Off / On
8. Defog





Off / Manual / Auto
9. Motion detection



Off / On (4 rectangular zones)
10. Privacy masking



Off / On (32 rectangular zones)
11. Gain control




Off / Low / Middle / High
12. White Balance




ATW / AWC / Manual / Indoor / Outdoor
Mercury / Sodium
13. Electronic shutter speed

 

Minimum / Maximum
Anti-flicker (2~1 / 12,000 sec)
14. Digital zoom




16x
15. Flip/Mirror




Off / On
16. Intelligent video analytics


Tampering, virtual line, enter/exit, (dis)appear
17. Alarm I/O




Input 4ea / Output 2ea (relay)
18. Remote control interface


RS-485
19. Protocol




RS-485: Samsung-T/E, Pelco-P/D, Sungjin, 
Panasonic, Honeywell, AD, Vicon, Bosch, GE
E. Electrical
a. Input Voltage and Current


24V DC +- 10%
b. Power Consumption


Maximum 24W (with heater off)
Maximum 65W (with heater on)
F. Mechanical And Environmental
1. Material



plastic + metal
2. Dimensions (W x H):

220.0 x 293.6mm (8.66 x 11.56in.)
3. Weight:



3.3kg (7.28 lb.)
4. Operating Temperature: 
-50° C to 55° C (-58° F to 131° F)
5. Humidity:


0 - 90%, non-condensing 
6. Environmental Rating:


a. Ingress Protection

IP66
b. Vandal resistance

IK10



END OF SECTION
PART  3    EXECUTION
3.01 INSTALLERS
A. Contractor personnel shall comply with all applicable state and local licensing requirements.
3.02 PREPARATION

A. The design and configuration shall be verified for compatibility and performance with the camera(s). 
B. Configuration shall be tested and qualified by the Contractor prior to camera installation.

C. All firmware found in products shall be the latest and most up-to-date provided by the manufacturer, or of a version as specified by the provider of the Video Management Application (VMA) or Digital Video Recorder (DVR). 

3.03 INSTALLATION
A. The Contractor shall carefully follow instructions in documentation provided by the manufacturer to insure all steps have been taken to provide a reliable, easy-to-operate system.

B. All equipment shall be tested and configured in accordance with instructions provided by the manufacturer prior to installation.

C. Before permanent installation of the system, the Contractor shall test the system in conditions simulating the final installed environment.
3.04 STORAGE

A. The camera hardware shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.
END OF SECTION
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