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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com
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PART  1  PRODUCTS
1.01 EQUIPMENT
A. Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
B. Model: PNP-9200RH
C. Alternates: None
1.02 [bookmark: _Toc173721624]GENERAL DESCRIPTION
A. Video Compression and Transmission – The 4K camera shall have the following properties relating to the video signals it produces.
1. H.265, H.264 and MJPEG compression, each derived from a dedicated encoder and capable of being streamed independently and simultaneously
a. H.265 and H.264 –30 fps at all resolutions
b. MJPEG –15 fps at all resolutions
2. The 4K camera shall be able to configure up to 10 independent video stream profiles with differing encoding, quality, frame rate, resolution, and bit rate settings. 
3. The 4K camera shall be able to stream up to three different profiles. 
4. Resolution selections
a. 3840 x 2160, 2592 x 1944, 2592 x 1464, 1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 800 x 450, 720 x 576, 640 x 480, 640 x 360, 320 x 240, 320 x 180
5. Simultaneous unicast access by up to 15 users
6. Multicast or unicast capable
7. Dynamic DNS (DDNS) support.
8. WiseStream and Dynamic GOV to efficiently manage bitrate of the video stream. 
B. Camera – The 4K camera device shall have the following physical and performance properties:
1. IK10 rated for protection against impacts.
2. Dust proof and water proof (IP66 rated)
3. IR corrected lens that synchronizes the focus location for short (Blue) to long (IR) wavelengths such that, when mixed day-time visible light and night-time IR lights are present, it does not deteriorate (no blurring effect due to out-of-focus).
4. Auto day/night operation with removable IR cut filter
a. Low light level operation to 0.0005 lux (color) and 0 lux (black and white)
5. 2D and 3D digital noise reduction
6. Mechanical anti-vibration for image stabilization
7. True WDR up to 120dB
8. Integral IR illumination, providing effective IR viewable length of 200m.
9. 16 privacy masking regions utilizing polygons with six different coloring.
C. Intelligence and Analytics – The 4K camera shall have a suite of integral intelligent operations and analytic functions to include:
1. Motion detection with four definable detection areas, minimum / maximum object size definition and a learning algorithm that ignores false alarms such as trees and waves on water.
2. Auto tracking for a moving object in a scene. 
3. Detection of logical events of specified conditions from the camera’s video input
a. camera tamper (scene change)
b. virtual line
c. enter/exit
d. appear/disappear
e. audio detection with metadata
D. Interoperability – The 4K camera shall be ONVIF Profile S and G compliant.
E. The 4K camera shall possess the following further characteristics.
1. Built-in web server, accessed via standard browsers including Internet Explorer, Firefox, Chrome & Safari
2. Micro SD/SDHC/SDXC memory card and NAS recording options, with configurable pre-alarm and post-alarm recording intervals
3. Bi-directional audio
4. Alarms and notifications
a. alarm notification triggers
1) alarm input
2) motion detection
3) intelligent video analytics
4) network disconnect
b. available notification means upon trigger
1) file upload via FTP and e-mail
2) notification via e-mail
3) record to local storage (SD/SDHC/SDXC card)
4) NAS recording at event triggers
5) external output
6) PTZ preset
5. Pixel Counter available in the plug-in web viewer. 
6. Azimuth that indicates the following directions as OSD.
a. East, West, South, North, Northeast, Southeast, Northwest, and Southwest
1.03 CAMERA SOFTWARE
A. The 4K camera shall have a built in web server which supports browser-based configuration using Internet Explorer, Google Chrome, Mozilla Firefox, and Apple Safari, for which web viewer plug-ins are available, from a PC or Mac.
B. The web viewer shall provide a monitoring screen which displays live camera video and simultaneously provides same-screen access to the following functions.
1. Live view window size
2. Resolution setting
3. Image (snapshot) capture
4. Manual recording to SD or NAS
5. Audio/microphone control
6. Access Playback and Setup menus
C. The web viewer shall provide a playback screen which provides access to the following functions.
1. Search date and time range
2. Search event type
3. Play an event video
4. Set resolution
5. Play audio if present
6. Generate a backup copy of saved video data
D. The web viewer shall provide a setup screen which provides access to the following configuration settings and functions in the camera.
1. Digital video profile to include compression type, maximum or target bit rate, frame rate, multicast parameters, crop encoding area
2. User profile to include password, access level, authentication
3. Date and time
4. Network settings and IP version
a. DDNS
b. SSL, including certificate management
c. 802.1x authentication
d. Quality of Service settings
e. SNMP to include version selection and settings
f. Auto configuration
5. Video setup to include flip and mirror mode, hallway view mode, video type, privacy zone
6. Audio setup to include source, audio codec type, gain, and bit rate
7. Camera settings to include image preset, sensor frame capture, dynamic range, white balance, back light, exposure, day/night operation, on-screen display, IR illumination, sharpness, contrast, and color level.
8. Event detection setup to include notification parameters, recording rules, time schedule, tamper protection, motion detection, event triggers
9. System function to include reboot, upgrade, check system and event logs, application (SDK) management
10. View profile information
E. Client requirements
1. Acceptable Operating Systems: Windows 7 / 8.1 / 10, MAC OS X 10.9~10.11
2. Acceptable browsers
a. Plug-in free web viewer: Google Chrome 47, MS Edge 20
b. Plug-in web viewer: MS Explore 11, Mozilla Firefox 43, Apple Safari 9 * Mac OS X only
1.04 DETAILED SPECIFICATIONS
A. Video
1. Imager
a. Sensor: 1/2.5" 8M CMOS
1) pixels per sensor: 3864 (H) x 2202 (V) total; 3840 (H) x 2160 (V) effective
2) scanning: progressive
b. Minimum illumination
1) Color mode: 0.3Lux (1/30sec, F1.8, 50IRE), 0.005Lux (2sec, F1.8, 50IRE), 0.1Lux (1/30sec, F1.8, 30IRE), 0.0005Lux(2sec, F1.8, 30IRE)
2) Black & white mode: 0Lux (IR LED on)
c. The following features with control settings shall be available:
1) Camera Title: Off / On (Displayed up to 60 characters per line)
2) Day/night setting: Auto (ICR) / Color / B/W
3) Backlight compensation (BLC): Off / BLC / WDR
4) WDR: 120dB
5) Contrast Enhancement: Off / On (Samsung Super Dynamic Range)
6) Digital Noise Reduction (DNR): Off / On (Samsung Super Noise Reduction)
7) Defog: Off / Auto / Manual
8) Motion Detection: Off / On (4ea polygonal zones)
9) Privacy Masking: Off / On (16ea polygonal zones)
a) Color: Gray / Green / Red / Blue / Black / White
10) Gain Control: Off / Low / Middle / High
11) White Balance: ATW / AWC / Manual / Indoor / Outdoor (Include mercury & sodium)
12) Electronic shutter speed
a) settings: Minimum / Maximum / Anti flicker (2 ~ 1/12,000sec)
13) Digital Zoom: 16x
14) Image flip: Off / On
15) Image mirror: Off / On
16) Alarm I/O: Input 4 / Output 2 (relay type)
17) Alarm Triggers: Alarm input, Motion detection, Intelligent video analytics, Network disconnect
18) Alarm Events: File upload via FTP and E-mail, Notification via E-mail, Local storage (SD/SDHC/SDXC) or NAS recording at event triggers, External output, PTZ preset
19) Remote Control Interface: RS-485/422
20) RS-485 Protocol: Samsung-T/E, Pelco-P/D, Panasonic, Honeywell, AD, Vicon, Bosch, GE
21) Pixel Counter: Available in the plug-in web viewer. 
d. Lens: 4.8 ~ 96 mm (optical 20x)
1) Max. Aperture Ratio: F1.8
2) Angle of view: H 65.1˚(Wide) ~ 3.8˚(Tele)  / V 38.4˚(Wide) ~ 2.2˚(Tele)
3) Min. Object Distance: 1.5 m (4.92ft)
4) Focus Control: Auto Focus, One-shot Auto Focus, Manual
5) Lens Type: DC Auto Iris (IR Corrected)
6) Mount Type: Board-in Type
2. IR Viewable Length: 200 m (656.17ft)
3. Video Streams 
a. The 4K camera shall be able to produce 10 video profiles, each of which may have the following properties
1) Encoding type
a) H.265
b) H.264
c) MJPEG
2) Resolution: 
a) 3840 x 2160, 2592 x 1944, 2592 x 1464, 1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 800 x 450, 720 x 576, 640 x 480, 640 x 360, 320 x 240, 320 x 180
3) Maximum frame rate: 
a) H.265 and H.264: 30 fps at all resolutions
b) MJPEG: 15 fps at all resolutions
4) Smart Codec: Manual mode (Area-based: 5ea), WiseStream, Dynamic GOV
5) Bit rate control method:
a) H.265 and H.264: 
i. target bitrate level control 
ii. constant bit rate (CBR) or variable bit rate (VBR)
b) MJPEG
i. quality level control
ii. variable bit rate (VBR)
4. Number of multi-streaming profiles: 3 maximum
5. Simultaneous users (total): 15 maximum (unicast)
6. Storage and Recording
a. The 4K camera shall have onboard SD card storage.
1) Card type:  Micro SD/SDHC/SDXC
2) Capacity: Up to 128 GB per card
3) Image content on the card shall have the ability to be downloaded to a selected destination.
b. NAS
c. Edge Storage
1) SD/SDHC/SDXC (128GB): Motion images recorded in the SD/SDHC/SDXC memory card can be downloaded. Camera can detect automatically when the memory is connected. 
2) Memory status display: Normal / Error / Active / Formatting / Lock). 
3) NAS (Network Attached Storage)
4) Local PC for instant recording (Plug-in viewer only)
7. Interoperability - Video streams shall be capable of supporting ONVIF protocol, profiles S and G.
8. Single Images - The 4K camera shall support jpg file image screenshot and export.
B. Network
1. Connectivity: 10/100 Base-T Ethernet via RJ-45 connector
2. Protocols supported:
a. Transmission Control Protocol (TCP), Internet Protocol (IP) v4 and v6, User Datagram Protocol (UDP)
b. Configuration: Dynamic Host Configuration Protocol (DHCP)
c. Web services: Hypertext Transfer Protocol (HTTP), Secure HTTP (HTTPS)
d. Network services: Address Resolution Protocol (ARP), Bonjour, Domain Name System (DNS), Internet Control Message Protocol (ICMP), Network Time Protocol (NTP), Protocol Independent Multicast-Sparse Mode (PIM-SM), Simple Network Management Protocol (SNMP v1/2c/3 – MIB-2), Universal Plug and Play (UPnP)
e. Media: Real-Time Transport Protocol (RTP), Real-Time Control Protocol, Real-Time Streaming Protocol (RTSP)
f. Multicast: Internet Group Management Protocol (IGMP)
g. Notifications: File Transfer Protocol (FTP), Simple Mail Transfer Protocol (SMTP)
h. Remote Access: Point-to-Point Protocol over Ethernet) (PPPoE)
3. DDNS – The 4K camera shall support DDNS services offered by the Manufacturer and other publicly available service offerings.
4. Quality of Service (QoS) – Layer 3 DSCP
5. Security features
a. user password protection
b. IP address filtering - list of allowed or blocked IP addresses 
c. HTTPS(SSL) login authentication
d. HTTPS(SSL) secured communications
e. Digest login authentication
f. User access log
g. 802.1x authentication
6. Discovery - Manufacturer shall offer a discovery program to identify all devices of his manufacture on the network.
C. Audio
1. Direction: bi-directional
2. Audio In: Selectable (Mic in / Line in), Supply voltage: 2.5V DC (4mA), Input impedance: approx. 2K Ohm
3. Audio Out: Line out (3.5mm mono jack), Max output level: 1Vrms
4. Compression
a. G.711 u-law/G.726 selectable
b. G.726 (ADPCM) 8KHz, G.711 8KHz
c. G.726: 16Kbps, 24Kbps, 32Kbps, 40Kbps
d. AAC-LC: 48Kbps at 16KHz
D. Electrical
1. Power
a. Input Voltage / Current: 24V AC
b. Power Consumption: Max. 60W / 90W (Heater off/on, IR on)
E. Mechanical And Environmental
1. Material
a. Housing: Aluminum, plastic
2. Dimensions (W x H): 236.9 x 407.7 mm (9.33 x 16.05 in.) 
3. Weight: 7.1kg (15.65 lb.)
4. Temperature
a. Operating: -50° C to 55° C (-58° F to 131° F)
b. Storage: -50° C to 60° C (-58° F to 140° F)
5. Humidity: 0 - 90%, non-condensing
6. Environmental Rating
a. Mechanical (Vandal) Protection: IK10
7. Ingress Protection: IP66

END OF SECTION

PNP-9200RH		4K 20x NETWORK IR PTZ DOME CAMERA
Jan 2017		Page 1
image1.png
WiseNeT




