GUIDE SPECIFICATION
MasterFormat 2014: Section 28 23 29
MasterFormat 2016: Section 28 2x xx
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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com

[bookmark: _Toc334350689]
 PRODUCTS
EQUIPMENT
Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
Model: PNV-A7082RZ
Alternates: PND-A7082RV, PNO-A7082R, PND-A9082RV, PNO-A9082R, PNV-A9082RZ
GENERAL DESCRIPTION
Video Compression and Transmission – The camera shall have the following properties relating to the video signals it produces.
H.265, H.264 and MJPEG compression, each derived from a dedicated encoder and capable of being streamed independently and simultaneously. (see detailed specifications)
The camera shall be able to configure various resolution selections. (see detailed specifications)
The camera shall be able to configure up to 10 independent video stream profiles with differing encoding, quality, frame rate, resolution, and bit rate settings
The camera shall support unicast video streaming up to 20 users.
The camera shall support multiple streaming up to 5 profiles and 3 virtual channels.
The camera shall support multicast video streaming.
The camera shall be able to configure Dynamic DNS (DDNS). DDNS shall be provided with no additional cost by the manufacturer.
[bookmark: _Hlk197931251][bookmark: _Hlk197932097]The camera shall provide WiseStream based on AI engine to efficiently manage bit rate of the video stream and reduce storage.
The camera shall provide WiseNRⅡ, an AI-based feature to reduce noise and blur on image.
Camera – The camera device shall have the following physical and performance properties.
[bookmark: _Hlk197931280]True day/night operation with removable IR cut filter. The IR function shall provide manual power adjustment, automatic mode based on objects in the center of the screen, and automatic mode based on objects anywhere in the scene.
[bookmark: _Hlk197931300]The camera shall be able to produce clear images in high-contrast scenes with multi-exposure wide dynamic range up to 120dB. The WDR function shall include the following modes and options: On / Off, Automatic mode, Automatic mode based on low light, Automatic mode based on Black/White mode.  The WDR function shall provide 3 level adjustments.
The camera shall support digital noise reduction using both 2D and 3D noise reduction technology.
The camera shall be able to configure privacy masking areas with polygonal zones.
[bookmark: _Hlk197931315]The camera shall support mobile applications (iOS, Android) for remote viewing angle adjustment, rotation and focus control during installation.
The camera shall have a dual NPU capable of running all AI & analytics functions fully on one NPU while the other is available for ISP functions, including AI-based noise reduction, WDR, & low light image enhancements.
Intelligence and Analytics – The camera shall have a suite of intelligent analytic functions.
Classified object type: Person / Face / Vehicle / License plate
Attributes: Person (Gender, Clothing top/bottom color, Bag), Face (Age, Gender, Mask, Glasses), Vehicle (Type: car / bus / truck / motorcycle / bicycle, Color)
BestShot supported
Re-ID (Person) supported
Analytics events based on AI engine: Motion detection, Object detection, Virtual line(Crossing / Direction), Virtual area(Loitering / Intrusion / Enter / Exit / Appear / Disappear), Slip & Fall detection, Face mask detection, Social distancing detection
Analytics events: Defocus detection, Tampering, Audio detection, Shock detection
[bookmark: _Hlk197931375][bookmark: _Hlk197932618]Business Intelligence: People / Vehicle / Crowd counting, Queue management, Heatmap based on AI engine
The camera shall provide configurable Dynamic Privacy Masking feature with selectable mosaic or color masking.  Mosaic masking shall provide multiple pixilation options while color masking shall provide 8 color options.  Masking shall be available for any AI-based object type.  Masking shall be available at full resolution/frame rate on a selected channel, allowing a VMS to record both the original and masked video.
Interoperability
The camera shall be ONVIF Profile S, G, T and M compliant.
The camera shall be compatible with the Hanwha Vision Cloud Portal, including OnCloud VMS, HealthPro, and SightMind, utilizing the provided CloudConnector Open Platform application.
The camera shall be compatible with Hanwha Vision AI packs, utilizing Open Platform, to add additional AI functions.
Additional Features
Micro SD/SDHC/SDXC memory slot with configurable pre-alarm and post-alarm recording intervals
NAS recording option with configurable pre-alarm and post-alarm recording intervals
Alarm triggers and notifications
[bookmark: _Hlk197931432]Impact protection (IK10), Water & Dust protection (IP66/67)
Support Wisepower (Power monitoring & ECO mode)
The camera uses recycled plastic in construction
Device certificate (Hanwha Vision Root CA), Secure storage (Secure element with FIPS 140-3 level 3/CC EAL6+ certified), S-BOM
The camera shall feature an admin session timeout to prevent a webpage user from leaving access to the camera for longer than a specified period.
DETAILED SPECIFICATIONS
[bookmark: _Toc173721624]Video
Imaging device: 1/1.8" CMOS
Resolution: 2592x1520, 2560x1440, 1920x1080, 1600x1200, 1280x960, 1280x720, 1024x768, 800x600, 640x480, 640x360, 320x240, 320x180
Maximum Framerate
H.265/H.264
WDR Off: Max. 60fps(60Hz) / 50fps(50Hz)
WDR On: Max. 30fps(60Hz) / 25fps(50Hz)
MJPEG: Max. 30fps (at 4MP Max. 5fps)
Minimum Illumination
Color: 0.03Lux (F1.5, 1/30sec, 30IRE)
B/W: 0.003Lux (F1.5, 1/30sec, 30IRE)
Video Out (for Installation): Micro USB Type C
Lens
Focal length: 4.6 ~ 9.35mm (2.0x) motorized varifocal
Max. Aperture Ratio: F1.3(Wide) ~ F2.15(Tele)
Field of View
H:105°(Wide) ~ 47°(Tele)
V:58°(Wide) ~ 27°(Tele)
D:128°(Wide) ~ 55°(Tele)
Min. Object Distance: 1.5m (4.92ft)
Focus Control: Simple focus
Lens Type: P-Iris(IR corrected)
Pan & Tilt & Rotate
Range: 0°~350° / 0°~85°/ -95°~95°
Remote adjustment (Max. 3,650 cycles)
Operational Functions
Camera Title: Displayed up to 85 characters
Day/Night: Auto (ICR)
Backlight Compensation: BLC / HLC / WDR / SSDR
WDR(Wide Dynamic Range): 120dB
Digital Noise Reduction: SSNRⅤ, WiseNRⅡ(AI-based)
Digital Image Stabilization: Supported
Defog: Supported
Motion Detection: 8 zones, each with 8-point polygonal shape
Privacy Masking
32 zones, each with 8-point polygonal shape
Color: gray/green/red/blue/black/white/purple/yellow
Mosaic
Dynamic Privacy Mask(Based on AI engine)
Color: gray/green/red/blue/black/white/purple/yellow
Mosaic
Gain Control: Off / Max Gain / Manual
White Balance: ATW / Narrow ATW / AWC / Manual / Indoor / Outdoor
Lens Distortion Correction: Supported (Fill / Stretch mode)
Electronic Shutter Speed
Min / Max / Anti-flicker (2 ~ 1/30,000sec)
Prefer shutter control (based on AI engine)
Video Rotation: Flip, Mirror, Hallway view (90° / 270°)
Analytics
Classified object type: Person / Face / Vehicle / License plate
Attributes: Person (Gender, Clothing top/bottom color, Bag), Face (Age, Gender, Mask, Glasses), Vehicle (Type: car / bus / truck / motorcycle / bicycle, Color)
BestShot supported
Re-ID (Person) supported
AI-based analytics events: Motion detection, Object detection, Virtual line(Crossing / Direction), Virtual area(Loitering / Intrusion / Enter / Exit / Appear / Disappear), Slip & Fall detection, Face mask detection, Social distancing detection
Analytics events: Defocus detection, Tampering, Audio detection, Shock detection
Business Intelligence: People / Vehicle / Crowd counting, Queue management, Heatmap based on AI engine
Alarm Input / Output
Alarm input (with Network I/O Box SPM-4210)
Alarm Triggers: Analytics, Network disconnection, Alarm input, Time schedule, MQTT subscription, Day/Night Storage disruption, Case tampering
Alarm Events (When alarm trigger occurred)
File upload(image): e-mail/FTP/SFTP
File upload(video clip): FTP/SFTP
Notification: e-mail
Recording: SD/SDHC/SDXC or NAS recording at event triggers
Handover: PTZ preset, Send message by HTTP / HTTPS / TCP
Audio clip playback
MQTT: publication
Audio in:
Supported voltage: 2.5V DC
Input impedance: 20kΩ
Audio out
Output voltage: Less than 2.74Vpp
Load resistance: More than 10kΩ
Light Type: IR LED (850nm)
[bookmark: _Hlk137643969][bookmark: _Hlk197931852]IR Viewable Length: WiseIR 60m(196.85ft)
Edge Storage
Micro SD/SDHC/SDXC 2TB (1TB x 2 slots), NAS support
Edge Storage (OnCloud)
Max. 2TB (1TB x 2 slot)
Hanwha Vision branded microSD cards have been certified and recommended for OnCloud edge recording.
Memory: 4GB RAM, 8GB eMMC
Webpage Language: English, Korean, Simplified Chinese, Traditional Chinese, French, Italian, Spanish, German, Japanese, Russian, Portuguese, Czech, Polish, Turkish, Dutch, Hungarian, Greek
Network
Ethernet: Metal shielded RJ-45 (10/100/1000 BASE-T)
Video compression
H.265/H.264: Main / Baseline / High
MJPEG
Audio Compression
G.711(PCM): 8kHz(64Kbps)
G.726(ADPCM): 8kHz(16/24/32/40Kbps)
AAC-LC: 16kHz(48Kbps)
OPUS: 48kHz(64Kbps)
Smart Codec: WiseStream (Based on AI engine)
Bitrate Control
H.265 / H.264: CBR or VBR
MJPEG: VBR
Streaming
Unicast(20 users) / Multicast
Multiple streaming (Up to 5 profiles, 3 virtual channel support)
Profile set: Max. 10 profiles
Application Programming Interface
ONVIF Profiles S, G, T, M
SUNAPI (HTTP API)
Hanwha Vision Open Platform
Protocol
Network: IPv4, IPv6, TCP/IP, UDP/IP
Streaming: RTP(UDP), RTP(TCP), RTCP, RTSP, SRTP
Services: NTP, HTTP, HTTPS, SSL/TLS, DHCP, DNS, DDNS
File Transfer: FTP/SFTP, SMTP(StartTLS)
Management: SNMPv1/v2c/v3(MIB-2), IGMP, UPnP, Bonjour, LLDP
Other: ICMP, ARP, QoS, CDP, MQTT, Syslog
DDNS – The camera shall support DDNS services offered by the manufacturer and others publicly available service offerings
QoS – Layer 3 DSCP
Security Feature
OS / Firmware Protect: Encrypted Firmware, Secure boot, Signed Firmware
User authentication: Digest Authentication, Prevent brute-force attack
Network authentication: IEEE 802.1X (EAP-TLS, EAP-LEAP, EAP-PEAP, MSCHAPv2)
Secure Communication: HTTPS, SRTP, WSS (WebSocket Secure)
Access Control: IP-based access control, MAC-based access control, Auto logout
Data Protect: Encryption Credentials, Encrypt compress for live recording file export
Audit: Access / System / Event Log management
Device ID: Device certificate (Hanwha Vision Root CA)
Secure Storage: Secure element, SD card partition encrypt
[bookmark: _Hlk197931491][bookmark: _Hlk197931906]Security Certificate: ETSI EN 303 645, Secure element (FIPS 140-3 level 3, CC EAL6+)
The device shall not provide a manufacturer default password. Default password change shall be required to access the camera.
A minimal level of password complexity shall be required by the camera.
The camera shall not have a manufacturer back-door password.
The manufacturer shall provide a tool that provides the ability to make password changes to multiple cameras at the same time. 
[bookmark: _Hlk197931509]Network filtering – The camera shall allow a list of allowed or blocked IP addresses/subnet mask and/or MAC addresses to be entered to restrict access to the device.
Discovery – The manufacturer shall offer a discovery program to identify all their devices on the network. 
Configuration – The manufacturer shall offer a configuration program that remotely allows users to change settings on multiple cameras simultaneously.
Firmware upgrade – The manufacturer shall offer a program capable of upgrading multiple cameras at the same time (not requiring access to individual cameras).
Camera backup setting – The manufacturer shall provide a program that provides the ability to save multiple camera settings to a file and restore these camera settings if needed.
Reporting – The manufacturer shall provide a tool that can generate a report including thumbnail view, MAC address, IP address, serial number and other camera settings.
Environmental & Electrical
[bookmark: _Hlk148096344]Operating
Temperature
 -50°C to +55°C (-58°F to +131°F)
+74°C(+165°F)(MAX) based on NEMA-TS 2(2.2.7)
 * Start up should be done at above -30°C
Humidity
0 ~ 100% RH(Condensing)
Humidity control with AIR vent
Storage
Temperature: -50°C to +60°C (-58°F to +140°F)
Humidity: Less than 90% RH
EPA(Effective Projected Area): 0.017㎡
Input Voltage: PoE+ (IEEE802.3at type 2, class 4)
Power Consumption
PoE+: Max. 15.0W, typical 9.0W
Support Wisepower
Power monitoring (Max./Current/Avg.)
Power Redundancy Failover
Mechanical
Color: White
Material: Aluminum
Bubble: Hard-coated dome
RAL Code: RAL9003
Dimensions (Width x Height): ø180 x 135mm (ø7.09 x 5.31")
Weight: 2,100g(4.63lb)
Compatible Conduit hole / Gang box
Conduit: 19.1mm(3/4") (M25)
Gang box: Single, double, 4" octagon, 4" square
Certifications & Standards
EMC 
FCC 47 CFR Part 15 Subpart B Class A
ICES-3(A)/NMB-3(A)
CE/UKCA: EN 55032 Class A, EN 50130-4, EN 61000-3-2, EN 61000-3-3
VCCI CISPR 32 Class A
RCM AS/NZS CISPR 32 Class A
KS C 9832 Class A, KS C9835
Safety
UL 62368-1, CAN/CSA C22.2 NO.62638-1
IEC/EN 62471
Environment
IEC/EN 63000
[bookmark: _Hlk227593904]IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK11
NEMA 250 Type 4X, NEMA-TS 2(2.2.7.2-8, 2.2.8, 2.2.9)
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Compatible Models
Hanging Adaptor: SBP-180HMW1
Back Box: SBV-180BW, SBV-180WW
Ceiling Mount(Assy): SBP-150CMI, SBP-300CMI, SBP-300CMW1, SBP-900CMW, SBP-300CMTW, SBP-300CMTS, SBP-156CMW
Ceiling Mount(Single Unit): SBP-180CMB, SBP-140CMB, SBP-180CMS, SBP-900CMP, SBP-300CMP, SBP-150CMP, SBP-C15P, SBP-C15H
Wall Mount: SBP-400WMW, SBP-250WMW, SBP-156WNW
Pole Mount: SBD-180PMW
[bookmark: _Hlk214039527]In-ceiling Mount: SHD-1370FPW
Corner Mount: SBD-180KMA
Parapet Mount: SBP-156LMW1, SBP-300LMW
Cabinet: SBP-150NBW, SBP-300NBW
Weather Cap: None (included)
Dome Cover: SPB-VAN87W
Interface Box: SPM-4210
Other Compatible Models: SBP-VAN88W, SBP-115PFA
DORI Distance
1. Detect (25PPM / 8PPF): Wide 39.8m(130.51ft) / Tele 119.2m(391.15ft)
2. Observe (63PPM / 19PPF): Wide 15.9m(52.20ft) / Tele 47.7m(156.46ft)
3. Recognize (125PPM / 38PPF): Wide 8.0m(26.10ft) / Tele 23.8m(78.23ft)
4. Identify (250PPM / 76PPF): Wide 4.0m(13.05ft) / Tele 11.9m(39.12ft)
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