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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com

[bookmark: _Toc334350689]
PART  1  PRODUCTS
1.01 EQUIPMENT
A. Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
B. Model: QRN-830S
C. Alternates: None
1.02 [bookmark: _Toc173721624]GENERAL DESCRIPTION
A. The eight channel Network Video Recorder (“NVR”) shall record video and audio from up to eight network video cameras to a hard disk and enable playback of video and audio.
B. The manufacturer shall be responsible for rigorous testing of NVR’s reliability. The manufacturer shall provide a list of compatible hard disks that have been tested to guarantee reliable recording. The list shall be available in the manufacturer’s home page.
C. The NVR shall provide auto recovery backup (ARB) to transfer video that is recorded on network camera’s SD cards during failures to the hard disk drive. The NVR shall allow users to set transfer speed or bandwidth dedicated for ARB in three levels; low, middle, high. If the bit-rate of video to be transferred exceeds the set bandwidth, then the NVR shall transfer video in the order of channel number until all transfer is finished or the video becomes more than 24 hours old based on NVR’s current time. The NVR with ARB shall be able to handle the following failures.
1. Network disconnection between cameras and NVR
2. Unexpected shutdown of NVR
D. The eight channel NVR shall receive text data from external devices and overlay it on live as well as recorded video. It shall also provide search for text data and list all video with previews that is relevant to the search queries. The text shall include but not limited to the following.
1. Text from PoS devices, namely the texts printed on the receipt of transactions
2. Text from automatic number plate recognition software
3. Text from automated teller machines (ATM)
E. The NVR shall provide a remote monitoring environment for video and audio over the network using a remote computer. The remote monitoring software shall allow users to receive live streams, search for recoded videos, and configure devices.
F. P2P Service: The NVR shall provide easy configuration of mobile viewer. The mobile viewer shall be freely available and connection shall be established by simply scanning QR code from a mobile device.
G. The NVR shall have the following further general properties.
1. Camera search and discovery: The NVR shall have the capability to search the network for connected compatible cameras.
a. If eight or fewer cameras are searched or discovered, each camera will be automatically registered and current camera information (fps, days of recording) will be displayed.
b. If more than eight cameras are searched or discovered, the NVR shall provide the ability to selectively register up to eight cameras.
2. The NVR shall support WiseStream and Dynamic GOV, a smart codec used by WiseNet IP cameras. The smart codec shall produce visually equal video quality while reducing storage required.
3. Recording and playback functions
a. Support recording from CIF up to 8 MP per channel
b. 80 Mbps network camera recording throughput
c. Simultaneous playback capability up to eight video channels in local and eight video channels in network
d. H.265, H.264, and MJPEG compression support
e. View status of connected storage hardware
f. Set recording schedules
g. Set up triggered recording based on
1) sensor (input) detection
2) camera event (sensor, motion detection, video analytics, defocus)
3) video loss detection
h. Available recording settings by channel for standard and event-based recording types
1) compression type
2) resolution
3) images per second
4) quality
5) data transfer limit
6) pre-event and post-event record duration
7) I-frame and full frame recording
i. Available actions upon reaching full HDD storage capacity (with automatic notifications to users)
1) stop recording
2) overwrite
j. Search recorded data by time, event, text, ARB events, or smart search. Smart search shall include search options for
1) Virtual line (in/out/both)
2) Enter/exit
4. Storage
a. 6TB HDDs in JBOD configuration
b. USB connection for memory/storage device for video clip backup and settings export
5. Live view
a. Live, remote monitoring using Windows Network Viewer or Manufacturer supplied viewer
b. Configure and exercise functions for connected PTZ cameras, including functionality with compatible USB joystick
c. Capture and save snapshot images
d. Record current video in BU, EXE format from GUI mode and AVI format from Webviewer
6. Remote access
a. Multicast or unicast
1) Simultaneous unicast access by up to 10 users
2) Simultaneous multicast access by up to 20 users
b. Mobile device
1) Supported platforms: Android, IOS
2) Supported remote users
a) Live unicast: 10
b) Live multicast: 20
c) Playback: 3
c. Dynamic DNS (DDNS) support
7. High Definition (HDMI) local monitor outputs for live viewing, playback, & backup functions
8. ONVIF Profile S compliance
1.03 NVR SOFTWARE
A. The NVR shall have a built in server which provides access for authorized users to live view of connected cameras, NVR recording and playback functions, and NVR configuration settings.
B. The NVR software shall provide a monitoring screen which displays live camera video and simultaneously provides same-screen access to the following functions:
1. Screen mode, allowing set up and display of live video channels in various layouts or sequence configurations.
2. Hallway view mode for hallway view cameras.
3. Status displays
a. camera live status
1) model
2) connection status
3) IP address
4) compression
5) resolution
6) frame rate
7) quality
b. camera record status
1) bit rate
a) record bit rate
b) input bit rate
c) bit rate limits
2) configured video profile
3) input/record frames per second 
4. Start/stop recording
5. Search recorded video
6. Play recorded video
7. Freeze live video
8. Audio on, off, and mute
9. Event monitoring
10. Digital zoom
11. Camera PTZ controls
12. Manual recording
13. Image (snapshot) capture
C. The NVR software shall provide setup screens which provide access to the following configuration settings and functions.
1. System
a. date and time
b. user passwords and permissions
c. system information
d. software upgrade
e. system logs
f. event logs
g. backup logs
2. Cameras
a. image preview of video
b. profile information
c. compression information
d. protocol information
e. model information
f. IP address
g. connection status
h. total amount of data received by channel
i. auto or manual search and register
j. select and setup ONVIF protocol operation
k. add, delete, and edit camera profile
l. adjust settings
1) camera name
2) resolution
3) frame rate
4) quality
5) bit rate
6) brightness
7) backlight
8) exposure
9) day/night
10) defog
11) focus
12) mirror and flip
13) motion detection
m. apply settings to groups of cameras
n. live streaming settings
3. Recording
a. setup recording schedule by day and time per channel
b. record settings per channel
1) all frames, key frames, or no record
2) data limit per channel
3) pre and post event recording times
4) include audio
c. set recording profile per channel
1) compression
2) resolution
3) frame rate
4) quality
d. HDD full capacity options – stop, overwrite
e. Event configuration
1) sensor operation
2) Camera events, including motion detection and video analytics
3) video loss detection
4) alarm output parameters
4. Storage media and devices
a. display working status, including current rate of recording, recording loss rate, and cumulative losses
b. storage use and capacity information
c. HDD temperature information
d. HDD alarm notifications
5. Monitor
a. HDMI video output
b. configure display parameters
6. Text device
a. channel allocation
b. encoding type and delimiting characters
c. network port
d. event configuration
1) keyword entry
2) dollar value trigger
7. Network
a. address settings per physical port
b. bandwidth limits
c. software ports and protocol
d. multicast parameters
e. DDNS
f. UPnP
g. security
1) IP filtering
2) SSL encryption and certificates
3) 802.1x parameters
h. NTP server
i. SMTP e-mail settings
j. SNMP settings
k. live stream selection
l. DHCP server settings
8. Notifications
a. event types
b. intervals
c. recipients
D. The NVR software shall provide Search and Playback functions as follows.
1. Search by
a. time
b. event
c. text
d. backup device
2. Playback
a. play forward and reverse at normal or accelerated speeds, frame by frame, and next record
b. go to first and go to last functions
c. color-coded timeline with play head scrub bar
d. set audio on or off
e. initiate backup
E. The NVR shall have a built in web server which supports browser-based configuration from a PC.
1. Acceptable browsers: Internet Explorer, Google Chrome and Apple Safari
2. The web viewer shall provide a monitoring screen which displays video from registered cameras and simultaneously provides same-screen access to the following functions.
a. display layout configuration
b. additional display functions as available with direct connection to the NVR server
3. The web viewer shall provide the same functionality as available when directly connecting to the NVR server with respect to the following.
a. system settings
b. backup and restoration of configuration settings to a file
c. camera configuration settings and functions
d. recording
e. storage media and devices
f. monitor
g. text device
h. network
i. events and notifications
j. search and playback
4. Minimum client requirements
a. Acceptable Operating Systems: Windows XP, Vista, 7, 8, 10, Mac OS X (10.9, 10.10, 10.11)
b. Acceptable browsers: Microsoft Internet Explorer, Microsoft Edge, Google Chrome, Apple Safari
1.04 DETAILED SPECIFICATIONS
A. Video
1. Compression: H.265, H.264, MJPEG
B. Recording
1. Channel capability: 8
2. Recording bandwidth: Up to 80 Mbps
3. Resolution range: CIF up to 8 MP
C. Events and Response Actions
1. Triggers
a. video loss
b. event defined by camera
c. VA event
2. Response Actions
a. record
b. e-mail
c. activate PTZ preset
d. beep output
e. monitor out
D. Playback
1. Number of simultaneous channels
a. Local: 8
b. Network: 8
2. Bandwidth: 32 Mbps
E. Storage
1. Internal
a. Number of HDD’s: 1
b. Capacity per HDD: Max. 6 TB/1ea
2. External
a. Acceptable types: USB HDD/Flash drive for backup of video clips, firmware update, settings backup/restore, log export
F. Network
1. Connectivity: 1 x RJ-45(10/100 BASE-T), 8 x RJ-45(PoE)
2. Protocols supported:
a. Transmission Control Protocol (TCP), Internet Protocol (IP) v4 and v6, User Datagram Protocol (UDP)
b. Configuration: Dynamic Host Configuration Protocol (DHCP)
c. Web services: Hypertext Transfer Protocol (HTTP), Secure HTTP (HTTPS)
d. Network services: Address Resolution Protocol (ARP), Domain Name System (DNS), Internet Control Message Protocol (ICMP), Network Time Protocol (NTP), Simple Network Management Protocol (SNMP v1/2c/3 – MIB-2), Universal Plug and Play (UPnP)
e. Media: Real-Time Transport Protocol (RTP), Real-Time Control Protocol, Real-Time Streaming Protocol (RTSP)
f. Multicast: Internet Group Management Protocol (IGMP)
g. Notifications: Simple Mail Transfer Protocol (SMTP)
h. Remote Access: Point-to-Point Protocol over Ethernet (PPPoE)
3. DDNS – The NVR shall support DDNS services offered by the Manufacturer and other publicly available service offerings.
4. Security features
a. user password protection with group restrictions
b. IP address filtering - list of allowed or blocked IP addresses
c. HTTPS(SSL) login authentication
d. User access log
e. 802.1x authentication
f. Restriction of all network access/web viewer access
5. Discovery - Manufacturer shall offer a discovery program to identify all devices of his manufacture on the network, as well as ONVIF Profile S conformant devices.
6. Transmission Bandwidth: 80Mbps
G. Audio
1. Channel capability: 8 channels
2. Compression: AAC (16/48KHz), G.711 u-law, G.726 selectable
H. Electrical
1. Input Power: 54 V DC / 1.55 A
2. PoE budget: 65 W maximum
3. Power Consumption: 84 W maximum (1 HDD, PoE On)
I. Mechanical And Environmental
1. Dimensions (W x H x D): 300.0 mm x 47.6 mm x 238.9 mm (11.8 in. x 1.87 in. x 9.4 in.)
2. Weight: 1.32Kg (2.92 lb.) (without HDD)
3. Temperature
a. Operating: 0° C to 40° C (32° F to 104° F)
4. Humidity: 20 - 85%, non-condensing

END OF SECTION

QRN-830S		8 CHANNEL NETWORK VIDEO RECORDER
APR 2022		Page 1
image1.png
WiseNeT




