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SBP 301HF PTZ MOUNTS
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SBP 301HF PTZ MOUNTS
A. This PTZ mount has built-in SFP (Small Form-Factor Pluggable) for PTZ cameras.
B. This PTZ mount is Ivory color in appearance with aluminum body.

2.03	Compatible Model	
	A. Camera List
	SNP-6321H/5321H



2.04	External Connection
	A. Alarm I/O
	Input 4ea / Output 2ea

	B. Remote Control Interface
	RS-485/422

	C. Audio
	Input / Output, 3.5mm type

	D. CVBS
	BNC type, For installation

	E. Power Line
	24V AC, 2-wire



2.05	Optical Characteristics
	A. Support SFP Voltage
	3.3V typical

	B. Support SFP Current
	Max. 300mA

	C. Support SFP Cage
	Standard mini-SFP cage (For 6.5mm pitch SFP)

	D. Support SFP Port Type
	LC type

	E. Required SFP Speed
	1250Mbps (For 1000Mbps Ethernet), 
155Mbps (For 100Mbps Ethernet)

	F. Required SFP's BER 
(Bit Error Rate)
	Max. 10^-12

	G. Transmission Method (Optical)
	Mode depends on SFP module

	H. Optical Mode (Long / Short Wave)
	Mode depends on SFP module

	I. Cable Insertion Loss (dB)
	Mode depends on SFP module



2.06	Network Characteristics
	A. RJ-45 : Ethernet Speed
	100Mbps

	B. RJ-45 : Ethernet Physical Layer
	100 Base-T


	C. RJ-45 : Ethernet Standard
	IEEE 802.3u support

	D. Speed Transition (100 1000Mbps)
	External Dip switch

	E. Fiber : Default Speed
	1000Mbps


	F. Fiber : Ethernet Speed
	100Mbps, 1000Mbps

	G. Fiber : Ethernet Physical Layer
	100 Base-FX, 1000 Base-X

	H. Fiber : Ethernet Standard
	IEEE 802.3u, IEEE 802.3z support



2.07	Environmental
	A. Operating Temperature / Humidity
	-50°C ~ +55°C (+14°F ~ 131°F) / Less than 90% RH

	B. Ingress Protection
	IP66

	C. Vandal Resistance
	IK10



2.08	Electrical
	A. Power Consumption
	Max. 65W, 3.1A (Heater on)

	B. Input Voltage / Current
	24V AC



2.09	Mechanical
	A. Dimension (WxHxD)
	Ø163.9 x 157.9mm (Ø6.45" x 6.22"), 
Ø163.9 x 187.9mm (Ø6.45" x 6.7") 
(With NPT-Coupling)

	B. Weight 
	[bookmark: _GoBack]1.1Kg (2.43 lb.), 1.4Kg (3.09 lb.) (With NPT-Coupling)

	C. Color/Material
	Ivory / Aluminum



2.10	WARRANTY
A. 3 years, parts and labor.
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