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SCB-3003 960H WDR BOX CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A. All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B. All systems and components shall have been thoroughly tested and proven in actual use.
C. All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.
D. All systems and components shall be provided with a one-day turnaround repair express and 24-hour parts replacement. The repair and parts express shall be guaranteed by the manufacturer on warranty and non-warranty items.

2.02	SCB-3003 960H WDR BOX CAMERA
A. The camera shall be compatible with C/CS mount lens type with capability of Manual or DC Auto Iris 
B. The camera shall support Super HAD CCD II (Double scan). The camera shall support privacy masking and shall provide a minimum of 12 programmable zones with polygonal masking. 
C. The camera shall provide a motion detection and video analytics which includes Fixed / Moved, Fence, Tracking, and Counting.
D. The camera shall provide True Day & Night (ICR) and SSNR III.
E. The camera shall support standard communication protocols and it shall provide a customizable on-screen display (OSD) which shall be available in English, Japanese, Spanish, French, Portuguese, Korean on NTSP system and English, French, German, Spanish, Italian, Chinese, Russian, Polish, Czech, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese on PAL system.


2.03	VIDEO	
	A. Imaging Device
	1/3" Super HAD CCD II (Double scan)

	B. Total Pixels
	

	
	1. SCB-3003N
	1,028(H) x 508(V)

	
	2. SCB-3003P
	1,028(H) x 596(V)

	C. Effective Pixels
	

	
	1. SCB-3003N
	976(H) x 494(V)

	
	2. SCB-3003P
	976(H) x 582(V)

	D. Scanning System
	2 : 1 Interlace

	E. Synchronization
	Internal / Line lock / Extern

	F. Frequency
	

	
	1. SCB-3003N
	H : 15.734KHz / V : 59.94Hz

	
	2. SCB-3003P
	H : 15.625KHz / V : 50Hz

	G. Horizontal Resolution
	

	
	1. Color
	700TV lines (ER mode)

	
	2. B/W
	700TV lines

	H. Min. Illumination
	

	
	1. Color
	0.1Lux@F1.2 (50IRE), 0.0002Lux (Sens-up, 512x)

	
	2. B/W
	0.01Lux@F1.2 (50IRE), 0.00002Lux (Sens-up, 512x)

	I. S/N Ratio
	52dB (AGC off, Weight on)

	J. Video Output
	CVBS : 1.0 Vp-p / 75Ω composite



2.04	LENS
	A. Focus Control
	[bookmark: _GoBack]Simple focus / Manual, Button control (Manual, Simple focus, Day & Night)

	B. Lens Type
	Manual / Auto iris (Video / DC)

	C. Mount Type
	C / CS



2.05	OPERATIONAL
	A. On Screen Display
	

	
	1. SCB-3003N
	English, Japanese, Spanish, French, Portuguese, Korean

	
	2. SCB-3003P
	English, French, German, Spanish, Italian, Chinese, Russian, Polish, Czech, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese

	B. Camera Title
	Off / On (Displayed 15 characters)

	C. Day & Night
	Auto (ICR) / External / Color / B/W

	D. Backlight Compensation
	Off / User BLC / HLC / WDR

	E. Wide Dynamic Range
	

	
	1. SCB-3003N
	128x (52dB)

	
	2. SCB-3003P
	160x (54dB)

	F. Contrast Enhancement
	SSDR (Off / On)

	G. Digital Noise Reduction
	SSNRIII (Off / On)

	H. VPS
	Off / On

	I. PIP
	Off / On

	J. Digital Image Stabilization
	Off / On

	K. Sens-up (Frame Integration)
	2x ~ 512x

	L. Motion Detection
	Built-in

	M. Intelligent Video Analytics
	Fixed / Moved, Fence, Tracking, Counting

	N. Privacy Masking
	Off / On (12 programmable zones with polygonal masking)

	O. Gain Control
	Off / Low / High

	P. White Balance
	ATW / Outdoor / Indoor / Manual / AWC (1,700°K ~ 11,000°K)

	Q. Electronic Shutter Speed
	

	
	1. SCB-3003N
	1/60 ~ 1/120,000sec

	
	2. SCB-3003P
	1/50 ~ 1/120,000sec

	R. Digital Zoom
	Off / On (1x ~ 16x)

	S. Reverse
	Off / H-Rev / V-Rev / HV-Rev

	T. Profile
	Basic / Day & Night / Backlight / ITS / Indoor / User

	U. Alarm
	1 Out

	V. Communication
	Coaxial control (SPC-300 compatible), RS-485

	W. Protocol
	Coax : Pelco-C (Coaxitron)
RS-485 : Samsung-T/E, Pelco-D/P, Panasonic, Bosch, Honeywell, Vicon,GE, AD



2.06	ELECTRICAL
	A. Voltage
	Dual (24V AC & 12V DC ±10%)

	B. Power Consumption
	Max. 4W



2.07	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature
	-10°C ~ +55°C (+14°F ~ +131°F)

	B. Operating Humidity
	Less than 90% RH



2.08	PHYSCIAL SPECIFICATIONS
	A. Dimension (WxHxD)
	73.1 x 67.2 x 123.9mm (2.88" x 2.65" x 4.88")

	B. Weight
	285g (0.63 lb)

	C. Color/Material
	Black, Silver / Aluminum, Plastic



2.09	CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark

2.10	WARRANTY
A. 3 years, parts and labor.



SCB-3003 AE 2015
