Page 2  SCB-6000 FULL HD HD-SDI CAMERA

SCB-6000 FULL HD HD-SDI CAMERA
TECHNICAL SPECIFICATIONS
SECURITY SYSTEM

DIVISION – 28 ELECTRONIC SAFETY AND SECURITY

LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE

LEVEL 2__28 23 00 VIDEO SURVEILLANCE

LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
PART 2 – PRODUCTS

2.01
GENERAL

A.
All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.
All systems and components shall have been thoroughly tested and proven in actual use.

C.
All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

D.
All systems and components shall be provided with a one-day turnaround repair express and 24-hour parts replacement. The repair and parts express shall be guaranteed by the manufacturer on warranty and nonwarranty items.

2.02
SCB-6000 FULL HD HD-SDI CAMERA
A. 
The HD-SDI indoor dome camera shall include the WiseNet II DSP chipset to provide Full HD 1080p TV lines. The camera shall operate in low light level (1Lux) interior environments and shall support high quality images in this environment. 

B.
The camera shall be compatible with C/CS mount lens type with capability of Manual or DC Auto Iris 
C.
The camera shall support virtual progressive scan CMOS. The camera shall support privacy masking and shall provide a minimum of 16 programmable zones. Support for motion detection shall also be provided.
D.   The camera shall support standard communication protocols and it shall provide a 
customizable on-screen display (OSD) which shall be available in English, Korean, French,     German, Spanish, Italian, Chinese, Russian, Polish, Swedish, Danish, Portuguese, Japanese, Serbian, Czech, Romanian, Turkish, Taiwanese, Thai
2.03
ELECTRICAL SPECIFICATIONS
A. Input Voltage
Dual 12V AC, 24V AC
B. Power Consumption
Max. 6 W 
2.04
VIDEO SPECIFICATIONS
A. Imaging Device
1/3” Progressive Scan CMOS
B. Total Pixels (horizontal x vertical)       
 2,010(H) x 1,108(V), 2.2M Pixels
C. Effective Pixels (horizontal x vertical) 1,944(H) x 1,092(V), 2.1M Pixels
D. Scanning system
Progressive Scan
E. Min. Illumination



1. Color 
1Lux@F1.2, 0.017 (Sens-up, 60x)

2. B/W
0.1Lux@F1.2, 0.0017Lux (Sens-up, 60x)
F. S / N (Y signal)
50dB (AGC off, Weight on)
G. Video Output
SMPTE292M (HD-SDI), CVBS: Monitoring
2.05
OPERATIONAL SPECIFICATIONS
A. On-Screen Display
English, Korean, French,     German, Spanish, Italian, Chinese, Russian, Polish, Swedish, Danish, Portuguese, Japanese, Serbian, Czech, Romanian, Turkish, Taiwanese, Thai

B. Camera Title
On, Off (Displays 15 characters)
C. Day & Night
Auto (ICR), Color & B/W, External
D. Contrast Enhancement
SSDR - On, Off 
E. Backlight Compensation
User BLC, HLC, Off
F. Motion detection
On, Off 
G. Digital Zoom
On, Off (1x-16x)

H. Privacy Masking
On, Off (16 programmable zones)

I. Digital Noise Reduction
On, Off - SSNRIII
J. Sens-up (Frame Integration)
Auto, Off (Selectable (2x ~ 60x)
K. Gain Control
Low, Medium, High, Off
L. White Balance
AWC, Manual, Indoor, Outdoor /
ATW (1,700ºK ~ 11,000ºK)
M. Electronic Shutter Speed
Esc/ A.FLK/ Manual (1/30~1/12,000)/ Fixed
N. Reverse
Off, H-Rev, V-Rev, HV-Rev
O. Alarm
(MD) Output 1, External D/N In 1

P. Communication
RS-485
Q. Protocol
SAMSUNG-T, SAMSUNG-E, Pelco-D, Pelco-P, BOSCH, Honeywell, VICON, PANASONIC, GE, AD
2.06
TRANSMISSION DISTANCE
A. 5C2V (75ohm)
Max. 100 ~ 140m

B. L-6CHD (75ohm)
Max. 200m

2.07
ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature
0°C ~ +50°C (+32°F ~ +122°F)
B. Operating Humidity
Less than 90% RH
2.08
MECHANICAL SPECIFICATIONS
Dimension
72.0 x 60.0 x 136.8mm (2.83" x 2.36" x 5.39”)
Weight

434g (0.96 lb) 
2.09
CERTIFICATIONS





FCC (Class A), UL/cUL Listed



CE (Class A), UL/cUL Listed
2.10
WARRANTY
A. Three years, parts and labor

2.11
ACCESORIES 



SPH-120R (Repeater), SPH-110C (Converter)
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