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SCO-2080RH 1/3” HIGH RESOLUTION WEATHERPROOF IR CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SCO-2080R 1/3” HIGH RESOLUTION WEATHERPROOF IR CAMERA
A. 	The high-resolution camera shall provide 600TV lines in color and 700TV lines in black/white, with minimum illumination of 0 Lux with IR LED on, with an IR distance of 50m (165ft).
B.	The camera shall provide a built-in varifocal lens (2.8~10mm), ICR for true day/night performance, motion detection, SSNRIII for digital noise reduction, and communication through RS-485 or coaxial control.
C. 	The camera shall have an IP66 weatherproof housing, built-in fan & heater.
D. 	The camera shall operate on dual power (12V DC and 24V AC).
E.	The camera shall provide a customizable on-screen display (OSD) which shall be available in English, Japanese, Spanish, French, Portuguese, Taiwanese, Korean in NTSC and English, French, German, Spanish, Italian, Chinese, Russian, Polish, Czech, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese in PAL.

2.03	ELECTRICAL SPECIFICATIONS
A. Input Voltage	Dual (12V AC, 24V AC +10%)
B. Power Consumption	Max 15W (heater on), Max 7.2W (heater off)

2.04	VIDEO SPECIFICATIONS
A. Imaging Device	1/3” Super HAD CCD
B. Total Pixels (horizontal x vertical)
	1. SCO-2080RHN	811 x 508 
	2. SCO-2080RHP	795 x 596
C. Effective Pixels (horizontal x vertical)
	1. SCO-2080RHN	768 x 494 
	2. SCO-2080RHP	752 x 582 
D. Scanning  system	2:1 Interlace
E. Synchronization	Internal, Line lock
F. Frequency (horizontal x vertical)
	1. SCO-2080RHN	15.734 KHz (H), 59.94Hz (V)
	2. SCO-2080RHP	15.625 KHz (H), 50Hz (V)
G. Horizontal Resolution
	1. Color	600TV Lines
	2. B/W	700TV Lines
H. Min. Illumination	
	1. Color 	0.15Lux @F1.2 (50IRE), 0.0003Lux (Sens-up, 512x)
	2. B/W	0.0Lux (IR LED On)
I. S / N (Y signal)	52dB (AGC off, Weight on)
J. Video Output	CVBS: 1.0 Vp-p, 75Ω composite

2.05	LENS SPECIFICATIONS
A. Focal Length (Zoom Ratio)	2.8 ~ 10mm (V/F, 3.6x)
B. Max. Aperture Ratio	1:1.2(Wide) ~ 2.8(Tele)
C. Minimum Object Distance	0.2m (.66ft)
D. Angular Field of View	94.4°(Wide) ~ 28°(Tele) (horizontal)
69.2°(Wide) ~ 21°(Tele) (vertical)
F. Focus Control	Manual
G. Lens Type	DC auto iris

2.06	OPERATIONAL SPECIFICATIONS
A. On-Screen Display
      1. SCO-2080RHN	English, Japanese, Spanish, French, Portuguese, Taiwanese, Korean
	2. SCO-2080RHP	English, French, German, Spanish, Italian, Chinese, 
		Russian, Polish, Czech, Romanian, Serbian, Swedish, 
		Danish, Turkish, Portuguese
B. Camera Title	On, Off (displays 15 characters)
C. Day & Night	Auto (ICR), Color, B/W
D. SSDR	On, Off (level adjustable)
E. Backlight Compensation	BLC, HLC, Off
F. Dynamic Range	SSDR (Off, On)
G. Digital Noise Reduction	SSNRIII (Off, On)
H. Digital Image Stabilization	On, Off
I. Motion Detection	On, Off (8 programmable zones)
J. Privacy Masking	On, Off (12 programmable zones)
K. Sens-up (Frame Integration)	2x ~ 512x
L. Gain Control	Low, High, Off
M. White Balance	ATW, Manual, Indoor, Outdoor, 
AWC (1,700K~11,000K)
N. Electronic Shutter Speed
	1. SCO-2080RHN	1/60 ~ 1/120,000
	2. SCO-2080RHP	1/50 ~ 1/120,000
O. Digital Zoom	On, Off (1x~16x)
P. Flip		Vertical, Horizontal
Q. Communication	RS-485, Coaxial control
R. Protocol
	1. Coax	Pelco-C (Coaxitron)
	2. RS-485	Samsung-T, Samsung-E, Pelco-D, Pelco-P, Bosch, 
			Honeywell, Vicon, Panasonic
S. IR Distance	50m (850nm IR LED: 32 each)

2.07	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	 -50°C ~ +50°C (-58°F ~ +122°F)
B. Operating Humidity	Less than 90% RH

2.08	MECHANICAL SPECIFICATIONS
A. Dimension 	
	1. Length w/ Bracket Angle of 180°	Ø114 x 383mm
B. Weight	1.7Kg (2.36lb)
C. Ingress Protection	IP66

2.09	CERTIFICATIONS	
A. SCO-2080RHN	FCC (Class A), UL/cUL Listed
B. SCO-2080RHP	CE (Class A), UL/cUL Listed

2.10	WARRANTY
A. Three years, parts and labor
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