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SCO-2081R 1/3” HIGH RESOLUTION WEATHERPROOF IR CAMERA
TECHNICAL SPECIFICATIONS
SECURITY SYSTEM

DIVISION – 28 ELECTRONIC SAFETY AND SECURITY

LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE

LEVEL 2__28 23 00 VIDEO SURVEILLANCE

LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
PART 2 – PRODUCTS

2.01
GENERAL

A.
All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.
All systems and components shall have been thoroughly tested and proven in actual use.

C.
All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02
SCO-2081R 1/3” HIGH RESOLUTION WEATHERPROOF IR CAMERA
A. 
The high-resolution camera shall provide 700TV lines with minimum illumination of 0 Lux with IR LED on, with an IR distance of 50m.
B.
The camera shall provide a built-in varifocal lens (2.8~10mm), ICR for true day/night performance, motion detection, SSNRIII for digital noise reduction, and communication through RS-485 or coaxial control.

C. 
The camera shall have an IP66 weatherproof housing.

D. 
The camera shall operate on dual power (12V DC and 24V AC).
E.
The camera shall provide a customizable on-screen display (OSD) which shall be available in English, Japanese, Spanish, French, Portuguese, Korean in NTSC and English, French, German, Spanish, Italian, Chinese, Russian, Polish, Czech, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese in PAL.
2.03
ELECTRICAL SPECIFICATIONS
A. Input Voltage
Dual (12V AC, 24V AC +10%)
B. Power Consumption
7.2W
2.04
VIDEO SPECIFICATIONS
A. Imaging Device
1/3” Super HAD CCD

B. Total Pixels (horizontal x vertical)

1. SCO-2081RN
1020 x 508 

2. SCO-2081RP
1020 x 596
C. Effective Pixels (horizontal x vertical)

1. SCO-2081RN
976 x 494 

2. SCO-2081RP
976 x 582 
D. Scanning  system
2:1 Interlace
E. Synchronization
Internal, Line lock
F. Frequency (horizontal x vertical)

1. SCO-2081RN
15.734 KHz (H), 59.94Hz (V)

2. SCO-2081RP
15.625 KHz (H), 50Hz (V)
G. Horizontal Resolution
700TV Line(ER mode)

H. Min. Illumination



1. Color 
0.15Lux @F1.2 (50IRE), 0.0002Lux (Sens-up, 512x)

2. B/W
0.0Lux (IR LED On)
I. S / N (Y signal)
52dB (AGC off, Weight on)
J. Video Output
CVBS: 1.0 Vp-p, 75Ω composite
2.05
LENS SPECIFICATIONS

A. Focal Length (Zoom Ratio)
2.8 ~ 10mm (V/F, 3.6x)
B. Max. Aperture Ratio
1:1.2(Wide) ~ 2.8(Tele)
C. Minimum Object Distance
0.2m (.66ft)

D. Angular Field of View
94.4°(Wide) ~ 28°(Tele) (horizontal)
69.2°(Wide) ~ 21°(Tele) (vertical)
E. Object Distance
0.2M (0.66ft)
F. Focus Control
Manual
G. Lens Type
DC auto iris
2.06
OPERATIONAL SPECIFICATIONS
A. On-Screen Display
      1. SCO-2081RN
English, Japanese, Spanish, French, Portuguese, Korean

2. SCO-2081RP
English, French, German, Spanish, Italian, Chinese, 


Russian, Polish, Czech, Romanian, Serbian, Swedish, 


Danish, Turkish, Portuguese
B. Camera Title
On, Off (displays 15 characters)
C. Day & Night
Auto (ICR), Color, B/W, External D/N
D. SSDR
On, Off 
E. Backlight Compensation
BLC, HLC, Off
F. Dynamic Range
SSDR (Off, On)
G. Digital Noise Reduction
SSNRIII (Off, On)
H. Digital Image Stabilization
On, Off
I. Motion Detection
On, Off 
J. Privacy Masking
On, Off (8 programmable zones)

K. Sens-up (Frame Integration)
2x ~ 512x
L. Gain Control
Low, Middle, High, Off
M. White Balance
ATW, Manual, Indoor, Outdoor, 
AWC (1,800K(~10,500(K)
N. Electronic Shutter Speed


1. SCO-2081RN
1/60 ~ 1/120,000

2. SCO-2081RP
1/50 ~ 1/120,000
O. Defog
Off, Auto, Manual
P. Reverse
H-Rev(Off/On)

Q. Communication
Coaxial control(SPC-300 compatible)
R. Protocol
Pelco-C (Coaxitron)

S. IR Distance
50m (IR LED: 36each)
2.07
ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature
 -10°C ~ +50°C (+14°F ~ +131°F)
B. Operating Humidity
Up to 100% RH

2.08
MECHANICAL SPECIFICATIONS
A. Dimension 
77.1 x 82.4 x 280.2mm(3.04” x 3.24” x 11.03”)
B. Weight
500g (1.1lb)
C. Ingress Protection
IP66
2.09
CERTIFICATIONS


A. SCO-2081RN
FCC (Class A), UL/cUL Listed
B. SCO-2081RP
CE (Class A), UL/cUL Listed
SCO-2081R A&E 2013

