Page 3 SNO-8081RP 5MEGAPIXEL Network IR Bullet CAMERA
SCO-5083RP 1000TVL (1280H) WEATHERPROOF IR CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETIES AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

[bookmark: _GoBack]2.02	SCO-5083RP 1000TVL (1280H) WEATHERPROOF IR CAMERA
A. This analog camera features high resolution of 1000TV lines in black and white as well as in color. 
B. Minimum illumination of this camera is 0Lux with IR led on. IR distance is 50m.
C. This camera has 3.3x varifocal lens which varies from 3 to 10 mm.
D. This camera features Wide Dynamic Range (WDR) which can record wider range of light than normal hence provide clear image even in backlighting. 
E. This camera features Day & Night mode that incorporates an infrared cutfilter removal (ICR) mechanism for greater light sensitivity and true color reproduction in the low light environment. 
F. This camera features Samsung Super Dynamic Range (SSDR) which enhances brightness of picture in dark areas.
G. This camera provides Samsung Super Noise Reduction IV (SSNR IV).
H. This camera provides Defog mode which intensifies color and contrast to produce higher quality video in foggy weather. 
I. This camera provides intelligent video analytics such as Fence, Appear/Disappear, and Counting. 
J. This camera has IP66 rating which shows high degree of protection against dust and liquids. 
K. This camera has IK10 rating which shows high degree of protection against vandalism.
L. The protocols used by this camera are Pelco-C (Coaxitron), RS-485, and Dual Power.

2.03	VIDEO	
	A. Imaging Device
	1/3" 1.3M CMOS

	B. Total Pixels
	1,312(H) x 1,069(V)

	C. Effective Pixels
	1,305(H) x 1,049(V)

	D. Scanning System
	Progressive scan

	E. Synchronization
	Internal

	F. Frequency
	H : 15.625KHz / V : 50Hz

	G. Horizontal Resolution
	

	
	Color
	1000TV lines

	
	B/W
	1000TV lines

	H. Min. Illumination
	

	
	Color
	0.05Lux (F1.4, 50IRE), 0.001Lux (1sec, F1.4, 50IRE),
0.02Lux (F1.4, 30IRE), 0.0006Lux (1sec, F1.4, 30IRE)

	
	B/W
	0Lux (IR LED on)

	I. S / N Ratio
	52dB (AGC off, Weight on)

	J. Video Output
	CVBS : 1.0 Vpp / 75Ω composite



2.04	LENS
	A. Focal Length (Zoom Ratio)
	3 ~ 10mm (3.3x) varifocal

	B. Max. Aperture Ratio
	F1.4

	C. Angular Field of View
	H : 82.0°(Wide) ~ 26.5°(Tele)
V : 59.7°(Wide) ~ 19.9°(Tele)

	D. Min. Object Distance 
	0.5m (1.64ft)

	E. Focus Control
	Manual

	F. Lens Type 
	DC auto iris

	G. Mount Type 
	Board type



2.05	OPERATION
	A. On Screen Display
	English, Chinese, Korean, Japanese, German, Italian, French, Spanish, Russian,
Czech, Polish, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese

	B. Camera Title
	Off / On (Displayed 15 characters)

	C. Day & Night
	Auto (ICR) / External / Color / B/W

	D. Anti IR Saturation
	Top / Bottom / Left / Right

	E. Backlight Compensation
	Off / User BLC / HLC / WDR

	F. Wide Dynamic Range
	120dB

	G. Contrast Enhancement
	SSDR (Off / On)

	H. Digital Noise Reduction
	SSNR IV (Off / On)

	I. Defog
	Off / Auto / Manual

	J. Purple Fringe Reduction
	Off / Low / Middle / High

	K. Digital Image Stabilization
	Off / On

	L. Tampering
	Off / On

	M. Motion Detection
	Off / On

	N. Intelligent Video Analytics
	Fence, (Dis)Appear, Counting (Off / On)

	O. Privacy Masking
	Off / On (24 programmable zones with 4 points polygonal masking)

	P. Gain Control
	Off / Low / Middle / High

	Q. White Balance
	ATW / Outdoor / Indoor / Manual / AWC / Mercury (1,800K° ~ 10,500K°)

	R. Electronic Shutter Speed
	1sec ~ 1/12,000sec

	S. Digital Zoom
	Off / On (1x ~ 16x)

	T. Reverse
	Off / H-Rev / V-Rev / HV-Rev

	U. Profile
	Basic, Day & Night, Backlight, ITS, Indoor, User

	V. Alarm
	1 Out

	W. Communication
	Coaxial control (SPC-300 compatible)

	X. Protocol
	

	
	Coax
	Pelco-C (Coaxitron)

	
	RS-485
	Samsung-T/E, Pelco-D/P, Panasonic, Bosch, Honeywell, Vicon, AD, GE

	Y. IR Distance
	50m (164.04ft) (IR LED 36ea)



2.06	ENVIRONMENTAL
	A. Operating Temperature / Humidity
	-30°C ~ +55°C (-22°F ~ +131°F) / Less than 90% RH
*Start up should be done at above -10°C (+14°F)

	B. Storage Temperature / Humidity
	-30°C ~ +60°C (-22°F ~ +140°F) / Less than 90% RH

	C. Ingress Protection
	IP66

	D. Vandal Resistance
	IK10



2.07	Electrical
	A. Input Voltage / Current
	Dual (24V AC & 12V DC ±10%)

	B. Power Consumption
	Max. 9.5W



2.08	Mechanical
	A. Color / Material
	Dark gray / ALDC

	B. Dimension (WxHxD)
	Ø78.0 x 272.8mm (3.07" x 10.74") (Without sun shield)

	C. Weight
	1.5Kg (3.31 lb)



2.09	CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark

2.10	WARRANTY
A. 3 years, parts and labor.
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