GUIDE SPECIFICATION
MasterFormat 2014: Section 28 23 29
MasterFormat 2016: Section 28 2x xx
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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com
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PART  1  PRODUCTS
1.01 EQUIPMENT
A. Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
B. Model: SCO-6025R
C. Alternates: None
1.02 GENERAL DESCRIPTION
A. Video and Transmission – The camera shall have the following properties relating to the video signals it produces.
1. 2 MP resolution, 30fps(60Hz)/25fps(50Hz)
2. Video signals are output in AHD/CVBS(selectable) format via BNC terminal.
3. Video shall be able to be transmitted up to 500 meters with 5c2v cable.
B. Camera – The camera device shall have the following physical and performance properties:
1. True day/night operation with removable IR cut filter
a. Low light level operation to 0.11 lux at F1.6, 1/30sec in color mode and 0 lux in black and white mode with IR LED on.
2. The camera shall be able to produce clear images in highly contrast scenes with digital wide dynamic range.
3. The camera shall support digital noise reduction using SSNR Ⅳ technology.
4. The camera shall be able to configure 8 privacy masking areas with rectangles.
C. Intelligence and Analytics – The camera shall have a suite of intelligent analytic functions.
1. Motion detection with 4 definable detection areas.
2. The camera shall be controlled by ACP or Coaxitron.

1.03 DETAILED SPECIFICATIONS
A. Video
1. Imaging device: 1/2.8" 2 MP CMOS
2. pixels per sensor: total 1,945 (H) x 1,109 (V), effective 1,945 (H) x 1,097 (V)
3. scanning: progressive
4. Minimum illumination: Color: 0.11Lux (F1.6, 1/30sec), B/W: 0 Lux (IR LED on)
5. Scanning System: Progressive Scan
6. Signal: Noise ratio: 52 dB
7. Video Output: BNC(AHD/CVBS selectable)
8. Resolution: 1920 x 1080
9. Max. Frame rate: 30fps(60Hz) / 25fps(50Hz) at 1920x1080
B. Lens: 
1. Focal length: 4mm fixed
2. Max. Aperture Ratio: F1.6
3. Field of View: H  87.6˚,  V 46.4°, D 104.5°
4. Min. Object Distance: 0.5m(1.64ft)
5. Lens Type: DC auto Iris
6. Mount Type: Board-in Type 
C. Operational Functions
1. IR Viewable Length: 30m (98.4ft)
2. On Screen Display: Displayed up to 15 characters
3. Day/Night Setting: Auto (ICR) / External / Color / B/W
4. Backlight Compensation: Off / User BLC / HLC 
5. WDR: D-WDR (Off/On)
6. Digital Noise Reduction: SSNR Ⅳ
7. Motion Detection: Off / On (4 zones)
8. Privacy Masking: Off / On (8 zones, rectangular)
9. Gain Control: Off / Low / Middle / High / Very High
10. White Balance: ATW / Outdoor / Indoor(4,500K° ~ 8,500K°) / Manual 
/ AWC (1,800K° ~ 10,500K°)
11. Electronic Shutter Speed: 1/30 sec ~ 1/12,000 sec(N), 1/25sec~ 1/12,000sec(P)
12. Alarm: MD output 1
13. Reverse: Off / H-Rev /V-Rev/HV-Rev
14. Remote Control Interface: Coaxial
15. Protocol: AHD: ACP (AHD Coax Protocol), CVBS: Pelco-C(Coaxitron)
16. Video Transmission Distance: 500m (1640.42 ft.) (5C2V coaxial cable)
17. DORI Distance
1) Detect (25PPM /8 PPF): 40m(131.38ft)
2) Observe (63PPM / 19PPF): 16m(52.55ft)
3) Recognize (125PPM /38 PPF): 8m(26.28ft)
4) Identify: (250PPM / 76PPF): 4m(13.14ft)
D. Electrical
1. Input Voltage: DC 12V
2. Power Consumption: DC 12V / 0.45A (Max 5.4W)
E. Mechanical
1. Color/Material: Dark gray, Plastic
2. Dimensions: Ø58.6 x 165.2 mm (Ø 2.31" x 6.50") without sunshield
3. Weight: 279g (0.62 lb)
F. Environmental
1. Operating Temperature: -30°C ~ +55°C (-22°F ~ +131°F) * Start up:  above -10°C
2. Operating Humidity: Less than 90% RH
3. Certification: IP66
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