GUIDE SPECIFICATION
MasterFormat 2014: Section 28 23 29
MasterFormat 2016: Section 28 2x xx
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]




[bookmark: _Toc334350683]Hanwha Techwin is a leading supplier of advanced video surveillance solutions for IP-video, analog and hybrid systems. Building on the company's history of innovation, Hanwha Techwin is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-efficiency. Hanwha Techwin is committed to the continued development of innovative systems products for professional security applications.

For additional information, visit http://security.hanwhatechwin.com/ 
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[bookmark: _Toc334350689]
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
[bookmark: _Toc334350690]
Notes to Specifier:
[bookmark: _Toc334350691]1.  Where several alternative parameters or specifications exist, or where, the specifier has the option of inserting text, such choices are presented in <bold text>.
2.  Explanatory notes and comments are presented in colored text.

	
Important:  See further notes on the following page.

Important Note to Security Systems Specifiers


CSI MasterFormat 2016 incorporates numerous significant changes affecting electronic safety and security. This document is written to provide flexibility in using either format, although adoption of MasterFormat 2016 is encouraged. The following is a guide to the MasterFormat numbers relevant to the product referenced in this specification.

Primary Specification Area:
MasterFormat 2014:
28 20 00 	Electronic Surveillance
	28 23 00 	Video Surveillance
			28 23 29	Video Surveillance Remote Devices and Sensors
MasterFormat 2016:
	28 20 00	Video Surveillance
		28 2x xx	Surveillance Cameras
			28 2x xx	IP Cameras

Related Requirements:
MasterFormat 2014:
	27 20 00 Data Communications 
	28 23 13 Video Surveillance Control and Management Systems
	28 23 16 Video Surveillance Monitoring and Supervisory Interfaces
	28 23 19 Digital Video Recorders and Analog Recording Devices
	28 23 23 Video Surveillance Systems Infrastructure

MasterFormat 2016
	27 15 01.xx	Video Surveillance Communications Conductors and Cables 
	27 20 00 	Data Communications 
	28 05 xx.xx	PoE Power Sources for Electronic Safety and Security 
	28 05 xx	Storage Appliances for Electronic Safety and Security 
		28 05 xx.xx	Network Video Recorders 
	28 05 xx	Cyber Requirements for Electronic Safety and Security
	28 05 xx	Safety and Security Network Communications Equipment 
	28 2x 00	Video Management System
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PART  1   GENERAL
1.01 SUMMARY
A. [bookmark: _Toc334350692]Section includes 1000TVL (1280H) analog camera. 
B. [bookmark: _Toc334350693]Product – An analog camera in a vandal resistant IP66/IK10 rated dome housing.
C. [bookmark: _Toc334350694]Related Requirements

Refer to MasterFormat notes at the beginning of this document to select requirements specific to the MasterFormat version being used in the specification.

1.02 REFERENCES
A. Abbreviations
1. AGC - Automatic Gain Control
2. ARP – Address Resolution Protocol
3. AWB  - Automatic White Balance
4. BLC – Back light compression
5. CBR – Constant Bit Rate
6. CVBS – Color, Video, Blanking, Sync
7. DHCP - Dynamic Host Configuration Protocol
8. DNR – Digital Noise Reduction
9. DNS - Domain Name Server
10. DDNS – Dynamic Domain Name Server
11. DSCP – Differentiated Services Code Point
12. fps - frames per second
13. FTP - File Transfer Protocol
14. GOV – Group of Video
15. GUI – Graphical User Interface
16. HD – High Definition
17. HTTP - Hypertext Transfer Protocol
18. ICMP – Internet Control Message Protocol
19. IGMP - Internet Group Management Protocol
20. IP - Internet Protocol
21. JPEG - Joint Photographic Experts Group
22. MJPEG - Motion JPEG
23. MP - Megapixel
24. MPEG - Moving Pictures Experts Group
25. NAS – Network Attached Storage
26. NTP - Network Time Protocol
27. PIM-SM - Protocol Independent Multicast-Sparse Mode
28. PoE - Power over Ethernet
29. PPPoE – Point to Point Protocol over Ethernet
30. RTP - Real-Time Transport Protocol
31. RTCP – Real-Time Control Protocol
32. RTSP - Real-Time Streaming Protocol
33. SDK – Software Development Kit
34. SMTP - Simple Mail Transfer Protocol
35. SNMP – Simple Network Management Protocol
36. SSL – Secure Sockets Layer
37. TCP - Transmission Control Protocol
38. UDP - User Datagram Protocol
39. UPnP – Universal Plug and Play
40. VBR – Variable Bit Rate
41. VMS - Video Management System
42. WDR – Wide Dynamic Range
43. DWDR – Digital Wide Dynamic Range
B. Reference Standards
1. Emissions
a. FCC-47 CFR Part 15 Subpart B Class B
b. CE EN 55022:2010
2. Immunity - CE
a. EN 50130-4:2011 
b. EN 61000-3-3:2014 
c. EN 61000-4-2:2009
d. EN 61000-4-3:2006+A2:2010
e. EN 61000-4-4:2012
f. EN 61000-4-5:2014
g. EN 61000-4-6:2009
3. Safety
a. UL listed
b. CE EN 50581:2012 (hazardous substances)
1.03 
SUBMITTALS
A. Product Data
1. Manufacturer’s printed or electronic data sheets
2. Manufacturer’s installation and operation manuals
3. Warranty documentation
1.04 QUALIFICATIONS
A. Manufacturer shall have a minimum of five years’ experience in producing IP video equipment.
B. Installers shall be trained and authorized by the Manufacturer to install, integrate, test, and commission the system.
1.05 DELIVERY, STORAGE AND HANDLING
A. Deliver the camera in the manufacturer’s original, unopened, undamaged container with identification labels intact. 
1.06 WARRANTY, LICENSING AND SUPPORT
A. Manufacturer shall provide a limited 3 year warranty for the product to be free of defects in material and workmanship.
B. Manufacturer shall provide video analytics embedded in the camera free of license charges.

END OF SECTION
PART  2 
 PRODUCTS
2.01 EQUIPMENT
A. Manufacturer: 	Hanwha Techwin 
http://security.hanwhatechwin.com/
B. Model		SCV-5082
C. Alternates: 		None
2.02 GENERAL DESCRIPTION
A. Video – 1000TVL (1280h) resolution
B. Camera – The 1000TVL (1280h)  analog camera device shall have the following physical and performance properties:
1. Auto day/night operation with removable IR cut filter
a. Low light level operation to 0.0006 lux (color) and 0.00006 lux (black and white)
2. Digital noise reduction
3. Digital zoom
4. Defog
5. 24 privacy masking regions utilizing a 4 point polygon
6. Digital image stabilization
C. Intelligence and Analytics – The camera shall have a suite of integral intelligent operations and analytic functions to include:
1. Motion detection 
2. Tampering
2.03 DETAILED SPECIFICATIONS
A. Video
1. Imager
a. Sensor			1/3" 1.3 MP CMOS
1.) pixels per sensor	1,312(H) x 1,069(V) total; 1,305(H) x 1,049(V) effective
2.) scanning		progressive
3.) synchronization		Internal
4.) frequency
a.) NTSC		H: 15.734KHz / V: 59.94Hz
b.) PAL		H: 15.625KHz / V: 50Hz
5.) Horizontal Resolution	
a.) Color 	 	1000TV lines
b.) B/W  		1000TV lines
b. Minimum illumination
1.) Color mode		0.05Lux (F1.4, 50IRE), 0.001Lux (1sec, F1.4, 50IRE),
0.02Lux (F1.4, 30IRE), 0.0006Lux (1sec, F1.4, 30IRE) 
2.) Black & white mode	0 0.005Lux (F1.4, 50IRE), 0.0001Lux (1sec, F1.4, 50IRE),
0.002Lux (F1.4, 30IRE), 0.00006Lux (1sec, F1.4, 30IRE)
c. Signal: Noise ratio		52 dB (AGC off, Weight on)
d. Video Output		CVBS: 1.0 Vpp / 75Ω composite
B. Lens					3 – 10 mm, varifocal
1.) Optical zoom ratio			3.3x
2.) Maximum aperture ratio   		F1.4
3.) Angle of view				H: 82.0°(Wide) ~ 26.5°(Tele) 
V: 59.7˚(Wide) ~ 19.9˚ (Tele)  
4.) Minimum Object Distance 		0.5 m (1.64ft.)
5.) Focus control				Manual
6.) Lens Type		DC auto iris
7.) Mount Type		Board
C. Operational
1.) On Screen Display			English, Chinese, Korean, Japanese, German, 
Italian, French, Spanish, Russian, 
Czech, Polish, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese
2.) Camera Title				On / Off (up to 15 characters)
3.) Day / Night				Auto (ICR) / External / Color / BW
4.) Backlight compensation (BLC)		Off / User BLC / HLC
5.) Contrast Enhancement			SSDR (Off / On)
6.) Digital Noise Reduction (DNR)		Off / On (Samsung Super Noise Reduction IV)
7.) Defog					Off / Manual / Auto
8.) Purple Fringe Reduction			Off / Low / Middle / High
9.) Digital Image Stabilization		Off / On
10.) Tampering				Off / On
11.) Motion detection			Off / On
12.) Privacy masking			
a.)	24 zones with 4 sided polygon
b.)	selectable for On/Off
13.) Gain control				Off / Low / Middle / High
14.) White Balance				ATW / Outdoor / Indoor / Manual / AWC / 
Mercury (1,800K° ~ 10,500K°)
15.) Electronic shutter speed 		1 - 1/12,000 sec.
16.) Digital Zoom				Off / On (1x ~ 16x)
17.) Reverse				Off / H-Rev / V-Rev / HV-Rev
18.) Profile					Basic, Day & Night, Backlight, ITS, Indoor, User
19.) Communication				Coaxial control (SPC-300 compatible)
20.) Protocol				Pelco-C (Coaxitron)
D. [bookmark: _Toc173721624]Electrical
a. Input Voltage and Current			Dual (24V AC & 12V DC ±10%)
b. Power Consumption			Maximum 5.6W
E. Mechanical And Environmental
1. Material				aluminum
2. Dimensions (W x H):  		137.0 x 106.1 mm (5.39 x 4.18 in.)
3. Weight:				730g (1.61 lb.)
4. Operating Temperature: 	-30° C to 55° C (-22° F to 131° F)
5. Humidity:			0 - 90%, non-condensing 
6. Environmental Rating:	
a. Ingress Protection				IP66
b. Mechanical (Vandal) Protection		IK10

END OF SECTION


PART  3    EXECUTION
3.01 INSTALLERS
A. Contractor personnel shall comply with all applicable state and local licensing requirements.
3.02 PREPARATION
A. The design and configuration shall be verified for compatibility and performance with the camera(s). 
B. Configuration shall be tested and qualified by the Contractor prior to camera installation.
C. All firmware found in products shall be the latest and most up-to-date provided by the manufacturer, or of a version as specified by the provider of the Video Management Application (VMA) or Digital Video Recorder (DVR). 
3.03 [bookmark: _GoBack]INSTALLATION
A. The Contractor shall carefully follow instructions in documentation provided by the manufacturer to insure all steps have been taken to provide a reliable, easy-to-operate system.
B. All equipment shall be tested and configured in accordance with instructions provided by the manufacturer prior to installation.
C. Before permanent installation of the system, the Contractor shall test the system in conditions simulating the final installed environment.
3.04 STORAGE
A. The camera hardware shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.
 
END OF SECTION
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