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SCV-5083 1280H WDR VANDAL-RESISTANT DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.
D.	All systems and components shall be provided with a one-day turnaround repair express and 24-hour parts replacement. The repair and parts express shall be guaranteed by the manufacturer on warranty and nonwarranty items.

2.02	SCV-5083 1280H WDR VANDAL-RESISTANT  DOME CAMERA
A.	The camera shall be compatible with Board type with DC Auto Iris
B.	The camera shall support virtual progressive scan CMOS. The camera shall support privacy masking and shall provide a minimum of 24 programmable zones. Support for motion detection shall also be provided.
C.   The camera shall support standard communication protocols and it shall provide a 
	      customizable on-screen display (OSD) which shall be available in English, Chinese, Korean,
	      Japanese, German, Italian, French, Spanish, Russian, Czech, Polish, Romanian, Serbian,
	      Swedish, Danish, Turkish, Portuguese

2.03	VIDEO	
	A. Imaging Device
	1/3" 1.3M CMOS

	B. Total Pixels
	1,312(H) x 1,069(V)

	C. Effective Pixels
	1,305(H) x 1,049(V)

	D. Scanning System
	Progressive scan

	E. Synchronization
	Internal

	F. Frequency
	

	
	1. SCV-5083N
	H : 15.734KHz / V : 59.94Hz

	
	2. SCV-5083P
	H : 15.625KHz / V : 50Hz

	G. Horizontal Resolution
	

	
	1. Color
	1000TV lines

	
	2. B/W
	1000TV lines

	H. Min. Illumination
	

	
	1. Color
	0.03Lux (F1.2, 50IRE)
0.001Lux (1sec, F1.2, 50IRE),
0.01Lux (F1.2, 30IRE)
0.0003Lux (1sec, F1.2, 30IRE)

	
	2. B/W
	0.003Lux (F1.2, 50IRE)
0.0001Lux (1sec, F1.2, 50IRE)
0.001Lux (F1.2, 30IRE)
0.00003Lux (1sec, F1.2, 30IRE)

	I. S/N Ratio
	52dB (AGC off, Weight on)

	J. Video Output
	CVBS : 1.0 Vpp / 75Ω composite



2.04	LENS
	A. Focal Length (Zoom Ratio)
	2.8 ~ 10.5mm (3.8x) varifocal

	B. Max. Aperture Ratio
	F1.2

	C. Angular Field of View
	H : 91.5°(Wide) ~ 27.7°(Tele) 
V : 68.3°(Wide) ~ 20.8°(Tele)

	D. Min. Object Distance
	0.5m (1.64ft)

	E, Focus Control
	Manual

	F. Lens Type
	DC auto iris

	G. Mount Type
	Board type



2.05	OPERATIONAL
	A. On Screen Display
	English, Chinese, Korean, Japanese, German, Italian, French, Spanish, Russian, Czech, Polish, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese

	B. Camera Title
	Off / On (Displayed 15 characters)

	C. Day & Night
	Auto (ICR) / External / Color / B/W

	D. Backlight Compensation
	Off / User BLC / HLC / WDR

	E. Wide Dynamic Range
	120dB

	F. Contrast Enhancement
	SSDR (Off / On)

	G. Digital Noise Reduction
	SSNR 4 (Off / On)

	H. Defog
	Off / Auto / Manual

	I. Purple Fringe Reduction
	Off / Low / Middle / High

	J. Digital Image Stabilization
	Off / On

	K. Tampering
	Off / On

	L. Motion Detection
	Off / On

	M. Intelligent Video Analytics
	Fence, (Dis)Appear, Counting (Off / On)

	N. Privacy Masking
	Off / On (24 programmable zones with 4 points polygonal masking)

	O. Gain Control
	Off / Low / Middle / High

	P. White Balance
	ATW / Outdoor / Indoor / Manual / AWC / Mercury (1,800K° ~ 10,500K°)

	Q. Electronic Shutter Speed
	1sec ~ 1/12,000sec

	R. Digital Zoom
	Off / On (1x ~ 16x)

	S. Reverse
	Off / H-Rev / V-Rev / HV-Rev

	T. Profile
	Basic, Day & Night, Backlight, ITS, Indoor, User

	U. Alarm
	1 Out

	V. Communication
	Coaxial control (SPC-300 compatible)

	W. Protocol
	Coax : Pelco-C (Coaxitron)



2.06	ELECTRICAL
	A. Voltage
	Dual (24V AC & 12V DC ±10%)

	B. Power Consumption
	Max. 5.6W



2.07	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature
	-30°C ~ +55°C (-22°F ~ +131°F)
*Start up should be done at above -10°C (+14°F)

	B. Operating Humidity
	Less than 90% RH



2.08	PHYSCIAL SPECIFICATIONS
	A. Dimension (WxH)
	Ø137.0 x 106.1mm (Ø5.39" x 4.18")

	B. Weight
	720g (1.59 lb)

	C. Color/Material
	Ivory / ALDC



2.09	CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark

2.10	WARRANTY
A. 3 years, parts and labor.
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