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SCV-5085 1000TVL (1280H) WDR Vandal-Resistant Dome Camera
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A. All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B. All systems and components shall have been thoroughly tested and proven in actual use.
C. All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SCV-5085 1000TVL (1280H) WDR Vandal-Resistant Dome Camera
A. The camera shall provide high resolution of 1000TV lines in black and white as well as in color.
B. The camera shall have minimum illumination of 0.03Lux in color and 0.003Lux in black and white at F1.2 and 50IRE.At F1.2 and 30IRE, the minimum illumination in color shall become 0.01Lux and in black and white, 0.001Lux.
C. The camera shall have motorized varifocal lens that varies from 3 to 8.5mm with zoom ratio of 2.8.
D. The camera shall feature WDR (Wide Dynamic Range) with gain of 120dB. 
E. [bookmark: _GoBack]The camera shall have Day & Night feature with built-in infrared cut filter removable (ICR) to provide true color reproduction and the best possible low light performance. 
F. The camera shall feature SSDR (Samsung Super Dynamic Range) that automatically detects and enhances brightness of dark area without affecting the rest to improve overall expression of the video. 
G. The camera shall feature SSNR (Samsung Super Noise Reduction) IV, the high performance noise reduction.
H. The camera shall feature defog mode that intensifies color and contrast in foggy and cloudy weather. 
I. The camera shall feature intelligent video analysis such as Fence, Appear/Disappear, and Counting.
J. The camera shall have IP66 and IK10 certification to show robust protection against weather and impact. 
K. The camera shall use Pelco-C protocol for control over coaxial cable. 


2.03	VIDEO	
	A. Imaging Device
	1/3" 1.3M CMOS

	B. Total Pixels
	1,312(H) x 1,069(V)

	C. Effective Pixels
	1,305(H) x 1,049(V)

	D. Scanning System
	Progressive scan

	E. Synchronization
	Internal

	F. Frequency
	

	
	NTSC
	H : 15.734KHz / V : 59.94Hz

	
	PAL
	H : 15.625KHz / V : 50Hz

	G. Horizontal Resolution
	

	
	1. Color
	1000TV lines

	
	2. B/W
	1000TV lines

	H. Min. Illumination
	

	
	1. Color
	0.03Lux (F1.2, 50IRE), 0.001Lux (1sec, F1.2, 50IRE),
0.01Lux (F1.2, 30IRE), 0.0003Lux (1sec, F1.2, 30IRE)

	
	2. B/W
	0.003Lux (F1.2, 50IRE), 
0.0001Lux (1sec, F1.2, 50IRE),
0.001Lux (F1.2, 30IRE), 
0.00003Lux (1sec, F1.2, 30IRE)

	I. S/N Ratio
	52dB (AGC off, Weight on)

	J. Video Output
	CVBS : 1.0 Vpp / 75Ω composite



2.04	LENS
	A. Focal Length (Zoom Ratio)
	3 ~ 8.5mm (2.8x) motorized varifocal lens

	B. Max. Aperture Ratio
	F1.2

	C. Angular Field of View
	H : 105.5°(Wide) ~ 37.1°(Tele)
V : 57.5°(Wide) ~ 21°(Tele)

	D. Min. Object Distance
	0.5m (1.64ft)

	E, Focus Control
	Manual

	F. Lens Type
	DC auto iris

	G. Mount Type
	Board type



2.05	OPERATIONAL
	A. On Screen Display
	English, Chinese, Korean, Japanese, German, Italian, French, Spanish, Russian,
Czech, Polish, Romanian, Serbian, Swedish, Danish, Turkish, Portuguese

	B. Camera Title
	Off / On (Displayed 15 characters)

	C. Day & Night
	Auto (ICR) / External / Color / B/W

	D. Backlight Compensation
	Off / User BLC / HLC / WDR

	E. Wide Dynamic Range
	120dB

	F. Contrast Enhancement
	SSDR (Off / On)

	G. Digital Noise Reduction
	SSNR IV (Off / On)

	H. Defog
	Off / Auto / Manual

	I. Purple Fringe Reduction
	Off / Low / Middle / High

	J. Digital Image Stabilization
	Off / On

	K. Tampering
	Off / On

	L. Motion Detection
	Off / On

	M. Intelligent Video Analytics
	Fence, (Dis)Appear, Counting (Off / On)

	N. Privacy Masking
	Off / On (24 programmable zones with 4 points polygonal masking)

	O. Gain Control
	Off / Low / Middle / High

	P. White Balance
	ATW / Outdoor / Indoor / Manual / AWC / Mercury (1,800K° ~ 10,500K°)

	Q. Electronic Shutter Speed
	1sec ~ 1/12,000sec

	R. Digital Zoom
	Off / On (1x ~ 16x)

	S. Reverse
	Off / H-Rev / V-Rev / HV-Rev

	T. Profile
	Basic, Day & Night, Backlight, ITS, Indoor, User

	U. Alarm
	1 Out

	V. Communication
	Coaxial control (SPC-300 compatible)

	W. Protocol
	Coax : Pelco-C (Coaxitron)



2.06	ELECTRICAL
	A. Input Voltage / Current
	Dual (24V AC & 12V DC ±10%)

	B. Power Consumption
	Max. 5W



2.07	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature
	-30°C ~ +55°C (-22°F ~ +131°F)

	B. Operating Humidity
	Less than 90% RH

	C. Ingress Protection
	IP66

	D. Vandal Resistance
	IK10



2.08	PHYSCIAL SPECIFICATIONS
	A. Dimension (WxH)
	Ø137.0 x 106.1mm (Ø5.39" x 4.18")

	B. Weight
	772g (1.7 lb)

	C. Color/Material
	Ivory / Aluminum



2.09	CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark

2.10	WARRANTY
A. 3 years, parts and labor.
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