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SMT 1722 and SMT-1723 17” TFT LCD MONITOR
TECHNICAL SPECIFICATIONS							SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS 

PART 2 – PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with an explicit manufacturer warranty.


2.02	SMT-1722 and SMT-1723 17” TFT LCD MONITOR 

A. The monitor shall have a 17” screen with protecting glass. It shall offer 1,280 x 1,024@ 120Hz resolution with 1,000:1 high contrast ratio, 250cd/m2 high brightness, and 5ms response time. 

B. All operation and configuration menus shall be provided in several languages, including support English, Spanish, French, German, Italian, Portuguese, Russian, Swedish, Chinese, Japanese, and Korean.

2.03	DISPLAY
A. Screen Size	17"
B. Max. Resolution	1,280 x 1,024 @120Hz
C. Brightness	250cd/m2
D. Contrast Ratio	1,000:1
E. Aspect Ratio	4:3
F. Viewing Angle (H/V)	160°, 160°
G. Display Color	16.7 Million
H. Response Time	5ms
I. Video System	NTSC, PAL
J. Panel Life	50,000 hours
K. Filter Type	3D Combfilter

2.04	INTERFACE	
A. Video Connector	BNC types: (2 in/2 out)
B. S-Video Connector	1CH input (Y/C), Loop Through out
C. RGB	
	1. Connector	One (1) Analog RGB 15-pin D-sub
	2. Input signal	0.7 Vp-p (0.5–1 Vrms)
	3. Available Format	640 x 350@70 Hz
		720 x 400@70 Hz
		640 x 480@60 Hz, 72 Hz, 75 Hz (VGA)
		800 x 600@56 Hz, 60 Hz, 72 Hz, 75 Hz (SVGA)
		1,024 x 768@60 Hz, 70 Hz, 75 Hz (XGA)
		1,152 x 864@75 Hz
		1,280 x 720@60 Hz
		1,280 x 960@60 Hz
		1,280 x 1,024@60 Hz, 75 Hz (SXGA)

D. HDMI	
	1. Connector	N/A
	2. Available Format	N/A
E. Audio 
	1. Connector	Two (2) RCA type (2 stereo inputs)
	2. Output signal	Loud Speakers : two (2) x 1 W
F. Application Support	Remote Controller

2.05	ON SCREEN DISPLAY	
A. Functions	Motion technology(120Hz), VESA™ DPM Compatible, PIP/PBP
B. Language	English, Spanish, French, German, Italian, Portuguese, Russian, Swedish, Chinese, Japanese, Korean
2.06	ELECTRICAL 	
A. Input Voltage
	1. 1722	AC100 ~ 240V (50/60Hz) 
	2. 1723	12V DC (External power supply)
B. Power consumption
	1. 1722	Type 34W
	2. 1723	Type 31W
C. Environmental 
	1. Operating Temperature	0 ~ +40°C (+32°F ~ +104°F)
	2. Humidity	20% ~ 90% (non-condensation)
D. Mechanical	
	1. Dimensions with stand 	371 x 368 x 220 mm (14.61" x 14.49" x 8.66")
	2. Dimensions w/out stand	371 x 331 x 67 mm (14.61" x 13.03" x 2.64")
	3. Mechanical Weight	5.95kg (13.12lbs)
	4. LCD Protection Glass	Yes
	5. Cabinet Color	Black
	6. VESA Mounts Interface	100 x 100mm

2.07	CERTIFICATIONS
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.08	WARRANTY
A. 3 years, parts and labor.
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