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SMT 1922/1923 MONITOR LCD TFT
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 REMOTE VIDEO SURVEILLANCE SENSORS AND DEVICES

PART 2 – PRODUCTS

2.01	GENERAL

A.	All equipment and materials used must be standard components regularly manufactured and used in the manufacturer's system.

B.	All systems and components must have been thoroughly tested and proven to be in effective use.

C.	All systems and components must be supplied with an explicit manufacturer's warranty.


2.02	SMT-1922/1923 MONITOR LCD TFT

A. The monitors must have a 19" LCD screen with protective glass. They must offer a resolution of 1,280 x 1,024 @ 120 Hz with a high contrast ratio of 1,000:1, high brightness of 250cd/m2 and a response time of 5 ms.

B. All operation and configuration menus shall be provided in multiple languages, including support for English, Spanish, French, German, Italian, Portuguese, Russian, Swedish, Chinese, Japanese, and Korean.

2.03	DISPLAY
A. Screen Size	19"
B. Maximum Resolution	1,280 x 1,024 @ 120 Hz 
C. Brightness	250cd/m2
D. Contrast Ratio	1.000:1
E. Aspect Ratio	4:3
F. Viewing Angle (H/V)	160°, 160°
G. Color Display	16.7 million
H. Response Time	5 ms
I. Video System	NTSC, PAL
J. Panel Life	40,000 hours	
K. Filter Type	3D comb filter


2.04	INTERFACE	
A. Video Connector	BNC Type: (2 Inputs/2 Outputs)	
B. S-Video Connector	1-channel input (Y/C), Connector output	
C. RGB	
	1. Connector	One (1) RGB Analog, 15-pin D-sub 
	2. Input Signal	0.7 Vp-p (0.5–1 Vrms)
	3. Available Formats	640 x 350 @ 70 Hz
		720 x 400 @ 70 Hz
		640 x 480@60 Hz, 72 Hz, 75 Hz (VGA)
		800 x 600@56 Hz, 60 Hz, 72 Hz, 75 Hz (SVGA)
		1,024 x 768@60 Hz, 70 Hz, 75 Hz (XGA)
		1,152 x 864 @ 75 Hz
		1,280 x 720 @ 60 Hz
		1,280 x 960 @ 60 Hz
		1,280 x 1,024@60 Hz, 75 Hz (SXGA)
D. HDMI	
	1. Connector	Not Applicable
	2. Available Format	Not Applicable
E. Audio
	1. Connector	Two (2) RCA type (2 stereo inputs)
	2. Output signal	Powerful Speakers: two (2) x 1 W
F. Application Support	Remote Control

2.05	DISPLAYING INFORMATION ON THE SCREEN
A. Functions	Motion Technology (120 Hz), Compatible with VESATM DPM, PIP/PBP Mounting	
B. Languages	English, Spanish, French, German, Italian, Portuguese, Russian, Swedish, Chinese, Japanese and Korean
2.06	ELECTRICAL SPECIFICATIONS
A. Input Voltage	
	1. SMT-1922	100~240V AC (50/60Hz)
	2. SMT-1923	12V DC (External Power Supply)
B. Consumption
	1. SMT-1922	37W nominal
	2. SMT-1923	34W nominal
C. Environmental Specifications 
	1. Operating Temperature	0 ~ +40°C 
	2. Humidity	20%~90% (non-condensative)
D. Mechanical Specifications	
	1. Dimensions with base	412 x 398 x 220 mm 
	2. Dimensions without the base	412 x 361 x 69 mm
	3. Mechanical Weight	6.85 kg
	4. LCD Protection Glass	Yes
	5. Cabinet Color	Black
	6. VESA Mounting Interface	100 x 100 mm 

2.07	CERTIFICATIONS
A. UL Certified
B. UL certified to Canadian safety standards
C. CE Mark
D. FCC Brand

2.08	WARRANTY
A. 3 years, parts and labor
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