GUIDE SPECIFICATION
MasterFormat 2014: Section 28 23 29
MasterFormat 2016: Section 28 2x xx
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]



[bookmark: _Toc334350683][bookmark: _GoBack]Hanwha Techwin is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Techwin is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Techwin is committed to the continued development of innovative systems products for professional security applications.

For additional information, visit http://www.hanwha-security.com/ 
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[bookmark: _Toc334350689]
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
[bookmark: _Toc334350690]
Notes to Specifier:
[bookmark: _Toc334350691]1.  Where several alternative parameters or specifications exist, or where, the specifier has the option of inserting text, such choices are presented in <bold text>.
2.  Explanatory notes and comments are presented in colored text.

	
Important:  See further notes on the following page.

Important Note to Security Systems Specifiers


CSI MasterFormat 2016 incorporates numerous significant changes affecting electronic safety and security. This document is written to provide flexibility in using either format, although adoption of MasterFormat 2016 is encouraged. The following is a guide to the MasterFormat numbers relevant to the product referenced in this specification.

Primary Specification Area:
MasterFormat 2014:
28 20 00 	Electronic Surveillance
	28 23 00 	Video Surveillance
			28 23 29	Video Surveillance Remote Devices and Sensors
MasterFormat 2016:
	28 20 00	Video Surveillance
		28 2x xx	Surveillance Cameras
			28 2x xx	IP Cameras

Related Requirements:
MasterFormat 2014:
	27 20 00 Data Communications 
	28 23 13 Video Surveillance Control and Management Systems
	28 23 16 Video Surveillance Monitoring and Supervisory Interfaces
	28 23 19 Digital Video Recorders and Analog Recording Devices
	28 23 23 Video Surveillance Systems Infrastructure

MasterFormat 2016
	27 15 01.xx	Video Surveillance Communications Conductors and Cables 
	27 20 00 	Data Communications 
	28 05 xx.xx	PoE Power Sources for Electronic Safety and Security 
	28 05 xx	Storage Appliances for Electronic Safety and Security 
		28 05 xx.xx	Network Video Recorders 
	28 05 xx	Cyber Requirements for Electronic Safety and Security
	28 05 xx	Safety and Security Network Communications Equipment 
	28 2x 00	Video Management System
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PART  1   GENERAL
1.01 SUMMARY
A. [bookmark: _Toc334350692]Section includes a 49 inch UHD LED monitor.
B. [bookmark: _Toc334350693]Product - A 49 inch UHD LED monitor manufactured for video surveillance with temperature sensors and panel life of 50,000 hours.
C. [bookmark: _Toc334350694]Related Requirements

Refer to MasterFormat notes at the beginning of this document to select requirements specific to the MasterFormat version being used in the specification.

1.02 REFERENCES
A. Abbreviations
1. UHD – Ultra High Definition
2. FHD – Full High Definition
3. LED – Light Emitting Diode
4. DHCP - Dynamic Host Configuration Protocol
1.03 SUBMITTALS
A. Product Data
1. Manufacturer’s printed or electronic data sheets
2. Manufacturer’s installation and operation manuals
3. Warranty documentation
1.04 QUALIFICATIONS
A. Manufacturer shall have a minimum of five years’ experience in producing IP video equipment.
B. Installers shall be trained and authorized by the Manufacturer to install, integrate, test, and commission the system.
1.05 DELIVERY, STORAGE AND HANDLING
A. Deliver the monitor in the manufacturer’s original, unopened, undamaged container with identification labels intact.
B. Store the monitor in a temperature environment specified in section 2.04 Detailed Specification, protected from mechanical and environmental conditions as designated by the manufacturer.
1.06 WARRANTY, LICENSING AND SUPPORT
A. Manufacturer shall provide at least a limited 3 year warranty for the product to be free of defects in material and workmanship.
B. Manufacturer shall provide embedded camera video analytics free of license charges.

END OF SECTION
PART  2 
 PRODUCTS
2.01 EQUIPMENT
A. Manufacturer: 	Hanwha Techwin 
http://www.hanwha-security.com/
B. Model		SMT-4933
C. Alternates: 		None
2.02 GENERAL DESCRIPTION
A. The monitor shall provide UHD resolution display with high contrast ratio of 4,700:1. 
B. The monitor shall have sensors monitoring temperature 24/7 to prevent overheating. 
C. The monitor shall have panel life of 50,000 hours which is equivalent to running more than 5 years without shutdown. 
D. The monitor shall have a fast response time of 8ms. 
E. The monitor shall support picture by picture mode displaying four FHD resolution videos. 
F. The monitor shall have built-in speakers. 
G. IP5X rated for dust protection. 
2.03 MONITOR SOFTWARE
A. The monitor shall provide automatic source switching and recovery after unexpected shutdown. 
B. The monitor shall have button lock to allow only authorized users can change configuration. 
C. The monitor shall support DHCP for network configuration. 
D. The monitor shall provide hot key options for fast selection of options. 
E. The monitor shall support Plug & Play. 
	
2.04 DETAILED SPECIFICATIONS
A. Display
1. Type 				LED
2. Screen Size 			49"
3. Max. Resolution 		3,840 x 2,160
4. Brightness 			500cd/m2
5. Contrast Ratio 			4,700 : 1
6. Aspect Ratio 			16 : 9
7. Viewing Angle (H/V) 		178° / 178°
8. Display Color 			16.7million
9. Response Time 		8ms
10. Operation Hour 			24 / 7
11. Panel Life 			50,000hours
12. Haze 				25%
B. Display
1. Dynamic C/R 			Mega
2. H-Scanning Frequency 		30 ~ 81KHz
3. V-Scanning Frequency 		48 ~ 75Hz
4. Maximum Pixel Frequency 	148.5MHz
C. Sound
1. Speaker Type 			Built-in speaker (10W + 10W)
D. Connectivity
1. Input 
a. RGB 			DVI-I (D-Sub common), Display port 1.2 (2)
b. Video 			HDMI (4)
c. Audio 			Stereo mini jack
d. USB 			USB (S/W update only)
2. Output 
a. Audio 			Stereo mini jack
3. External Control 		RS-232C (in / out), RJ-45
4. External Sensor 		IRDisplay
E. [bookmark: _Toc173721624]General
1. Electrical
a. Input Voltage 		100 ~ 240V AC (±10%) (50/60Hz)
b. Power Consumption 	100 (Typical), 140 (Rating), 154 (Max)
2. Sleep Mode 			less than 0.5W
3. Off Mode 			less than 0.5W
F. Environmental
1. Operating Temperature 		0 ~ +40°C (+32°F ~ +104°F)
2. Operating Humidity 		10% ~ 80% (Non-condensing)
G. Mechanical
1. Dimensions with Stand (WxHxD) 	1195.0 x 721.0 x 177.0mm (47.05" x 28.39" x 6.97")
2. Dimensions without Stand (WxHxD) 	1099.4 x 634.0 x 36.8mm (43.28" x 24.96" x 1.45")
3. Bezel Size 				Top 11.0mm (0.43") / Side 11.0mm (0.43")
Bottom 12.0mm (0.47")
4. Weight / Package 			13.4Kg (29.54 lb) / 17.9Kg (39.46 lb)
5. Rack Mounts	 			Optional
6. VESA Mounts Interface 			400 x 400mm
H. Special
1. H/W 					Temperature sensor, Pivot display, 
Clock battery (80hrs clock keeping),
Built-in speaker (10W 2CH), IP5x
2. S/W					FHD 4 PBP support (2 / 3 / 4 PBP), 
Auto source switching & recovery,
LFD home UI, Button lock, DHCP with RJ45 MDC, 
Hot key option, Plug & play (Initial setting)
I. Certification					Safety 60950-1
J. EMC 					Class A
K. Environment 				ENERGY STAR 7.0 (USA)
L. Accessories
1. Included 				Quick setup guide, Warranty card, Power cord, 
Remote controller, Batteries
2. Optional Stand 				SBM-4955ST
3. Media Player 				SBB-DA/DI

END OF SECTION


PART  3    EXECUTION
3.01 INSTALLERS
A. Contractor personnel shall comply with all applicable state and local licensing requirements.
3.02 PREPARATION
A. The network design and configuration shall be verified for compatibility and performance. 
B. Network configuration shall be tested and qualified by the Contractor prior to installation.
C. All firmware found in products shall be the latest and most up-to-date provided by the manufacturer, or of a version as specified by the provider of the Video Management Application (VMA) or Network Video Recorder (NVR). 
3.03 INSTALLATION
A. The Contractor shall carefully follow instructions in documentation provided by the manufacturer to insure all steps have been taken to provide a reliable, easy-to-operate system.
B. All equipment shall be tested and configured in accordance with instructions provided by the manufacturer prior to installation.
C. Before permanent installation of the system, the Contractor shall test the system in conditions simulating the final installed environment.
3.04 STORAGE
A. The hardware shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.
 
END OF SECTION
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