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SNB-3002P 4CIF NETWORK BOX CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SND-3002P 4CIF NETWORK BOX CAMERA
A.  The camera is network dome camera that shall provide resolution support with 30fps at 4CIF resolution.
B.  The camera shall support simultaneous transmission of multiple codec (H.264, MPEG-4, and MJPEG). 
C.  The camera shall have Manual DC Auto Iris. lens 
D. The camera shall provide PoE (Power over Ethernet)
E.	The camera shall provide a customizable on-screen display (OSD) which shall be available in English, French, German, Spanish, Italian, Chinese, and Korean.

2.03 ELECTRICAL SPECIFICATIONS
A. Input Voltage	24VAC, 12V DC, PoE (IEEE802.3af)
B. Power Consumption, max.	6W

2.03	CAMERA	
A. Imaging Device	1/3” Super HAD PS CCD
B. Scanning System	Progressive. (Interlaced Scan if WDR is on)
C. Horizontal Resolution, min.	600TV Lines in color
D. Min. Illumination
	1. Color	0.4Lux (F1.2, 50IRE), 0.001 Lux (Sens-up, 512x)
	2. Black/White	0.04Lux (F1.2, 50IRE), 0.001 Lux (Sens-up, 512x)


H. S/N Ratio	52dB
I. Video Output	CVBS: 1.0wp-p, 75 ohms composite

2.04	LENS
A. Drive Type	DC auto iris
B. Mount Type	C/CS


2.05	OPERATIONAL SPECIFICATIONS
A. Camera Title	On, Off (displays up to 15 characters)
B. Day and Night	Auto,(ICR)
C. Backlight Compensation	BLC, WDR, Off
D. Wide Dynamic Range
	1. NTSC	128x, 52dB
	2. PAL	160x, 52dB
E. Contract Enhancement,                       SSDR	Off, On
F. Digital Noise Reduction,                       Motion adaptive 2D+3D noise filter  Off, Low, Middle, High, User
G. Digital Image Stabilization	On, Off
H. Motion Detection	On, Off (4 programmable zones)
I. Privacy Masking	On, Off (12 polygonal programmable zones,
4 point polygonal method)
J. Sens-up (Frame Integration)	Off, Auto (2x ~ 512x)
K. Gain Control	AGC (Low, Middle, High)
L. White Balance	ATW1, ATW2, AWC, 3200K, 5600K
M. Electronic Shutter Speed
	1. NTSC	1/100 ~ 1/10,000sec
	2. PAL	1/120 ~ 1/10,000sec
N. Flip/Mirror	Off, On 
O. Profile 	Standard, ITS, Backlight, Day & Night, Gaming, Custom
P. Intelligent Video Analytics	People counting (line-based, area based)
Q. PIP		Off, On
R. Alarm I/O	Input, 1 each. Output, 1 each (relay)

2.07	NETWORK
A. Ethernet	RJ-45 (10/100Base-T)
B. Video Compression	H.264, MPEG-4, MJPEG Multiple codec 
C. Resolution
	1. NTSC	704 x 480, 640 x 480, 352 x 240
	2. PAL	704 x 576, 640 x 480, 352 x 288
D. Max Framerate	30fps
E. Video Quality
	1. H.264, MPEG-4	Compression level, Target bitrate level control
	2. MJPEG	Quality level control


F. Bitrate Control
	1. H.264, MPEG-4	VBR or CBR
	2. MJPEG	VBR
G. Streaming	Dual streaming (MPEG-4+MJPEG or H.264+MJPEG) 
H. IP		IPv4, IPv6			
I. Network Protocol	TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP, 
			HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
			IGMP,  SNMPv1, v2c, v3 (MIB-2), ARP, DNS, DDNS, 
			ONVIF
J. Security	HTTPS (SSL) login authentication, Digest login 
		authentication, User access log
K. Streaming Method	Unicast, Multicast
L. User Access 	10 users at Unicast level
M. Memory Slot	SD/SDHC 
N. ONVIF Conformance	Yes
O. Webpage Language	English, French, German, Spanish, Italian, Chinese 
and Korean
P. Web Viewer
	1. Supported OS	Windows XP, Windows Vista, Windows 7, MAC OS
	2. Supported Browser	Internet Explorer 6.0 or higher
Q. Central Management Software	NET-i Viewer

2.08	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-10°C ~ +50°C (+14°F ~ +122°F)
B. Operating Humidity		20% ~ 80% RH

2.09	PHYSCIAL SPECIFICATIONS
A. Dimension
	1. SND-3080C 	72 x 136mm (Ø2.83" x 5.39")
B. Weight
	1. SND-3080C	440g (0.97 lb) 
C. Color	gray 
D. Case	Plastic

2.10	CERTIFICATIONS	
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.11	WARRANTY
A. 3 years, parts and labor.

2. 12	MODELS
A. NTSC
	1. SNB-3002P	basic version
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