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SNB 6005 2MEGAPIXEL FULL HD NETWORK CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SNB 6005 2MEGAPIXEL FULL HD NETWORK CAMERA
A. The network camera shall offer Max. 2M (1920 x 1080) resolution.
B. The cameras shall support Min. illumination of 0.015Lux at F1.2 when in color mode and 0.0015Lux at F1.2 when in black and white mode.
C. The camera shall provide 1/1.9" 2.42M CMOS.
D. The camera shall support H.264, MJPEG dual codec and multiple streaming.
E. The camera shall feature WDR (120dB), Simple focus, P-Iris, and Defog.
F. The camera shall feature Audio / Face / Motion detection.
G. The camera shall support SD/SDHC/SDXC memory slot.
H. The camera shall support multi-crop streaming.
I. The camera shall support PoE and UPnP.
J. The camera shall support Bi-directional audio.
 
2.03	VIDEO	
	A. Imaging Device
	1/1.9" 2.42M CMOS

	B. Total Pixels
	1,952(H) x 1,241(V) approx 2.42M pixels

	C. Effective Pixels
	1,937(H) x 1,097(V) approx 2.12M pixels

	D. Scanning System
	Progressive

	E. Min. Illumination
	

	
	1. Color
	0.03Lux (1/30sec, F1.2, 50IRE), 
0.015Lux (1/30sec, F1.2, 30IRE)

	
	2. B/W
	0.003Lux (1/30sec, F1.2, 50IRE), 
0.0015Lux (1/30sec, F1.2, 30IRE)

	F. Video Output
	CVBS : 1.0 Vpp / 75Ω composite, 
720 x 480(N), 720 x 576(P), for installation
DIP connector type

	G. S/N Ratio
	50dB



2.04	LENS
	A. Focus Control
	Simple focus (Motorized V/F) / Manual,
Remote control via network, 
Button control (Manual, Simple focus)

	B. Lens Type
	Manual / DC auto iris, P-Iris

	C. Mount Type
	C / CS



2.05	OPERATION
	A. Camera Title
	Off / On (Displayed up to 45 characters)

	B. Day & Night
	Auto (ICR) / Color / B/W / External / Schedule

	C. Backlight Compensation
	Off / BLC / WDR

	D. Wide Dynamic Range
	120dB

	E. Contrast Enhancement
	SSDR (Samsung Super Dynamic Range) (Off / On)

	F. Digital Noise Reduction
	SSNRIII (2D+3D noise filter) (Off / On)

	G. Digital Image Stabilization
	Off / On

	H. Defog
	Off / Auto / Manual

	I. Motion Detection
	Off / On (4 zones with 4 points polygonal)

	J. Privacy Masking
	Off / On (32 zones with 4 points of polygonal)

	K. Gain Control
	Off / Low / Medium / High / Manual

	L. White Balance
	ATW / AWC / Manual / Indoor / Outdoor

	M. Electronic Shutter Speed
	Minimum / Maximum / Anti flicker (2 ~ 1/12,000sec)

	N. Flip / Mirror
	Off / On

	O. Intelligent Video Analytics
	Tampering, Virtual line, Enter / Exit, (Dis)Appear, Audio detection,
Face detection - Support Metadata

	P. Alarm I/O
	Input 1ea / Output 1ea

	Q. Remote Control Interface
	RS-485

	R. RS-485 Protocol
	Samsung-T/E, Pelco-P/D, Sungjin, Panasonic, Honeywell, AD, Vicon, GE, Bosch

	S. Alarm Triggers
	Motion detection, Tampering detection, Audio detection, Face detection,
Network disconnection, Video analytics, Alarm input

	T. Alarm Events
	File upload via FTP and E-mail, Notification via E-mail,
Local storage (SD/SDHC/SDXC) or NAS recording at event triggers, External output



2.06	NETWORK
	A. Ethernet
	RJ-45 (10/100BASE-T)

	B. Video Compression Format
	H.264 (MPEG-4 part 10/AVC) : Main / Baseline / High , MJPEG

	C. Resolution
	1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768,
800 x 600, 720 x 576, 800 x 450, 640 x 480, 
640 x 360, 320 x 240, 320 x 180

	D. Max. Framerate
	

	
	1. H.264
	Max. 60fps@ all resolutions

	
	2. MJPEG
	Max. 15fps@1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768
Max. 30fps@800 x 600, 800 x 450, 640 x 480, 
[bookmark: _GoBack]640 x 360, 320 x 240, 320 x 180

	E. Smart Codec
	Manual mode (Area-based : 5ea), 
Face detection mode

	F. Video Quality Adjustment
	

	
	1. H.264
	Compression level, Target bitrate level control

	
	2. MJPEG
	Quality level control

	G. Bitrate Control Method
	

	
	1. H.264
	CBR or VBR

	
	2. MJPEG
	VBR

	H. Streaming Capability
	Multiple streaming (Up to 10 profiles)

	I. Audio In
	Selectable (Mic in / Line in),
Supply voltage : 2.5V DC (4mA), Input impedance : approx. 2K Ohm

	J. Audio Out
	Line out (3.5mm stereo mini jack), 
Max output level : 1 Vrms

	K. Audio Compression Format
	G.711 u-law/G.726 selectable, G.726 (ADPCM) 8KHz, G.711 8KHz
G.726 : 16Kbps, 24Kbps, 32Kbps, 40Kbps

	L. Audio Communication
	Bi-directional audio (2-way)

	M. IP
	IPv4, IPv6

	N. Protocol
	TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP,RTSP, NTP, HTTP, HTTPS, SSL, DHCP, PPPoE, FTP,
SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP, DNS, DDNS, QoS, PIM-SM, UPnP, Bonjour

	O. Security
	HTTPS(SSL) login authentication
Digest login authentication
IP address filtering
User access log
802.1x authentication

	P. Streaming Method
	Unicast / Multicast

	Q. Max. User Access
	15 users at unicast mode

	R. Edge Storage
	SD/SDHC/SDXC - Motion Images recorded in the SD/SDHC/SDXC memory card can be downloaded. NAS (Network Attached Storage)

	S. Application Programming interface
	ONVIF profile S, SUNAPI (HTTP API), SVNP, Samsung camera application platform

	T. Webpage Language
	English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese,
Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch,
Croatian, Hungarian, Greek

	U. Web Viewer
	

	
	1. Supported OS
	Windows XP / VISTA / 7 / 8 / 8.1 or higher, 
MAC OS X 10.7

	
	2. Supported Browser
	Microsoft Internet Explorer (Ver. 8 ~ 11) 
Mozilla Firefox (Ver. 9 ~ 19), 
Google Chrome (Ver. 15 ~ 25)
Apple Safari (Ver. 6.0.2(Mac OS X 10.8, 10.7 only), 5.1.7) * Mac OS X only

	V. Central Management Software
	SmartViewer, SSM



2.07	ELECTRICAL
	A. Input Voltage
	24V AC, 12V DC, PoE (IEEE802.3af, Class3)

	B. Power Consumption
	Max. 11.44W (24V AC, 50/60Hz), Max. 10.1W (12V DC), Max. 11.1W (PoE, Class3)



2.08	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature / Humidity
	-30°C ~ +55°C (-22°F ~ +131°F) / Less than 90% RH
* Start up should be done at above -10°C (+14°F)

	B. Storage Temperature / Humidity
	-30°C ~ +60°C (-22°F ~ +140°F) / Less than 90% RH



2.09	PHYSCIAL SPECIFICATIONS
	A. Dimension (WxHxD)
	73.1 x 66.6 x 147.8mm (2.88" x 2.62" x 5.82")

	B. Weight 
	430g (0.95 lb)

	C. Color/Material
	Black, Ivory / Aluminum, Plastic



2.10	CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark

2.11	WARRANTY
A. 3 years, parts and labor.
SNB 6005 A&E 2015
