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SNB 6010 2MEGAPIXEL FULL HD NETWORK REMOTE HEAD CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SNB 6010 2MEGAPIXEL FULL HD NETWORK REMOTE HEAD CAMERA
A. These cameras shall support multi-streaming technologies, transferring real-time high resolution images.  It shall support 30fps at all available resolution when using H.264.
B. All operation and configuration menus shall be provided in English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Denish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatia, Hungary, Greek, Finnish and Norwegian.
C. The camera shall be of a dome type suitable for internal installation. The main unit shall be ivory and the camera unit shall be black in appearance.
D. The camera should be capable of capturing an image size of 1920 x 1080 at 30 images per second.
E. The camera shall feature Wide Dynamic Range with a gain of 120dB.
F. The camera shall provide memory slot for micro SD, SDHC and SDXC.
G. The camera shall provide Multi-crop streaming.

2.03	VIDEO	
	A. Imaging Device
	1/2.8" 2.38M CMOS

	B. Total Pixels
	1,952(H) x 1,116(V)

	C. Effective Pixels
	1,944(H) x 1,104(V)

	D. Scanning System
	Progressive

	E. Min. Illumination
	

	
	1. Color
	Color : 0.5Lux (1/30sec, F2.5, 50IRE)



2.04	LENS
	A. Focal Length
	4.6mm pinhole

	B. Max. Aperture Ratio
	F2.5

	C. Angular Field of View
	H : 71° / V : 38°

	D. Min. Object Distance
	0.3m

	E. Mount Type
	RJ-12 connected with main unit



2.05	OPERATION
	A. Camera Title
	Off / On (Displayed up to 45 characters)

	B. Day & Night
	Auto (Electrical) / Color / B/W / Schedule

	C. Backlight Compensation
	Off / BLC / WDR

	D. Wide Dynamic Range
	120dB

	D. Contrast Enhancement
	SSDR (Samsung Super Dynamic Range) (Off / On)

	E. Digital Noise Reduction
	SSNRIII (2D+3D noise filter) (Off / On)

	F. Digital Image Stabilization
	Off / On

	G. Defog
	Off / Auto / Manual

	H. Motion Detection
	Off / On (4ea 4 points polygonal zone)

	I. Privacy Masking
	Off / On (32 zones with 4 points of polygonal)

	J. Gain Control
	Off / Low / Middle / High

	K. White Balance
	ATW / AWC / Manual / Indoor / Outdoor

	L. Electronic Shutter Speed
	Minimum / Maximum / Anti flicker (1.2 ~ 1/10,000sec)

	M. Flip / Mirror
	Off / On

	N. Intelligent Video Analytics
	Tampering, Virtual line, Enter / Exit, (Dis)Appear

	O. Alarm I/O
	Input 1ea / Output 1ea

	P. Alarm Triggers
	Motion detection, Alarm input, Video analytics, Network disconnection

	Q. Alarm Events
	File upload via FTP and E-mail
 Notification via E-mail
Local storage (SD/SDHC/SDXC) or NAS recording at Event (Alarm triggers)
External output



2.06	NETWORK
	A. Ethernet
	RJ-45 (10/100BASE-T)

	B. Video Compression Format
	H.264 (MPEG-4 part 10/AVC), MJPEG

	C. Resolution
	1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 800 x 450, 640 x 480, 
640 x 360, 320 x 240, 320 x 180

	D. Max. Framerate
	

	
	1. H.264
	Max. 30fps @  all resolutions

	
	2. MJPEG
	Max. 30fps @ 800 x 600, 800 x 450, 640 x 480, 640 x 360, 320 x 240, 320 x 180
Max. 15fps @ 1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768

	E. Video Quality Adjustment
	

	
	1. H.264
	Compression level, Target bitrate level control

	
	2. MJPEG
	Quality level control

	F. Bitrate Control Method
	

	
	1. H.264
	CBR or VBR

	
	2. MJPEG
	VBR

	G. Streaming Capability
	Multiple streaming (Up to 10 profiles)

	H. IP
	IPv4, IPv6

	I. Protocol
	TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP,RTSP, NTP, HTTP, HTTPS, SSL, DHCP, PPPoE, FTP,
SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP, DNS, DDNS, QoS, PIM-SM, UPnP, Bonjour

	J. Security
	HTTPS(SSL) login authentication
Digest login authentication
IP address filtering
User access log
802.1x authentication

	K. Streaming Method
	Unicast / Multicast

	L. Max. User Access
	15 users at unicast mode

	M. Edge Storage
	micro SD/SDHC/SDXC
Motion Images recorded in the SDXC/SDHC/SD memory card can be downloaded

	N. Application Programming interface
	ONVIF profile S, HTTP API (SUNAPI) 2.0, SVNP 1.2

	O. Webpage Language
	English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, Greek, Finnish, Norwegian

	P. Web Viewer
	

	
	1. Supported OS
	Windows XP / VISTA / 7 / 8 / 8.1, MAC OS X 10.7

	
	2. Supported Browser
	Microsoft Internet Explorer (Ver. 11 ~ 8)
Mozilla Firefox (Ver. 19 ~9) * Windows only
Google Chrome (Ver. 25 ~ 15) * Windows only
Apple Safari (Ver. 6.0.2(Mac OS X 10.8, 10.7 only), 5.1.7) * Mac OS X only

	Q Central Management Software
	Smart Viewer, SSM



2.07	ELECTRICAL
	A. Voltage
	PoE (IEEE802.3af), 12V DC

	B. Power Consumption
	PoE : Max. 7.5W
12V DC : Max. 6.5W



2.08	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature / Humidity
	-10°C ~ +55°C (+14°F ~ +131°F) / Less than 90% RH

	B. Storage Temperature / Humidity
	-30°C ~ +60°C (-22°F ~ +140°F) / Less than 90% RH



2.09	PHYSCIAL SPECIFICATIONS
	A. Dimension
	

	
	1. Head Unit
	Ø25.0 x 44.0mm (Ø0.98" x 1.73")

	
	2. Body
	76.0mm x 121.1mm x 28.0mm (2.99" x 4.77" x 1.1")

	B. Weight
	

	
	1. Head Unit
	20g (0.04 lb)

	
	2. Body
	285g (0.63 lb)

	C. Color/Material
	

	
	1. Head Unit
	Black / Plastic

	
	2. Body
	Ivory / Plastic



2.10	CERTIFICATIONS	
[bookmark: _GoBack]A. CE mark
B. FCC mark
C. UL mark

2.11	WARRANTY
A. 3 years, parts and labor.
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