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SND-5061 1.3MEGAPIXEL HD NETWORK DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SND-5061 1.3MEGAPIXEL HD NETWORK DOME CAMERA
A.  This network camera that shall provide up to 1.3M (1280x1024) resolution with 16:9 full HD (720p) resolution.
B.  The camera shall have 3.0 ~ 8.5mm vari-focal 
C.  	The camera shall support simultaneous transmission of multiple codec (H.264 and MJPEG).
D. 	The camera shall support PoE.
E.  	The camera shall support indoor housing.
F.	The camera shall provide a customizable on-screen display (OSD) which shall be available in English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, and Greek.

2.03 ELECTRICAL SPECIFICATIONS
A. Input Voltage	12V DC, PoE (IEEE802.3af)
B. Power Consumption, max.	3.7 W  max  4W  PoE
	
2.04	CAMERA	
A. Imaging Device	1/3” 3M PS CMOS
B. Total Pixels (horizontal x vertical)	1,384 x 1,076
C. Effective Pixels (horizontal x vertical)	1,329 x 1,049 
D. Scanning System	Progressive
E. Min. Illumination
	1. Color	0.7Lux (F1.2, 50IRE)
F. DNR		SSNR (Off/On)
G. Video Output	DIP Connector type
	1. NTSC	704x480, for installation
	2. PAL	704x576, for installation






2.05	LENS
A. Focus control	Manual
B. Drive Type	DC auto iris
C. Mount Type	Board In
D. Aperture	F1.2
E. Angular View	H: 88.3(W) 32.4* (Tele) 71.5(W) 26* (Tele)	

2.06	OPERATIONAL SPECIFICATION
A. Camera Title	On, Off (displays up to 15 characters)
B. Day and Night	Auto (SW), Color, B/W
C. Backlight Compensation	BLC,Off
D. Digital Noise Reduction, 	SSNR   Off, On
E. Motion Detection	On, Off (4 programmable zones 20FPS)
F. Privacy Masking	On, Off (12 rectangle programmable zones)
G. Sens-up (Frame Integration)	Off, Auto (2x ~ 60x)
H. Gain Control	Off, Low, Medium, High, 
I. White Balance	ATW AWC, Manual, Indoor, Outdoor
J. Electronic Shutter Speed	Auto, A.FLK, Manual (1/30~12,000sec)
K. Flip/Mirror	Off, On
L. Intelligent Video Analytics	Scene change, 20 FPS
M. Alarm I/O	Input, 1 each. 

2.08	NETWORK
A. Ethernet	RJ-45 (10/100Base-T)
B. Video Compression	H.264,MJPEG  
C. Resolution 	1280 x 1024, 1280 x 720P (HD), 1024 x 768, 
800 x 600, 640 x 480, 320 x 240
D. Max Frame rate	30fps (1280 x 1024), 30fps (720P HD)
E. Video Quality
	1. H.264, MPEG-4	Compression level, Target bit rate level control
	2. MJPEG	Quality level control
F. Bitrate Control
	1. H.264, MPEG-4	VBR or CBR
	2. MJPEG	VBR
G. Streaming	Multiple, up to 10 profiles
H. IP		IPv4, IPv6			
I. Network Protocol	TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP, 
			HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
			IGMP,  SNMPv1, v2c, v3 (MIB-2), ARP, DNS, DDNS, 
			ONVIF
J. Security	HTTPS (SSL) login authentication, Digest login 
		authentication, IP Address filtering, User access log, 
K. Streaming Method	Unicast, Multicast
L. User Access 	10 users at Unicast 
M. ONVIF Conformance	Yes
N. Webpage Language	English, French, German, Spanish, Italian, Chinese, 
		Korean, Russian, Japanese, Swedish, Danish, 
		Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, 
		Dutch, Croatian, Hungarian, and Greek


O. Web Viewer
	1. Supported OS	Windows XP, Windows Vista, Windows 7, MAC OS
	2. Supported Browser	Internet Explorer 6.0 or higher, Firefox, Chrome, Safari
P. Central Management Software	NET-i Viewer

2.09	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-10°C ~ +55°C (+14°F ~ +131°F)
B. Operating Humidity		< 90% RH

2.10	PHYSCIAL SPECIFICATIONS
A. Dimension	115.8 x 92.7  (4.56 x 3.65)
B. Weight	345g (0.76 lb) 
C. Color	Ivory 
D. Material	Plastic

2.11	CERTIFICATIONS	
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.12	WARRANTY
A. 3 years
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