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SND 7061 3 MEGAPIXEL FULL HD NETWORK DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SND 7061 3 MEGAPIXEL FULL HD NETWORK DOME CAMERA
A. 	The network camera shall offer 3M resolution (2048 x 1536) with 16:9 full HD (1080p) resolution support.

B.	The camera shall provide video compression dual codec ( H.264 and MJPEG).

C.   The camera shall provide Smart codec (ROI encoding).

D.	The camera shall provide a customizable on-screen display (OSD) which shall be available in English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, Greek, Norwegian, Finnish

2.03	CAMERA
A. Imaging Device	1. 28” 3M PS CMOS
B. Total Pixels 	2,144(H) x 1,588(V)
C. Effective Pixels 	2,096(H) x 1,561(V)
D. Scanning System	Progressive 
F. Min. Illumination			0.4Lux (F1.2, 50IRE), 0.007Lux (Sens-up 60x)
G. S / N Ratio	50dB
H. Video Output	CVBS:	1.0Vp-p / 75ohm composite, 704x480(N), 704x576(P), for installation

2.04	LENS TYPE
A. Focus Control	Manual 
B. Lens Type	DC auto iris
C. Mount Type	Board-in type

2.05	OPERATION
A. Camera Title 	Off, On (Displayed up to 15 characters)
B. Day & Night 	Auto (ICR), Color, B/W, External B/W
C. Backlight Compensation		Off, BLC
D. Digital Noise Reduction SSNR 	On, Off
E. Motion Detection 	Off, On (4 programmable zones, 3M 15fps, 2M 20fps)
F. Privacy Masking 			Off, On (12 rectangular zone)
G. Sens-up (Frame Integration) 	Off, Auto (2x ~ 60x)
G. Gain Control 	Off, Low, Middle, High
I. White Balance 	ATW, AWC, Manual, Indoor, Outdoor
J. Electronic Shutter Speed 	Auto, A.FLK, Manual (1/30 ~ 12,000sec)
K. Flip / Mirror 	Off, On
L. Intelligent Video Analytics	Tampering(3M 15fps, 2M 20fps)
M. Alarm I/O 	Input 1ea

2.06	NETWORK PROTOCOL
A. Ethernet 	RJ-45 (10/100Base-T)
B. Video Compression Format 	H.264, MJPEG
C. Resolution 
		1. 3M Mode, 	2048 x 1536, 1920 x 1080p(Full HD), 1600 x 1200, 
	1280 x 1024, 1280 x 960, 1280 x 720p (HD), 1024 x 768, 800 x 600, 800 x 450, 640 x 480, 640 x 360, 320 x 240, 320 x 180  
		2. 2M Mode			1920 x 1080p(Full HD), 1280 x 960, 1280 x 720p(HD),
1024 x 768, 800 x 600, 800 x 450, 640 x 480, 640 x 360, 320 x 240, 320 x 180
D. Max. Framerate 	
		1. 3M Mode, H.264 		Max 20 fps at all resolutions
2. 3M Mode, MJPEG 		800 x 600 ~ 320 x 180, 20fps
1280 x 1024 ~1920 x 1080, 15fps
2048 x 1536, 10fps
3. 2M Mode, H.264 		Max. 30fps at all resolutions 
4. 2M Mode, MJPEG 		800 x 600 ~ 320 x 180, 30fps
			1280 x 1024 ~ 1920 x 1080, 15fps 
E. Video Quality Adjustment 	
	1. H.264 	Compression level, Target bit rate level control
	2. MJPEG 	Quality level control
F. Bitrate Control Method 	
	1, H.264	CBR or VBR
	2. MJPEG 	VBR
G. Streaming Capability 	Multiple streaming (Up to 5 profiles)
H. IP 		IPv4, IPv6
I. Protocol 				TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTSP, NTP,
HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
IGMP, SNMPv1, v2c, v3(MIB-2), ARP, DNS, DDNS, QOS, ONVIF
J. Security 	HTTPS(SSL) login authentication, 
Digest login authentication, IP address filtering, 
User access log, 802.1x authentication
K. Streaming Method 	Unicast, Multicast
L. Max. User Access 	10 users at Unicast mode
M. ONVIF Conformance 	Yes
N. Webpage Language 	English, French, German, Spanish, Italian, Chinese, 
		Korean, Russian, Japanese, Swedish, Danish, 
		Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, 
			Dutch, Croatian, Hungarian, Greek, Norwegian, Finnish
O. Web Viewer 
1. Supported OS 	Windows XP, Windows Vista, Windows 7, 
			Mac OS X 10.7 or higher
	2. Supported Browser	Internet Explorer 7.0 or higher, Firefox, Chrome, Safari
P. Central Management Software 	NET-i viewer

2.07	ELECTRICAL
A. Voltage	12V DC, PoE (IEEE802.3af) 
B. Consumption	Maximum 3.7W (12V DC) 
		Maximum 4.3W(PoE)

2.08	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-10°C ~ +55°C (14°F ~ 131°F) 
B. Operating Humidity	Less than 90% RH
C. Storage Temperature	-30°C ~ +60°C (-22°F ~ 140°F)
D. Storage Humidity 	Less than 90% RH
	
2.09	PHYSCIAL SPECIFICATIONS
A. Dimension (WxH)	Φ115.8.0 x 92.7mm (Φ4.56” x 3.65”)
B. Weight	345g (0.76 lb)
C. Color	Ivory
D. Material	Plastic

2.10	CERTIFICATIONS	
A. CE mark
B. FCC mark

2.11	WARRANTY
A. 3 years, parts and labor.
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