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SND L6083R 2 MEGAPIXEL NETWORK IR DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SND L6083R 2 MEGAPIXEL NETWORK IR DOME CAMERA
1. The camera shall be of a DOME type suitable for interior installation. The camera shall be ivory in appearance with a plastic body.
1. The camera shall provide video compression dual codec ( H.264 and MJPEG). 
1. The network camera shall feature up to 2 Mega Pixel resolution in a 16:9 format. 4:3 format shall also be available in smaller resolutions.
1. The camera shall feature an Adaptive Infrared illumination system with IR LEDs giving a viewable distance of 15m (49.21ft) in complete darkness. 

2.03	CAMERA	
	A. Imaging Device
	1/2.9" 2.19M CMOS

	B. Total Pixels
	2,000(H) x 1,121(V)

	C. Effective Pixels
	1,984(H) x 1,105(V)

	D. Scanning System
	Progressive

	E. Min. Illumination
	

	
	1. Color
	0.95Lux (1/30sec, F1.4), 0.002Lux (2sec, F1.4)

	
	2. B/W
	0Lux (IR LED on)



2.04	LENS TYPE
	A. Focal Length (Zoom Ratio)
	[bookmark: _GoBack]2.8 ~ 12mm (4.3x) varifocal

	B. Max. Aperture Ratio
	F1.4

	C. Angular Field of View
	H: 103.8 ˚ ~ 32.4˚ / V: 53.7 ˚ ~ 18.4˚ / D: 121.9 ˚ ~ 37.1˚

	D. Min. Object Distance
	0.5m (1.64ft)

	E. Lens Type
	Fixed

	F. Mount Type
	Board type

	G. Focus Control
	Manual



2.05	PAN/TILT/ROTATE
	A. Pan Range
	0 ˚ ~ 350 ˚

	B. Tilt Range
	0 ˚ ~ 67 ˚

	C. Rotate Range
	0 ˚ ~ 355 ˚



2.06	OPERATION
	A. Camera Title
	Off / On (Displayed up to 15 characters)

	B. Day & Night
	Electric Day & Night

	C. Backlight Compensation
	Off / BLC

	D. Contrast Enhancement
	SSDR (Samsung Super Dynamic Range) (Off / On)

	E. Digital Noise Reduction
	SSNR (Off / On)

	F. Motion Detection
	Off / On (4ea rectangular zones)

	G. Privacy Masking
	Off / On (6ea rectangular zones)

	H. Gain Control
	Off / Low / Middle / High

	I. White Balance
	ATW / AWC / Manual / Indoor / Outdoor

	J. LDC(Lens Distortion Correction)
	Off / On (5 levels with min / max)

	K. Electronic Shutter Speed
	Minimum / Maximum / Anti flicker

	L. Flip / Mirror
	Flip / Mirror / Hallway view

	M. Intelligent Video Analytics
	Motion detection with metadata, Tampering

	N. Alarm Triggers
	Motion detection, Tampering detection, SD card error, NAS error

	O. Alarm Events
	File upload via FTP and E-mail
Local storage recording at event
Notification via E-mail

	P. IR Viewable Length
	15m(49.21ft)



2.07	NETWORK PROTOCOL
	A. Ethernet
	RJ-45 (10/100BASE-T)

	B. Video Compression Format
	H.264, MJPEG

	C. Resolution
	1920 x 1080, 1280 x 960, 1280 x 720, 1024 x 768,
800 x 600, 720 x 576, 640 x 480, 320 x 240

	D. Max. Framerate
	

	
	1. H.264
	Max. 30fps at all resolutions

	
	2. MJPEG
	Max. 1fps@1920 x 1080, 1280 x 960, 1280 x 720, 1024 x 768
Max. 15fps@other resolution

	E. Video Quality Adjustment
	

	
	1. H.264
	Target bitrate level control

	
	2. MJPEG
	Quality level control

	F. Bitrate Control Method
	

	
	1. H.264
	CBR or VBR

	
	2. MJPEG
	VBR

	G. Streaming Capability
	Multiple streaming (Up to 3 profiles)

	H. Audio In
	Built-in mic

	I.  Audio Compression Format
	G.711 u-law / G.726 selectable
G.726 (ADPCM) 8KHz, G.711 8KHz
G.726 : 16Kbps, 24Kbps, 32Kbps, 40Kbps

	J. Audio Communication
	Uni-directional audio

	K. IP
	IPv4, IPv6

	L. Protocol
	TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP, RTSP, NTP, HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP, DNS, DDNS, QoS, PIM-SM, UPnP, Bonjour

	M. Security
	HTTPS(SSL) login authentication
Digest login authentication
IP address filtering
User access log
802.1x authentication

	N. Streaming Method
	Unicast / Multicast

	O. ax. User Access
	6 users at unicast mode

	P. Edge Storage
	micro SD/SDHC max. 32G, NAS
- Motion images recorded in the SD memory card can be downloaded
- Manual recording at local PC

	Q. Application Programming interface
	ONVIF Profile S, G, SUNAPI (HTTP API)

	R. Webpage Language
	English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, Greek, Norwegian, Finnish

	S. Web Viewer
	

	
	1. Supported OS
	Windows XP / VISTA / 7 / 8 / 8.1, MAC OS X 10.7 ~ 10.10

	
	2. Supported Browser
	Microsoft Internet Explorer (Ver. 8 ~ 11), 
Mozilla Firefox (Ver. 9 ~ 35),
Google Chrome (Ver. 15 ~ 40), 
Apple Safari (Ver. 8.0.2(Mac OS X 10.10),
7.0.6(Mac OS X 10.9), 6.0.2 (Mac OS X 10.8, 10.7 only), 5.1.7) * Mac OS X only

	T. Central Management Software
	SmartViewer



2.08	ELECTRICAL
	A. Voltage
	PoE (IEEE802.3af, Class2)

	B. Consumption
	Max. 5.4W



2.09	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature / Humidity
	-10°C ~ +55°C (+14°F ~ +131°F) / Less than 90% RH

	B. Storage Temperature / Humidity
	-30°C ~ +60°C (-22°F ~ +140°F) / Less than 90% RH



2.10	PHYSCIAL SPECIFICATIONS
	A. Dimension
	Ø119.8 x 98.8mm (Ø4.72" x 3.89")

	B. Weight
	290g (0.64 lb)

	C. Color/Material
	Ivory / Plastic



2.11	CERTIFICATIONS	
A. CE mark
B. FCC mark

2.12	WARRANTY
A. 3 years, parts and labor.
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