Page 3 SNO 7084R 3 MEGAPIXEL WEATHERPROOF NETWORK IR CAMERA	

SNO 7084R 3 MEGAPIXEL WEATHERPROOF NETWORK IR CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SNB 7084R 3 MEGAPIXEL WEATHERPROOF NETWORK IR CAMERA
1. [bookmark: _GoBack]The camera shall be of a bullet type suitable for external installation. The camera shall be dark grey in appearance with an aluminium body and integrated wall bracket.
1. The camera shall feature an Adaptive Infrared illumination system with 20 LEDs giving a viewable distance of 30m (98.43ft) in complete darkness. 
1. The network camera shall feature up to 3 Mega Pixel resolution in a 16:9 format. 4:3 format shall also be available in smaller resolutions.

2.03	CAMERA
A. Imaging Device	1/ 2.8” PS Exmor 3.2M CMOS
B. Total Pixels 	2,065(H) x 1,565(V)
C. Effective Pixels 	2,065(H) x 1,553(V)
D. Scanning System	Progressive 
E. Min. Illumination
1. Color				0.1 Lux (F1.2, 50IRE), 
					0.06Lux (F1.2, 30IRE)		     
 2. B/W 				0 Lux (F1.2, 50IRE)
					0 Lux (F1.2, 30IRE)
F. S / N Ratio	50dB
G. Video Output	CVBS : 1.0 Vp-p / 75Ω composite, 704x480(N), 				704x576(P), for installation
			- DIP connector type

2.04	LENS TYPE
A. Focal Length (Zoom Ratio)		3 ~ 8.5mm (2.8x) motorized varifocal
B. Max. Aperture Ratio			F1.2
C. Angular Field of View			H : 100.12°(Wide) ~ 35.38°(Tele) / 
					V : 73.76°(Wide) ~ 26.58°(Tele)
D. Min. Object Distance			0.5m (1.64ft)\

E. Lens Type	Simple Focus / DC Auto Iris, P-Iris
F. Mount Type	Board-in type
	G. Focus Control			Simple focus (Motorized V/F) / Manual, 
						Remote control via network (Manual, Simple focus)

2.05	OPERATION
	A. IR LED				20ea
B. Viewable Length	30m(98.43ft)
C Camera Title 	Off / On (Displayed up to 45 characters)
D Day & Night 	Auto (ICR) / Color / B/W / External / Schedule
E Backlight Compensation		Off, BLC, WDR
F Wide Dynamic Range 	120dB 
G Contrast Enhancement `	SSDR (Samsung Super Dynamic Range) (Off / On)
H. Digital Noise Reduction 	SSNRIII (2D + 3D noise filter) (Off  / On)
I. Motion Detection 	Off / On (4ea 4 Points Polygonal zones)
J. Privacy Masking 			Off / On (32ea Rectangular zones)
K. Gain Control 	Off / Low / Middle / High
L. White Balance 	ATW / AWC / Manual / Indoor / Outdoor
M. Electronic Shutter Speed 	Minimum / Maximum / Anti flicker (1 ~ 1/12,000sec)
N. Flip / Mirror 	Off, On
O. Intelligent Video Analytics	Tampering, Virtual Line, Enter/Exit, Appear / Disappear, 
		Audio Detection, Face Detection with metadata
P. Alarm I/O 	Input 1ea / Output 1ea
Q. Alarm Triggers 	Motion detection, Tampering, Audio Detection, Face 			Detection, Video Analytics, Alarm Input, Network 			Disconnection
R. Alarm Events	File upload via FTP and E-Mail Notification via E-Mail, local storage(SD/SDHC/SDXC) recording at Network disconnected & Event (Alarm Triggers) External output
S. Defog	Auto/Manual/Off
T. Digital Image Stabilization	Off / On

2.06	NETWORK PROTOCOL
A. Ethernet 	RJ-45 (10/100Base-T)
B. Video Compression Format 	H.264(MPEG-4 part 10/AVC), MJPEG
C. Resolution 	2048 x 1536 / 1920x1080 / 1600x1200 / 1280x1024 			/ 1280x960 / 1280x720 / 1024x768 / 800x600 / 800x450 			/ 640x480 / 640x360 /  320x240 / 320x180
D. Max. Framerate 	
	1. H.264	Max 30fps@2048x1536, Max 60fps at all resolutions
	       2. Motion JPEG			Max. 10fps@2048 x 1536Max. 15fps@1920 x 1080,
			1600 x 1200, 1280 x 1024, 1280 x 960, 1280 x 720,
			1024 x 768Max. 30fps@800 x 600, 800 x 450, 				640 x 480, 640 x 360, 320 x 240, 320 x 180
	 E. Smart Codec	Manual mode (Area-based : 5ea), Face detection mode
F. Video Quality Adjustment 	
	1. H.264 	Compression level, Target bit rate level control
	2. MJPEG 	Quality level control
G. Bitrate Control Method 	
	1, H.264	CBR or VBR
	2. MJPEG 	VBR
H. Streaming Capability 	Multiple Streaming (Up to 10 Profiles)
I. Audio In	Selectable (Mic in / Line in / Built-in mic), 
			Supply voltage : 2.5V DC (4mA), 
			Input impedance : approx. 2K Ohm
J. Audio Out	Line out (3.5mm mono jack), Max output level : 1 Vrms
K.  Audio Compression Format 	G.711 u-law /G.726 Selectable
			G.726 (ADPCM) 8KHz, G.711 8KHz
			G.726 : 16Kbps, 24Kbps, 32Kbps, 40Kbps
L. Audio Communication 	Bi-directional audio
M. IP 		IPv4, IPv6
N. Protocol 				TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP, RTSP, 							NTP, HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, 							ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP, DNS, 							DDNS, QoS, PIM-SM, UPnP, Bonjour
O. Security 				HTTPS(SSL) Login Authentication
					Digest Login Authentication
					IP Address Filtering
					User access Log
					802.1x Authentication
P. Streaming Method 	Unicast, Multicast
Q. Max. User Access 	15 users at Unicast mode
R. Edge Storage				micro SD/SDHC/SDXC
					4GB SD memory built-in, Motion images recorded in 
					the SDXC/SDHC/SD memory card can be downloaded
S. Application Programming interface 	ONVIF profile S, SUNAPI (HTTP API) v2.0, SVNP 1.2
T. Webpage Language 			English, French, German, Spanish, Italian, Chinese, 					  		Korean, Russian, Japanese, Swedish, Danish, 								Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, 							Dutch, Croatian, Hungarian, Greek, Norwegian, Finnish
U. Web Viewer 
1. Supported OS 	Windows XP / VISTA / 7 / 8, MAC OS X 10.7
2. Supported Browser	Microsoft Internet Explorer (Ver. 7~10), 
		Mozilla Firefox (Ver. 9~19), 
		Google Chrome (Ver. 15~25), 
		Apple Safari (Ver. 6.0.2(Mac OS X 10.8, 10.7 Only), 			5.1.7)
		* Mac OS X Only
3. Central Management Software 	SmartViewer

2.07	ELECTRICAL
A. Voltage	AC24V±10%, DC12V±10%,PoE(IEEE802.3af,Class3)
B. Consumption	Max. 13.0W / 19.0W (AC 24V, Heater off / on)
			Max. 11.5W (DC 12V)
			Max. 12.5W (PoE, Class3)

2.08	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature / Humidity	-10°C ~ +55°C (14°F ~ 131°F) 
			Less than 90% RH
B. Storage Temperature / Humidity	-30°C ~ +60°C (-22°F ~ +140°F)
			Less than 90% RH
C. Ingress Protection	IP66
D. Vandal Resistance	IK10

2.09	PHYSCIAL SPECIFICATIONS
A. Dimension	90.4 x 96.0 x 333.2mm (3.56” x 3.78” x 13.12”)
B. Weight	1.19Kg(2.62lb)
C. Color	Dark gray / Aluminium
2.10	CERTIFICATIONS	
A. CE mark
B. FCC mark

2.11	WARRANTY
A. 3 years, parts and labor.
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