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SNP-3430H NETWORK CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.
D.	All systems and components shall be provided with a one-day turnaround repair express and 24-hour parts replacement. The repair and parts express shall be guaranteed by the manufacturer on warranty and nonwarranty items.

2.02	SNP-3430H NETWORK CAMERA
A.	The camera shall provide 1/4” 600TV lines resolution and a minimum illumination performance to 0.7 Lux. 
B.	The camera shall provide high-speed pan and tilt at 360° tilt and 180° range.
C.	In addition, these models include a WDR backlight compensation, VPS, and intelligent video analytics.

2.03 ELECTRICAL SPECIFICATIONS
A. Input Voltage/Current 		Class 2 24V~50/60Hz, hPOE44~57V
B. Power Consumption		Max. 20W, if heater off
Max 50W, if heater on
hPOE 24W

2.04 	VIDEO SPECIFICATIONS
A. Imaging Device		1/4" Ex-view HAD PS CCD
B. Total Pixels		
	1. NTSC 		811(H) x 508(V)
	2. PAL		795(H) x (596 (V)
C. Effective Pixels		
	1. NTSC		768(H) x 494(V)
	2. PAL		752 (H) x 582 (V)
D. Scanning System		Progressive (if VPS On), Interlaced Scan (if WDR On)
E. Synchronization		Internal
F. Frequency		
	1. NTSC		15.734KHz (H), 59.94Hz (V)
	2  PAL 		15.625KHz (H), 50 Hz (V)
G. Horizontal Resolution		Color: 600 TV Lines in color 
H. Min. Illumination		Color : 0.7Lux (50 IRE@F1.6), 
B/W : 0.007Lux (50 IRE@F1.6)
I. S / N (Y signal) 		52dB 
J. I. Video Output		CVBS: 1.0 Vp-p, 75Ω composite

2.05	LENS
A. Zoom Ratio		43x
B. Focal Length		3.2 ~ 138.5mm
C. Max. Aperture Ratio		F1.6(Wide) ~ F3.7(Tele)
D. Min. Object Distance		100cm (3.28 ft)
E. Angular Field of View		61.2°(Wide) ~ 1.47°(Tele) (H)
47.2°(Wide) ~ 1.1°(Tele) (V)
F. Focus		AF, One-Shot AF, Manual
G. Zoom Movement Speed		Max. 3.2 sec (Wide Tele)
H. Lens Type		DC Auto Iris
I. Mount Type		Board-in

2.06 	PAN/TILT/ROTATE
A. Pan Range		360° endless
B. Pan Speed		Preset : 360°/sec  
			Manual: 0.05°/sec ~ 200°/sec
C. Tilt Range		180° (0° ~ 180°)
D. Tilt Speed		Preset: 360°/sec 
Manual: 0.05°/sec ~ 200°/sec
E. Preset Positions		255 each

2.07 	OPERATIONAL SPECIFICATIONS
A. On-Screen Display		English	
B. Camera Title		On, Off (Displays up to 32 characters)
C. Day & Night		Auto (IRC), Color, B/W
D. Motion Detection		Yes
E. Wide Dynamic Range	
	1. NTSC		128x
	2. PAL		160x
F. Backlight Compensation		Off, BLC
G. Contrast Enhancement		XDR (eXtended Dynamic Range)
(Off, Low, Medium, High)
H. Digital Image Stabilization		On, Off
I. Privacy Masking		On, Off (12 polygonal programmable zones)
J. Digital Noise Reduction		Motion adaptive 2D+3D Noise Filter
(Off, Low, Medium, High)
K. Sens-up (Frame Integration)		Off, Auto (2x ~ 512x)
L. Gain Control		Off, Low, Medium, High, Manual
M. White Balance		AWT (in), ATW (out), AWC, Manual
N. Electronic Shutter Speed		
	1. NTSC		Off, A.Flk, Manual (1/120 ~ 1/10,000sec) 
	2. PAL		Off, A.Flk, Manual (1/100 ~ 1/10,000sec)
O. Digital Zoom		16x
P. Flip		Off, On
Q. Profile		Yes
R. VPS		Off, On
S. Intelligent Video Analytics		Moved, Fixed
T. PIP		Off, On
U. Schedule		Day/Time schedule
V. Communication		RS-485/422, Coaxial control
W. RS-485 Protocol		Samsung-T, Samsung-E, Pelco-D, Pelco-P, 
		Panasonic, Honeywell (DK6), Honeywell (VCLTP),
				Vicon, GE (Kalatel) and AD
X. Alarm		8 In, 4 Out (Relay)

2.08.	NETWORK
A. Ethernet 		RJ-45 (10/100 BASE-T)
B. Video Compression Format		H.264, MPEG4, MJPEG
C. Resolution		7
	1. NTSC		704 x 480, 640x480, 352x240
	2. PAL		704 x 576, 640x480, 352x288
D. Frame Rate
	1. NTSC		30 fps
	2. PAL		25 fls
E. Video Quality Adjustmen		H.264/MPEG4: Compression Level, Target Bitrate Level
MJPEG : Quality Level Control
F. Bitrate Control Method		H.264/MPEG4: CBR or VBR
			MJPEG : VBR
G. Streaming Capability 		Multiple Streaming (Up to 10 Profiles)
H. Audio I/O		Line in / Line out
I. Audio Compression Format 		G.711 μ-law
J. Audio Communication		2-Way
K. IP 		IPv4, IPv6
L. Protocol 		TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTSP, NTP,
 HTTP, HTTPS, SSL,DHCP, PPPoE, FTP, SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP,DNS, DDNS
M. Security		HTTPS(SSL) Login Authentication, 
Digest Login Authentication, IP Address Filtering,
User access Log
N. Streaming Method 		Unicast / Multicast
O. Max. User Access 		10 users at Unicast Mode
P. Memory Slot 		SD/SDHC Memory Slot
Q. ONVIF Conformance 		Yes
R. Web Viewer Supported OS		Windows XP, Windows VISTA, Windows 7
MAC OS
S. Supported Browser		Internet Explorer 6.0 or Higher, Firefox, Chrome, Safari
T. Central Management		NET-I Viewer

2.09	ENVIRONMENTAL
A. Operating Temperature 		-50°C ~ +50°C (-58°F ~ +122°F)
B. Operating Humidity		20% ~80% RH
C. Ingress Protection		IP66 (waterproof)

2.10 	MECHANICAL 
A. Dimension		ø178mm x  290.5
B. Weight		4.5 kh

2.11	CERTIFICATIONS 
A. FCC (Class A), UL/cUL Listed
B. CE (Class A), UL/cUL Listed

2.12	WARRANTY
A. 3 years parts and service
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