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SNP-6201 2MEGAPIXEL FULL HD NETWORK PTZ DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SNP-6201 2MEGAPIXEL FULL HD NETWORK PTZ DOME CAMERA
A. These cameras shall support multi-streaming technologies, transferring real-time high
resolution images at 30 fps with video compression in H.264 and MJPEG codec.

B. The camera shall provide 4.45~89mm (20x) optical zoom with 8x digital zoom. It shall
support PoE plus, SD memory, and bi-directional audio.

C. All operation and configuration menus shall be provided in English, Korean, Japanese,
Chinese, French, German, Spanish, Italian, Russian, Polish, Czech, Turkish, Dutch, Portuguese, 
Swedish, Danish, Thai, Romanian, Serbian, Croatian, Hungarian, and Greek.

D. The camera shall be of a dome type suitable for internal installation. The camera shall be ivory 
    in appearance.

E. The camera shall feature a motorized pan and tilt mechanism capable of panning at 500°/s and 
     tilt movement at 500°/s

F. The camera should be capable of capturing an image size of 1920x1080 at 30 images per
    second

G. The camera shall feature a day / night mode that incorporates an infrared cut filter removal
[bookmark: _GoBack]    mechanism for true colour reproduction and the best possible low light performance

H. The camera shall feature a 20x zoom lens with continuous and one shot autofocus functions

2.03 ELECTRICAL SPECIFICATIONS
A. Input Voltage	24V AC, PoE+ (IEEE802.3af)
B. Power Consumption, max.	PoE+ : Max 13W, 24V AC : Max 15W
2.04	CAMERA	
A. Imaging Device	1/3” 2M PS CMOS
B. Total Pixels (horizontal x vertical)	2,010(H) x 1,108(V)
C. Effective Pixels (horizontal x vertical)	1,944(H) x 1,092(V) 
D. Scanning System	Progressive
E. Min. Illumination
	1. Color	1.5Lux (F1.6, 50IRE) 
	2. B/W	0.1Lux(F1.6, 50IRE)
F. S / N ratio	50dB
G. Video Output	CVBS:1.0 Vp-p
	1. NTSC	704x480, for installation
	2. PAL	704x576, for installation

2.05	LENS
A. Focus control	Auto / Manual / Oneshot
B. Drive Type	DC auto iris
C. Mount Type	Board-in type
	D. Focal Length(Zoom Ratio)		4.45mm ~ 89mm(20X)
	E. Max. Aperture Ratio			F1.6(Wide)/F2.9(Tele)
	F. Angular Field of View			H:63°(Wide) ~ 3.49°(Tele) / V: 37°(Wide) ~ 1.99°(Tele)
	G. Min. Object Distance			1m(3.28ft)

2.06	PAN/TILT/ROTATE
	A. Pan/Tilt Range			360°Endless / 210°(-15° ~ 195°)
	B. Pan/Tilt Speed			Preset : 500°/sec, Manual : 0.024°/sec ~ 120°/sec
	C. Preset / Preset Accuracy		255ea / +-0.2°

2.07	OPERATIONAL SPECIFICATION
A. Camera Title	On, Off (displays up to 15 characters)
B. Day and Night	Auto (ICR), Color, B/W
C. Backlight Compensation	BLC, HLC, Off
D. Digital Noise Reduction 	SSNR   Off, On
E. Wide Dynamic Range	Off, On
F. Motion Detection	Yes(4ea)
G. Privacy Masking	On, Off (12 programmable zones)
H. Sens-up (Frame Integration)	Off, Auto (2x ~ 60x)
I. Gain Control	Off, Low, Medium, High, Manual 
J. White Balance	AWC, Manual, Indoor, Outdoor, ATW(2,400°K~11,000°K)
K. Electronic Shutter Speed	ESC, FLK, Manual (1/30~33,000sec)
L. Flip/Mirror	Off, On
M. Intelligent Video Analytics	Tampering, Virtual line, Enter / Exit, Appear / Disappear, 			Audio detection, Face detection(5ea) 
N. Alarm I/O	Input 4ea / Output 2ea(relay). 
O. Wide Dynamic Range	60dB
P. Alarm Triggers	Alarm input, Motion detection, Intelligent video analytics, 			Network disconnect
Q. Alarm Events	File upload via FTP, E-Mail, Notification via E-Mail and 			TCP, Local storage(SD/SDHC) recording at Network 			disconnected, External output, PTZ preset

2.08	NETWORK
A. Ethernet	RJ-45 (10/100Base-T)
B. Video Compression	H.264,MJPEG  
C. Resolution 	1920 x 1080p(Full HD), 1280 x 1024, 1280 x 960, 
		1280 x 720P (HD), 1024 x 768, 800 x 600, 640 x 480, 320 x 240
D. Max Frame rate	30fps at all resolutions *when WDR on, Max. 
		framerate is Max. 15fps. 
E. Video Quality
	1. H.264	Compression level, Target bit rate level control
	2. MJPEG	Quality level control
F. Bitrate Control
	1. H.264	VBR or CBR
	2. MJPEG	VBR
G. Streaming	Multiple, up to 10 profiles
H. IP		IPv4, IPv6			
I. Network Protocol	TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP, 
			HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
	IGMP,  SNMPv1, v2c, v3 (MIB-2), ARP, DNS, DDNS, QoS, ONVIF, PIM-SM, UPnP
J. Security	HTTPS (SSL) login authentication, Digest login 
		authentication, IP Address filtering, User access log,
			802.1x authentication. 
K. Streaming Method	Unicast, Multicast
L. User Access 	10 users at Unicast 
M. Memory Slot	SD/SDHC memory slot
N. ONVIF Conformance	Yes
O. Webpage Language	English, French, German, Spanish, Italian, Chinese, 
		Korean, Russian, Japanese, Swedish, Danish, 
		Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, 
		Dutch, Croatian, Hungarian, and Greek
P. Web Viewer
	1. Supported OS	Windows XP, Windows Vista, Windows 7, MAC OS
	2. Supported Browser	Internet Explorer 7.0 or higher, Firefox, Chrome, Safari
Q. Central Management Software	Smart Viewer

2.09	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-10°C ~ +55°C (+14°F ~ +131°F)
B. Operating Humidity		20% ~ 80% RH
C. Vandal Resistance	SNP-6201 only
			(When SNP-6201 + SHP-3701H : IK 10 	accessary 			housing)

2.10	PHYSCIAL SPECIFICATIONS
A. Dimension	Ø152.0 x 218.0mm (Ø5.98” X 8.58”)
B. Weight	1.8kg (3.97 lb) 
C. Color	Ivory 
D. Material	Plastic

2.11	CERTIFICATIONS	
A. UL Listed
B. CE mark
C. FCC mark

2.12	WARRANTY
A. 3 years
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