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SNV 5084 1.3MEGAPIXEL HD VANDAL-RESISTANT NETWORK DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A. All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B. All systems and components shall have been thoroughly tested and proven in actual use.
C. All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SNV 5084 1.3MEGAPIXEL HD VANDAL-RESISTANT NETWORK DOME CAMERA
A. The camera shall be of a dome type suitable for outdoor installation. The camera shall be ivory in appearance with a aluminum body.
B. The camera shall provide video compression dual codec ( H.264 and MJPEG). 
C. The network camera shall feature up to 1.3 Megapixel resolution in a 16:9 format.
D. The camera shall provide Defog and WDR.
E. The camera shall provide Audio, Face and Motion detection.
F. The camera shall provide memory slot for SD, SDHC and SDXC.
G. The camera shall provide Multi-crop streaming.
H. The camera shall support Bi-directional audio.
I. All operation and configuration menus shall be provided in English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, Greek, Norwegian, and Finnish.

2.03	CAMERA	
	A. Imaging Device
	1/3" 1.3M CMOS

	B. Total Pixels
	1,312(H) x 1,069(V)

	C. Effective Pixels
	1,305(H) x 1,049(V)

	D. Scanning System
	Progressive

	E. Min. Illumination
	

	
	1. Color
	0.05Lux (1/30sec, F1.2, 50IRE)
0.0008Lux (2sec, F1.2, 50IRE)
0.008Lux (1/30sec, F1.2, 30IRE)

	
	2. B/W
	0.005Lux (1/30sec, F1.2, 50IRE)
0.002Lux (1/30sec, F1.2, 30IRE)

	F. S/N Ratio
	50dB

	G. Video Output
	CVBS : 1.0 Vpp / 75Ω composite, 720 x 480(N), 720 x 576(P), for installation
DIP connector type



2.04	LENS TYPE
	A. Focal Length (Zoom Ratio)
	3 ~ 8.5mm (2.8x) motorized varifocal

	B. Max. Aperture Ratio
	F1.2

	C. Angular Field of View
	H : 93.3°(Wide) ~ 33.2°(Tele) 
V : 73.7°(Wide) ~ 26.6°(Tele)

	D. Min. Object Distance
	0.5m (1.64ft)

	E. Lens Type
	DC auto iris, P-Iris

	F. Mount Type
	Board-in type

	G. Focus Control
	Simple focus (Motorized V/F) / Manual
Remote control via network (Manual, Simple focus)



2.05	PAN/TILT/ROTATE
	A. Pan Range
	0° ~ 354° 

	B. Tilt Range
	0° ~ 67° 

	C. Rotate Range
	0° ~ 355°



2.06	OPERATION
	A. Camera Title
	Off / On (Displayed up to 40 characters)

	B. Day & Night
	Auto (ICR) / Color / B/W / External / Schedule

	C. Backlight Compensation
	Off / BLC

	D. Wide Dynamic Range
	130dB

	E. Contrast Enhancement
	SSDR (Samsung Super Dynamic Range) (Off / On)

	F. Digital Noise Reduction
	SSNRIII (2D+3D noise filter) (Off / On)

	G. Digital Image Stabilization
	Off / On

	H. Defog
	Off / Auto / Manual

	I. Motion Detection
	Off / On (4ea 4 points polygonal zones)

	J. Privacy Masking
	Off / On (32 zones with 4 points of polygonal)

	K. Gain Control
	Off / Low / Middle / High

	L. White Balance
	ATW / AWC / Manual / Indoor / Outdoor

	M. Electronic Shutter Speed
	Minimum / Maximum / Anti flicker (2 ~ 1/12,000sec)

	N. Flip / Mirror
	Off / On

	O. Intelligent Video Analytics
	Tampering, Virtual line, Enter / Exit, (Dis)Appear, Audio detection, Face detection

	P. Alarm I/O
	Input 1ea / Output 1ea

	Q. Alarm Triggers
	Motion detection, Tampering, Audio detection, 
Face detection, Video analytics, 
Network disconnection, Alarm input

	R. Alarm Events
	File upload via FTP and E-mail
Notification via E-mail
Local storage (SD/SDHC/SDXC) or NAS recording at Event (Alarm triggers)
External output



2.07	NETWORK PROTOCOL
	A. Ethernet
	RJ-45 (10/100BASE-T)

	B. Video Compression Format
	H.264 (MPEG-4 part 10/AVC), MJPEG

	C. Resolution
	1280 x 1024, 1280 x 720P (HD), 1024 x 768, 800 x 600, 640 x 480, 320 x 240

	D. Max. Framerate
	

	
	1. H.264
	Max. 60fps @ all resolutions

	
	2. MJPEG
	Max. 30fps @ all resolutions

	E. Video Quality Adjustment
	

	
	1. H.264
	Compression level, Target bitrate level control

	
	2. MJPEG
	Quality level control

	F. Bitrate Control Method
	

	
	1. H.264
	CBR or VBR

	
	2. MJPEG
	VBR

	G. Streaming Capability
	Multiple streaming (Up to 10 profiles)

	H. Audio In
	Selectable (Mic in / Line in), Max output level : 1 Vrms
Supply voltage : 2.5V DC (4mA), Input impedance : approx. 2K Ohm

	I. Audio Out
	Line out (3.5mm stereo mini jack)

	J.  Audio Compression Format
	G.711 u-law/G.726 selectable
G.726 (ADPCM) 8KHz, G.711 8KHz
G.726 : 16Kbps, 24Kbps, 32Kbps, 40Kbps

	K. Audio Communication
	Bi-directional audio

	L. IP
	IPv4, IPv6

	M. Protocol
	TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP,RTSP, NTP, HTTP, HTTPS, SSL, DHCP, PPPoE, FTP,
SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP, DNS, DDNS, QoS, PIM-SM, UPnP, Bonjour

	N. Security
	HTTPS(SSL) login authentication, Digest login authentication
IP address filtering, User access log, 802.1x authentication

	O. Streaming Method
	Unicast / Multicast

	P. Max. User Access
	15 users at unicast mode

	Q. Edge Storage
	SD/SDHC/SDXC - motion Images recorded in the SD/SDHC/SDXC memory card can be downloaded. NAS (Network Attached Storage)

	R. Application Programming interface
	ONVIF profile S, HTTP API (SUNAPI) 2.0, SVNP 1.2

	S. Webpage Language
	English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, Greek, Finnish, Norwegian

	T. Web Viewer
	

	
	1. Supported OS
	Windows XP / VISTA / 7 / 8 / 8.1, MAC OS X 10.7

	
	2. Supported Browser
	Microsoft Internet Explorer (Ver. 11 ~ 8)
Mozilla Firefox (Ver. 19 ~ 9) * Windows only
Google Chrome (Ver. 25 ~ 15) * Windows only
Apple Safari (Ver. 6.0.2(Mac OS X 10.8, 10.7 only), 5.1.7) * Mac OS X only

	U. Central Management Software
	SmartViewer



2.08	ELECTRICAL
	A. Voltage
	12V DC, 24V AC, PoE (IEEE802.3af, Class3)

	B. Consumption
	Max. 12.95W (PoE - Heater on), Max. 14W (12V DC, 24V AC - Heater on)



2.09	ENVIRONMENTAL SPECIFICATIONS
	A. Operating Temperature / Humidity
	-40°C ~ +55°C (-40°F ~ +131°F) / Less than 90% RH
* Start up should be done at above -35°C (-31°F)

	B. Storage Temperature / Humidity
	-30°C ~ +60°C (-22°F ~ +140°F) / Less than 90% RH

	C. Ingress Protection
	IP66

	D. Vandal Resistance
	IK10



2.10	PHYSCIAL SPECIFICATIONS
	A. Dimension
	Ø160.0 x 118.5mm (Ø6.3" x 4.67")

	B. Weight
	985g (2.17 lb)

	C. Color/Material
	Ivory / Aluminum



2.11	CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark


2.12	WARRANTY
A. 3 years, parts and labor.
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