
Page Page 2Page  SNV-7080 3Megapixel Full HD Vandal-Resistent Network Dome Camera
SNV-7080 3MEGAPIXEL FULL HD VANDAL-RESISTENT NETWORK DOME CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
PART 2 – PRODUCTS
2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.
2.02	SNV-7080 3MEGAPIXEL FULL HD VANDAL-RESISTENT NETWORK DOME CAMERA
A.	This network dome camera shall provide resolution support of at least 3M (2048x1536) with 16:9 full HD (1080p) resolution.
B.	The camera shall have 3 ~ 8.5mm motorized varifocal (2.8x) lens.
C.	The camera shall support simultaneous transmission of dual codec (H.264 and MJPEG), with smart codec (ROI encoding).
D.	The camera shall support WDR in 2M mode.
E.	This camera shall have an IP66 vandal-resistant, waterproof body.
F.	The camera shall provide a customizable on-screen display (OSD) which shall be available in English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Romanian, Serbian, Dutch, Croatian, Hungarian, and Greek.
2.03	ELECTRICAL SPECIFICATIONS
A. Input Voltage	24V AC, 12V DC, PoE (IEEE802.3af)
B. Power Consumption, max.	7W (heater off); 11W (heater on)
2.04	CAMERA
A. Imaging Device	1/2.8” 3M PS CMOS
B. Total Pixels (horizontal x vertical)	2,144 x 1,588
C. Effective Pixels (horizontal x vertical)	2,096 x 1,561
D. Scanning System	Progressive
E. Min. Illumination
1. Color	0.1Lux (F1.2, 50IRE), 0.017 Lux (Sens-up, 60x)
2. Black/White	0.08Lux (F1.2, 50IRE), 0.001 Lux (Sens-up, 60x)
F. SN Ratio	50dB
G. Video Output	CVBS: 1.0 Vp-p, 75 ohms composite
1. NTSC	704x480, for installation
2. PAL	704x576, for installation
2.05	LENS
A. Focal Length (Zoom Ratio)	3~ 8.5mm (2.8x) motorized varifocal
B. Aperture ratio, max.	F1.2


C. Angular Field of View	H: 100°(Wide) ~ 35.3°(Tele)
V: 74.6°(Wide) ~ 26°(Tele)
D. Min. Object Distance	0.5m (1.64ft)
E. Focus control	Remote control via network (Manual, One-shot AF)
F. Drive Type	DC auto iris
G. Mount Type	Board-in
2.06	PAN/TILT
A. Pan Range	0° ~ 355°
B. Tilt Range	0° ~ 90°
C. Rotate Range	0° ~ 355°
2.07	OPERATIONAL SPECIFICATIONS
A. Camera Title	Off, On (displays 15 characters)
B. Day and Night	Auto (ICR), Color, B/W, External B/W
C. Backlight Compensation	BLC, HLC, WDR, Off
D. Wide Dynamic Range	52dB (2M mode only)
E. Contract Enhancement, SSDR	Off, On
F. Digital Noise Reduction,
SSNRIII 2D+3D noise filter	Off, On
G. Motion Detection	Off, On (4 programmable zones)
H. Privacy Masking	Off, On (1 each, 4 point polygonal + 16 each rectangular
zones)
I. Sens-up (Frame Integration)	Off, Auto (2x ~ 60x)
J. Gain Control	Off, Low, Medium, High
K. White Balance	ATW AWC, Manual, Indoor, Outdoor
L. Electronic Shutter Speed	Auto, A.FLK, Manual (1/30~30,000sec)
M. Flip/Mirror	Off, On
N. Alarm I/O	Input, 1 each. Output, 1 each (relay)
2.08	NETWORK
A. Ethernet	RJ-45 (10/100Base-T)
B. Video Compression	H.264, MJPEG
C. Resolution 3M
1. H.264	20fps max, all resolutions
2. MJPEG	800 x 600 ~ 320 x 180, 20fps
1280 x 1024 ~1600 x 1200, 15fps
1920 x 1080 ~ 2048 x 1536, 10fps
D. Resolution 2M
1. H.264	30fps max, all resolutions but 15fps if WDR is on
2. MJPEG	800 x 600 ~ 320 x 180, 30fps
1280 x 1024 ~1920 x 10800, 15fps
E. Max Framerate
1. 3M Mode	20fps
2. 3M Mode	30fps max. 15fps if WDR is on
F. Smart Codec	Area based method, Face detection method
G. Video Quality Adjustment
1. H.264	Compression level, Target bitrate level control
2. MJPEG	Quality level control
H. Bitrate Control
1. H.264, MPEG-4	VBR or CBR
2. MJPEG	VBR
I. Streaming	Multiple, up to 6 profiles
J. Audio I/O	Mic/ Line in, Line Out
K. Audio Compression Format	G.711 u-law
L. Audio Communication	Bi-directional audio


M. IP	IPv4, IPv6
N. Network Protocol	TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP,
HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
IGMP, SNMPv1, v2c, v3 (MIB-2), ARP, DNS, DDNS,
ONVIF
O. Security	HTTPS (SSL) login authentication, Digest login
authentication, IP Address filtering, User access log,
802.1x authentication
P. Streaming Method	Unicast, Multicast
Q. User Access	10 users at Unicast level
R. Memory Slot	SD/SDHC
S. ONVIF Conformance	Yes
T. Webpage Language	English, French, German, Spanish, Italian, Chinese,
Korean, Russian, Japanese, Swedish, Danish,
Portuguese, Turkish, Polish, Czech, Romanian, Serbian,
Dutch, Croatian, Hungarian, and Greek
U. Web Viewer
1. Supported OS	Windows XP, Windows Vista, Windows 7, MAC OS
2. Supported Browser	Internet Explorer 6.0 or higher, Firefox, Chrome, Safari
V. Central Management Software	NET-i Viewer
2.09	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-40°C ~ +50°C (-40°F ~ +122°F)
B. Operating Humidity	<90% RH
C. Ingress Protection	IP66 (Waterproof)
2.10	PHYSCIAL SPECIFICATIONS
A. Dimension	Ø160 x 134.5mm (Ø6.3" x 5.3")
B. Weight	1.4Kg (3.09lb)
C. Color	Ivory
D. Materials	Aluminum
2.11	CERTIFICATIONS
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark
2.12	WARRANTY
A. 3 years, parts and labor.
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