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SNV 7082 3 MEGAPIXEL FULL HD VANDAL-RESISTANT NETWORK CAMERA
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
PART 2 – PRODUCTS
2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.
2.02	SNV 7082 3 MEGAPIXEL FULL HD VANDAL-RESISTANT NETWORK CAMERA
A.	The network camera shall offer 3M resolution (2048 x 1536) with 16:9 full HD (1080p) resolution support.
B.	The camera shall provide video compression dual codec ( H.264 and MJPEG).
C.	The camera shall provide WDR and Smart codec (ROI encoding).
D.	The camera shall provide a customizable on-screen display (OSD) which shall be available in English, French, German, Spanish, Italian, Chinese, Korean, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, and Greek.
2.03	CAMERA
A. Imaging Device	1. 3” 3.1M PS CMOS
B. Total Pixels	2,064(H) x 1,578(V)
C. Effective Pixels	2,052(H) x 1,536(V)
D. Scanning System	Progressive
F. Min. Illumination
1. Color	0.7Lux (F1.2, 50IRE), 0.011Lux (Sens-up 60x)
2. B/W	0.07Lux (F1.2, 50IRE), 0.001Lux (Sens-up 60x)
G. S / N Ratio	50dB
H. Video Output	CVBS:  1.0Vp-p / 75ohm composite, 704x480(N),
704x576(P), for installation
2.04	LENS TYPE
A. Lens Type	Manual, DC auto iris
B. Mount Type	C/CS
2.05	OPERATION
A. Camera Title	Off, On (Displayed up to 15 characters)
B. Day & Night	Auto (ICR), Color, B/W, External B/W
C. Backlight Compensation	Off, BLC, HLC, WDR
D. Wide Dynamic Range	Off, / On (96dB) 3M mode : 20fps 2M mode : 30fps
E. Contrast Enhancement SSDR	On, Off
F. Digital Noise Reduction SSNRIII	On, Off
G. Motion Detection	Off, On (4 programmable zones)
H. Privacy Masking	Off, On (1 each 4 point-polygonal and 16 each
rectangular zone)
I. Sens-up (Frame Integration)	Off, Auto (2x ~ 60x)
J. Gain Control	Off, Low, Middle, High
K. White Balance	ATW, AWC, Manual, Indoor, Outdoor
L. Electronic Shutter Speed	Auto, A.FLK, Manual (1/30 ~ 12,000sec)
M. Flip / Mirror	Off, On
N. Intelligent Video Analytics	Audio detection, Face detection, Tampering, Virtual line, Enter / Exit, Appear / Disappear
O. Alarm I/O	Digital 1/1
P. Alarm Triggers	Motion detection, Video analytics, Sensor input
Q. Alarm Events	File upload via FTP, E-mail / Notification via E-mail,
TCP / Local storage (SD/SDHC) recording at network disconnected,
External output
2.06	NETWORK PROTOCOL
A. Ethernet	RJ-45 (10/100Base-T)
B. Video Compression Format	H.264(MPEG-4 part 10/AVC), MJPEG
C. Resolution
1. 3M Mode, H.264	Max 20 fps at all resolutions
2. 3M Mode, MJPEG	800 x 600 ~ 320 x 180, 20fps
1280 x 1024 ~1600 x 1200, 15fps
1920 x 1080 ~ 2048 x 1536, 10fps
3. 2M Mode, H.264	Max. 30fps at all resolutions
4. 2M Mode, MJPEG	800 x 600 ~ 320 x 180, 30fps
1280 x 1024 ~ 1920 x 1080, 15fps
D. Max. Framerate
1. 3M Mode	20fps
2. 2M Mode	30fps
E. Video Quality Adjustment
1. H.264	Compression level, Target bit rate level control
2. MJPEG	Quality level control
F. Bitrate Control Method
1, H.264	CBR or VBR
2. MJPEG	VBR
G. Streaming Capability	Multiple streaming (Up to 6 profiles)
H. Audio I/O	Mic/ Line in, Line out
I. Audio Compression Format	G.711 u-law, G.726 (16kbps, 24kbps, 32kbps, 40kbps)
J. Audio Communication	Bi-directional audio
K. IP	IPv4, IPv6
L. Protocol	TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTSP, NTP,
HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
IGMP, SNMPv1, v2c, v3(MIB-2), ARP, DNS, DDNS,
QOS, UPNP, ONVIF
M. Security	HTTPS(SSL) login authentication,
Digest login authentication, IP address filtering,
User access log, 802.1x authentication
N. Streaming Method	Unicast, Multicast
O. Max. User Access	10 users at Unicast mode
P. Memory Slot	SD/SDHC memory slot
Q. ONVIF Conformance	Yes
R. Webpage Language	English, French, German, Spanish, Italian, Chinese,
Korean, Russian, Japanese, Swedish, Danish,
Portuguese, Turkish, Polish, Czech, Rumanian, Serbian,
Dutch, Croatian, Hungarian, and Greek
S. Web Viewer
1. Supported OS	Windows XP, Windows Vista, Windows 7,
Mac OS X 10.7 or higher
2. Supported Browser	Internet Explorer 7.0 or higher, Firefox, Chrome, Safari
T. Central Management Software	NET-i viewer
2.07	ELECTRICAL
A. Voltage	12V DC, PoE (IEEE802.3af)
B. Consumption	Maximum 9W (12V DC, PoE(Class3) – Heater off) ,
Maximum 12.95W(PoE(Class3) – Heater on)
2.08	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-10°C ~ +55°C (14°F ~ 131°F)
B. Operating Humidity	20% ~ 80% RH
2.09	PHYSCIAL SPECIFICATIONS
A. Dimension (WxH)	Ø160.0 x 134.5mm (Ø6.3” x 5.3”)
B. Weight	1.42Kg (3.13 lb)
C. Color	Ivory
D. Material	Aluminum
2.10	CERTIFICATIONS
A. CE mark
B. FCC mark
2.11	WARRANTY
A. 3 years, parts and labor.
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