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SNV-8081R 5Megapixel Vandal-Resistant Network IR Dome Camera
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer. The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SNV-8081R 5Megapixel Vandal-Resistant Network IR Dome Camera
A. The camera shall feature up to 5M resolution with frame rate of 30 fps. At 2M resolution, it shall feature frame rate of 60 fps.  
B. The minimum illumination shall be 0.15Lux at the aperture ratio of F1.3 in color mode. In black and white mode with IR LED on, it shall be 0Lux. 
C. The camera shall feature motorized varifocal lens which varies between 3.93mm and 9.4mm.
D. The camera shall feature H.265, H.264 and MJPEG codec. 
E. The camera shall feature Day & Night mode with a removable infrared cut filter (ICR) for precise color reproduction and the best possible low light performance. 
F. The camera shall feature intelligent video and audio analytics such as tampering and audio detection.
G. The camera shall provide memory slots for SD/SDHC/SDXC and support recording to NAS and local PC.
H. The camera shall provide hallway view which rotates the scene to 90 or 270 degrees. The hallway view is particularly useful for corridors where vertical view is desired.
I. The camera shall feature LDC (Lens Distortion Correction) which corrects the distortions caused by lens of camera for true reproduction of objects. 
J. The camera shall provide IP66 and IK10 ratings to prove strong protection against solid and liquid objects and impact.
2.03	CAMERA
A. Imaging Device	1/1.8” 6M CMOS
B. Total Pixels 	3,096(H) x 2,094(V)
C. Effective Pixels 	2,616(H) x 1,976(V)
D. Scanning System	Progressive 
E. Min. Illumination
1. Color				0.3Lux (1/30sec, F1.3, 50IRE)
0.005Lux (2sec, F1.3, 50IRE)
0.15Lux (1/30sec, F1.3, 30IRE) 
0.003Lux (2sec, F1.3, 30IRE)	
2. B/W 	      			0Lux (IR LED on)
F. S / N Ratio	50dB
G. Video Output	CVBS: 1.0 Vpp / 75Ω composite, 704 x 480(N), 704 x 576(P), for installation
		DIP connector type
2.04	LENS TYPE
A. Focal Length (Zoom Ratio)		3.93 ~ 9.4mm (2.4x) motorized varifocal
B. Max. Aperture Ratio			F1.3
C. Angular Field of View			H: 93.4°(Wide) ~ 39.2°(Tele)  
V: 68.1°(Wide) ~ 29.3°(Tele) 
D. Min. Object Distance			0.5m (1.64ft)\
E. Lens Type	DC auto iris, support P-Iris mode
F. Mount Type	Board-in type
	G. Focus Control			Simple focus (Motorized V/F) 
Manual, Remote control via network 
(Manual, Simple focus)
2.05	PAN / TILT / ROTATE
	A. Pan / Tilt / Rotate Range		0° ~ 354° / 0° ~ 67° / 0° ~ 355°
2.06	OPERATION
A. Viewable Length	30m (98.43ft), Smart IR
B. Camera Title	Off / On (Displayed up to 15 characters)
C. Day & Night	Auto (ICR) / Color / B/W / External / Schedule
D. Backlight Compensation	Off / BLC / WDR
E. Wide Dynamic Range	120dB
F. Contrast Enhancement	SSDR (Samsung Super Dynamic Range) (Off / On)
G. Digital Noise Reduction	SSNR (2D+3D noise filter) (Off / On)
H. Motion Detection	Off / On (4ea, Rectangle)
I. Privacy Masking	Off / On (6ea, Rectangle) - Color: Black / Blue / Red / Grey / White / Green
J. Gain Control	Off / Low / Medium / High
K. White Balance	ATW / AWC / Manual / Indoor / Outdoor (Include mecury & Sodium)
L. LDC (Lens Distortion Correction)	Off / On (Level auto control)
M. Electronic Shutter Speed	Minimum / Maximum / Anti flicker (2 ~ 1/12,000sec)
N. Flip / Mirror	Off / On, Hallway : 90° /270°
O. Intelligent Video Analytics	Tampering, Audio detection - with metadata
P. Alarm I/O	Input 1ea / Output 1ea
Q. Alarm Triggers	Alarm input, Motion detection, Tampering, Audio detection, Network disconnect
R. Alarm Events	File upload via FTP and E-mail, Notification via E-mail
		Local storage (SD/SDHC/SDXC) or NAS recording at event triggers, External output
S. Pixel Counter	Support

2.07	NETWORK PROTOCOL
A. Ethernet 	RJ-45 (10/100BASE-T)
B. Video Compression Format 	H.265: Main, 
	H.264 (MPEG-4 part 10/AVC): Main / Baseline / High, MJPEG






C. Resolution 
1. 5M Mode	2592 x 1944, 2592 x 1464, 1920 x 1080, 1600 x 1200, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 720 x 576, 720 x 480, 640 x 480, 320 x 240
2. 2M Mode	1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 720 x 576, 720 x 480, 640 x 480, 320 x 240 
D. Max. Frame rate 	
	1. 5M Mode	H.265 / H.264 - 30fps in all resolutions
			MJPEG - 2592 x 1944 ~ 2592 x 1464: 2fps, 
			1920 x 1080 ~ 1600 x 1200: 4fps 
			1280 x 1024 ~ 1024 x 768: 5fps, 
			800 x 600 ~ 320 x 240: 15fps	
	2. 2M Mode	H.265 / H.264 - 60fps in all resolutions
			MJPEG - 1920 x 1080: 4fps, 
			1280 x 1024 ~ 1024 x 768: 5fps, 
			800 x 600 ~ 240: 15fps 
E. Smart Codec	Manual mode (Area-based: 4ea)
F. Video Quality Adjustment 	
	1. H.264 / H.265	Compression level, Target bitrate level control
	2. MJPEG 	Quality level control
G. Bitrate Control Method 	
	1, H.264 / H.265	CBR or VBR
	2. MJPEG 	VBR
H. Streaming Capability 	Multiple streaming (Up to 3 profiles) - Total 3 stream at the same time (Including recording stream)
I. Audio In	Selectable (Mic. in / Line in)
			Supply voltage: 2.5V DC (4mA) 
			Input impedance: approx. 2K Ohm
J. Audio Out	Line out (3.5mm stereo mini jack)
			Max output level: 1Vrms
K.  Audio Compression Format 	G.711 u-law/G.726 selectable, G.726 (ADPCM): 8KHz, G.711: 8KHz, G.726: 16Kbps, 24Kbps, 32Kbps, 40Kbps
L. Audio Communication 	Bi-directional audio (2-way)
M. IP 		IPv4, IPv6
N. Protocol 	TCP/IP, UDP/IP, RTP(UDP), RTP(TCP), RTCP, RTSP, NTP, HTTP, HTTPS, SSL, DHCP, PPPoE, FTP,
SMTP, ICMP, IGMP, SNMPv1/v2c/v3(MIB-2), ARP, DNS, DDNS, QoS, PIM-SM, UPnP, Bonjour
O. Security 	HTTPS(SSL) login authentication, Digest login authentication, IP address filtering, User access log, 802.1x authentication (EAP-TLS, EAP-LEAP)
P. Streaming Method 	Unicast, Multicast
Q. Max. User Access 	10 users at Unicast mode
R. Edge Storage 	SD/SDHC/SDXC (128GB) - Motion images recorded in the SD/SDHC/SDXC memory card can be downloaded, Camera can detect automatically when the memory is connected, Memory status display (Normal / Error / Active / Formatting / Lock), NAS (Network Attached Storage), Local PC for instant recording
S. Application Programming Interface 	ONVIF profile S, SUNAPI (HTTP API), SVNP, Samsung Techwin Open Platform 
T. Webpage Language 	English, French, German, Spanish, Italian, Chinese, Russian, Japanese, Swedish, Danish, Portuguese, Turkish, Polish, Czech, Rumanian, Serbian, Dutch, Croatian, Hungarian, Greek 
U. Web Viewer 
1. Supported OS 	Windows XP / VISTA / 7 / 8 / 8.1 or higher
	MAC OS X 10.7 ~ 10.10
	2. Supported Browser		Microsoft Internet Explorer (Ver. 8 ~ 11),
				Mozilla Firefox (Ver. 9 ~ 35), 
				Google Chrome (Ver. 15 ~ 40),
	Apple Safari (Ver. 8.0.2 (Mac OS X 10.10), 7.0.6 (Mac OS X 10.9), 6.0.2 (Mac OS X 10.8, 10.7 only), 5.1.7) 
	* Mac OS X only
V. Central Management Software 	SmartViewer, SSM

2.08	ELECTRICAL
A. Input Voltage / Current	24V AC ±10%, 12V DC ±10% 
		PoE (IEEE802.3af, Class3)
B. Consumption	Max. 12W/13.5W (24V AC, Heater off / on) 
		Max. 10W/11.5W (12V DC, Heater off / on)
		Max. 11.5W/12.95W (PoE, Heater off / on)

2.09	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-40°C ~ +55°C (40°F ~ 131°F) 
			Startup should be done at above -35°C(-31°F)
B. Operating Humidity	Less than 90% RH
C. Storage Temperature	-30°C ~ +60°C (-22°F ~ +140°F)
D. Storage Humidity	Less than 90% RH
E. Ingress Protection	IP66
F. Vandal Resistance	IK10

2.10	PHYSICAL SPECIFICATIONS
A. Dimension (WxHxD)	Φ160.0 x 118.5mm (Φ6.3” x 4.67”)
B. Weight	955g (2.11 lb.)
C. Color	Ivory
D. Material	Aluminum

2.10     CERTIFICATIONS	
A. CE mark
B. FCC mark
C. UL mark

2.11      WARRANTY
[bookmark: _GoBack]A. 3 years, parts and labor.
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