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Hanwha Techwin is a leading supplier of advanced video surveillance solutions for IP-video, analog and hybrid systems. Building on the company's history of innovation, Hanwha Techwin is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-efficiency. Hanwha Techwin is committed to the continued development of innovative systems products for professional security applications.
For additional information, visit http://security.hanwhatechwin.com/ .
2 MP VANDAL RESISTANT NETWORK IR FLAT CAMERA
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
Notes to Specifier:

1.  Where several alternative parameters or specifications exist, or where, the specifier has the option of inserting text, such choices are presented in <bold text>.
2.  Explanatory notes and comments are presented in colored text.

Important:  See further notes on the following page.

Important Note to Security Systems Specifiers

CSI MasterFormat 2016 incorporates numerous significant changes affecting electronic safety and security. This document is written to provide flexibility in using either format, although adoption of MasterFormat 2016 is encouraged. The following is a guide to the MasterFormat numbers relevant to the product referenced in this specification.

Primary Specification Area:

MasterFormat 2014:

28 20 00 
Electronic Surveillance

28 23 00 
Video Surveillance




28 23 29
Video Surveillance Remote Devices and Sensors

MasterFormat 2016:

28 20 00
Video Surveillance



28 2x xx
Surveillance Cameras




28 2x xx
IP Cameras

Related Requirements:

MasterFormat 2014:


27 20 00 Data Communications 


28 23 13 Video Surveillance Control and Management Systems


28 23 16 Video Surveillance Monitoring and Supervisory Interfaces


28 23 19 Digital Video Recorders and Analog Recording Devices


28 23 23 Video Surveillance Systems Infrastructure
MasterFormat 2016


27 15 01.xx
Video Surveillance Communications Conductors and Cables 

27 20 00 
Data Communications 

28 05 xx.xx
PoE Power Sources for Electronic Safety and Security 

28 05 xx
Storage Appliances for Electronic Safety and Security 


28 05 xx.xx
Network Video Recorders 

28 05 xx
Cyber Requirements for Electronic Safety and Security


28 05 xx
Safety and Security Network Communications Equipment 

28 2x 00
Video Management System
2 MP VANDAL RESISTANT NETWORK IR FLAT CAMERA

PART  1   GENERAL

1.01 SUMMARY
A. Section includes a full HD IP video camera with built-in 3.6mm fixed lens. 
B. Product - A 2 MP IP video camera, with multi-streaming H.264 and MJPEG capability in a vandal resistant IP66/IK10 rated dome housing with integral IR illuminator.
C. Related Requirements
Refer to MasterFormat notes at the beginning of this document to select requirements specific to the MasterFormat version being used in the specification.

1.02 REFERENCES
A. Abbreviations
1. AGC - Automatic Gain Control
2. ARP – Address Resolution Protocol
3. AWB  - Automatic White Balance
4. BLC – Back light compression
5. CBR – Constant Bit Rate

6. CVBS – Color, Video, Blanking, Sync
7. DHCP - Dynamic Host Configuration Protocol
8. DNR – Digital Noise Reduction
9. DNS - Domain Name Server
10. DDNS – Dynamic Domain Name Server
11. DSCP – Differentiated Services Code Point
12. fps - frames per second
13. FTP - File Transfer Protocol
14. GOV – Group of Video
15. GUI – Graphical User Interface
16. HD – High Definition
17. HTTP - Hypertext Transfer Protocol
18. ICMP – Internet Control Message Protocol
19. IGMP - Internet Group Management Protocol
20. IP - Internet Protocol
21. JPEG - Joint Photographic Experts Group
22. MJPEG - Motion JPEG
23. MP - Megapixel
24. MPEG - Moving Pictures Experts Group
25. NAS – Network Attached Storage
26. NTP - Network Time Protocol
27. PIM-SM - Protocol Independent Multicast-Sparse Mode

28. PoE - Power over Ethernet
29. PPPoE – Point to Point Protocol over Ethernet
30. RTP - Real-Time Transport Protocol
31. RTCP – Real-Time Control Protocol
32. RTSP - Real-Time Streaming Protocol
33. SDK – Software Development Kit
34. SMTP - Simple Mail Transfer Protocol
35. SNMP – Simple Network Management Protocol
36. SSL – Secure Sockets Layer
37. TCP - Transmission Control Protocol
38. UDP - User Datagram Protocol
39. UPnP – Universal Plug and Play
40. VBR – Variable Bit Rate
41. VMS - Video Management System
42. WDR – Wide Dynamic Range
43. LDC – Lens Distortion Control
B. Reference Standards
1. Network - IEEE
a. 802.3 Ethernet Standards

b. 802.1x  Port-based Network Access Control
2. Video

a. ISO / IEC 14496–10, MPEG-4 Part 10 ( ITU H.264)

b. ISO / IEC 10918 – JPEG 
c. ONVIF – Profiles S and G
3. Emissions
a. FCC-47 CFR Part 15 Subpart B Class B
b. CE EN 55022:2010
4. Immunity - CE

a. EN 50130-4:2011 

b. EN 61000-3-3:2014 

c. EN 61000-4-2:2009

d. EN 61000-4-3:2006+A2:2010

e. EN 61000-4-4:2012

f. EN 61000-4-5:2014

g. EN 61000-4-6:2009

5. Safety

a. UL listed

b. CE EN 50581:2012 (hazardous substances)
6. Ingress Protection and Vandal Resistance
a. ANSI / IEC60529 – Degrees of Protection Provided by Enclosures – IP66
b. IEC EN 62262 - Degrees of protection provided by enclosures for electrical equipment against external mechanical impacts – IK10

c. IEC 60068-2-75

C. Definitions

1. GOV (Group of Video object planes) - A set of video frames for H.264 compression, indicating a collection of frames from the initial I-Frame (key frame) to the next I-Frame. GOV consists of 2 kinds of frames: I-Frame and P-Frame.
2. Multi-exposure wide dynamic range - Operation which  automatically adjusts shutter speed to provide a wide range between dark and light areas visible at the same time, preventing backlighting issues. Long exposure is used for bright areas and a short exposure is used in dark areas.
3. Smart Codec – Operation in which the camera adaptively alters the video compression for a portion of the camera’s field of view to improve the quality of video in the area specified.
1.03 SUBMITTALS
A. Product Data
1. Manufacturer’s printed or electronic data sheets
2. Manufacturer’s installation and operation manuals
3. Warranty documentation

1.04 QUALIFICATIONS
A. Manufacturer shall have a minimum of five years’ experience in producing IP video equipment.
B. Installers shall be trained and authorized by the Manufacturer to install, integrate, test, and commission the system.
1.05 DELIVERY, STORAGE AND HANDLING

A. Deliver the camera in the manufacturer’s original, unopened, undamaged container with identification labels intact.
B. Store the camera in a temperature environment of -30° C to 60° C (-22° F to 140° F), protected from mechanical and environmental conditions as designated by the manufacturer.
1.06 WARRANTY, LICENSING AND SUPPORT
A. Manufacturer shall provide a limited 3 year warranty for the product to be free of defects in material and workmanship.
B. Manufacturer shall provide embedded camera video analytics free of license charges.

END OF SECTION

PART  2  PRODUCTS

2.01 EQUIPMENT
A. Manufacturer: 
Hanwha Techwin
http://security.hanwhatechwin.com/
B. Model

SNV-L6013R
C. Alternates: 

None

2.02 GENERAL DESCRIPTION

A. Video Compression and Transmission – The 2 MP camera shall have the following properties relating to the video signals it produces.
1. H.264 and MJPEG compression, each derived from a dedicated encoder and capable of being streamed independently and simultaneously

a. H.264 – frame rates to 30 fps

b. MJPEG – frame rates to 15 fps

Maximum frame rates are available at selected resolutions:

H.264: 30 fps is available at all resolutions

MJPEG: 15 fps available up to and including 800 x 600 resolutions: 1 fps at all higher resolutions

2. The 2 MP camera shall be able to configure up to 10 independent video stream profiles with differing encoding, quality, frame rate, resolution, and bit rate settings. 
3. Resolution selections

a. 1080p (1920 x 1080) and 720p (1280 x 720) HD

b. 1280 x 960, 1024 x 768, 800 x 600, 720 x 576, 640 x 480, 320 x 240
4. Simultaneous unicast access by up to 6 users

5. Multicast or unicast capable

6. Dynamic DNS (DDNS) support

B. Camera – The 2 MP camera device shall have the following physical and performance properties:
1. Dustproof, waterproof, and IP66 rated.
2. NEMA 250 type 4x enclosure.
3. Railway standards including EN50155 class T3 and EN50121
4. True day/night operation with removable IR cut filter
a. Low light level operation to 0.003 lux (color) and 0 lux (black and white)

5. 2D and 3D digital noise reduction

6. Integral IR illumination, providing effective visibility of 15m at 0 Lux when activated in Black & White mode.
7. 6 privacy masking regions utilizing a 4 point polygon
C. Intelligence and Analytics – The 2 MP camera shall have a suite of integral intelligent operations and analytic functions to include:

1. Motion detection with four definable detection areas, minimum / maximum object size definition and a learning algorithm that ignores false alarms such as trees and waves on water.

2. Detection of logical events of specified conditions from the camera’s video input

a. camera tamper (scene change)
D. Interoperability – The 2 MP camera shall be ONVIF Profile S and G compliant.
E. The 2 MP camera shall possess the following further characteristics:
1. Built-in web server, accessed via standard browsers including Internet Explorer, Firefox, Chrome & Safari
2. Micro SD/SDHC memory card and NAS recording options, with configurable pre-alarm and post-alarm recording intervals
3. Uni-directional audio
4. Alarms and notifications
a. alarm notification triggers:

1.) motion detection
2.) tampering detection
3.) SD card error
4.) NAS error
b. available notification means upon trigger:

1.) file upload via FTP and e-mail

2.) notification via e-mail

3.) record to local storage (SD card)

5. POE capable
2.03 CAMERA SOFTWARE
A. The 2 MP camera shall have a built in web server which supports browser-based configuration using Internet Explorer, Google Chrome, Mozilla Firefox, and Apple Safari, for which web viewer plug-ins are available, from a PC or Mac. 
B. The web viewer shall provide a monitoring screen which displays live camera video and simultaneously provides same-screen access to the following functions:

1. Live view window size

2. Resolution setting
3. Image (snapshot) capture

4. Manual recording to SD or NAS

5. Audio control

6. Access Playback and Setup menus
C. The web viewer shall provide a playback screen which provides access to the following functions:

1. Search date and time range

2. Search event type

3. Play an event video

4. Set resolution

5. Play audio if present

6. Generate a backup copy of saved video data
D. The web viewer shall provide a setup screen which provides access to the following configuration settings and functions in the camera:

1. Digital video profile to include compression type, maximum or target bit rate, frame rate, multicast parameters, crop encoding area

2. User profile to include password, access level, authentication
3. Date and time

4. Network settings and IP version

a. DDNS

b. SSL, including certificate management

c. 802.1x authentication

d. Quality of Service settings

e. SNMP to include version selection and settings

f. Auto configuration

5. Video setup to include flip and mirror mode, hallway view mode, video type, privacy zone 

6. Audio setup to include source, audio codec type, gain, and bit rate

7. Camera settings to include image preset, sensor frame capture, dynamic range, white balance, back light, exposure, day/night operation, on-screen display, IR illumination, sharpness, contrast, color level, lens distortion control.
8. Event detection setup to include notification parameters, recording rules, time schedule, tamper protection, motion detection, event triggers
9. System function to include reboot, upgrade, check system and event logs, application (SDK) management

10. View profile information

E. Minimum client hardware requirements
1. Processor:
a. 1920x1080 30 fps: 
 Intel Core 2 Duo 2.4 GHz or higher

2. RAM:


2 GB 

3. Acceptable Operating Systems:
Windows XP / VISTA / 7 / 8 / 8.1, MAC OS X 10.7~10.10
4. Display:


1280X1024 pixels or higher (32 bit color)
5. Acceptable browsers:
Microsoft Internet Explorer, Mozilla Firefox, Google Chrome, Apple Safari

2.04 DETAILED SPECIFICATIONS

A. Video
1. Imager
a. Sensor:


1/2.9" 2.19 MP CMOS
1.) pixels per sensor:
2000 (H) x 1121(V) total; 1984 (H) x 1105 (V) effective
2.) scanning
:
progressive
b. Minimum illumination

1.) Color mode: 

0.15Lux (1/30 sec, F1.8), 0.003Lux (2sec, F1.8)
2.) Black & white mode: 
0Lux (IR LED on)
c. The following features with control settings shall be available:

1.) Backlight compensation (BLC):

On/Off

2.) Camera title:



 up to 15 characters

3.) Contrast enhancement:


On/Off (Samsung Super Dynamic Range)
4.) Day/night setting:


Auto, Color, Black & White,  External, Schedule

5.) Digital Noise Reduction (DNR):

On/Off

6.) Electronic shutter speed: 


a.) settings:



min, max, anti-flicker
7.) Image flip:



On/Off

8.) Image mirror:



On/Off
9.) Hallway view:



On/Off
10.) Automatic gain control:


3 levels or Off

11.) Motion detection

a.) 4 zones with 4 sided polygon

b.) selectable for On/Off

12.) Privacy masking

a.) 6 zones with 4 sided polygon

b.) selectable for On/Off

d. Lens:


3.6 mm, fixed
1.) Angle of view:

H : 86.5° / V : 47.8° / D : 101.2°
2.) Focus control:

manual
3.) Maximum aperture ratio:   F1.8
4.) Minimum objet distance: 0.5 m (1.64ft)
e. Manual positional settings:
a.) pan:

-5o – 5o
b.) tilt:


0 – 67o
c.) rotation

90o
2. IR Viewable Length:

15 m (49.21ft)
3. Video Streams 
a. The 2 MP camera shall be able to produce 10 video profiles, each of which may have the following properties:
1.) Encoding type:
a.) H.264
b.) MJPEG
2.) Resolution:

1920 x 1080, 1280 x 960, 1280 x 720, 1024 x 768,

800 x 600, 720 x 576, 640 x 480, 320 x 240



3.) Bit rate control method:
a.) H.264


i. target bitrate level control 
ii. constant bit rate (CBR) or variable bit rate (VBR)
b.) MJPEG
i. quality level control
ii. variable bit rate (VBR)
4.) Maximum frame rate:

a.) H.264:

30 fps at all resolutions
b.) MJPEG:
i. 15fps @ 800 x 600, 720 x 576, 640 x 480, 320 x 240
ii. 1fps @ 1920 x 1080, 1280 x 960, 1280 x 720, 1024 x 768
4. Number of multi-streaming profiles:
3 maximum 

5. Simultaneous users (total):

6 maximum (unicast)
6. Storage and Recording
a. The 2 MP camera shall have onboard SD card storage.
1.) Card type:
 Micro SD/SDHC
2.) Capacity:
4 GB – 32 GB per card
3.) Image content on the card shall have the ability to be downloaded to a selected destination.
7. Interoperability - Video streams shall be capable of supporting ONVIF protocol, profiles S and G.
8. Single Images - The 2 MP camera shall support jpg file image screenshot and export.
B. Network
1. Connectivity: 
10/100 Base-T Ethernet via RJ-45 connector
2. Protocols supported:
a. Transmission Control Protocol (TCP), Internet Protocol (IP) v4 and v6, User Datagram Protocol (UDP)
b. Configuration: Dynamic Host Configuration Protocol (DHCP)
c. Web services: Hypertext Transfer Protocol (HTTP), Secure HTTP (HTTPS)
d. Network services: Address Resolution Protocol (ARP), Bonjour, Domain Name System (DNS), Internet Control Message Protocol (ICMP), Network Time Protocol (NTP), Protocol Independent Multicast-Sparse Mode (PIM-SM), Simple Network Management Protocol (SNMP v1/2c/3 – MIB-2), Universal Plug and Play (UPnP)
e. Media: Real-Time Transport Protocol (RTP), Real-Time Control Protocol, Real-Time Streaming Protocol (RTSP)
f. Multicast: Internet Group Management Protocol (IGMP)

g. Notifications: File Transfer Protocol (FTP), Simple Mail Transfer Protocol (SMTP)
h. Remote Access: Point-to-Point Protocol over Ethernet) (PPPoE)

3. DDNS – The 2 MP camera shall support DDNS services offered by the Manufacturer and other publicly available service offerings.
4. Quality of Service (QoS) – Layer 3 DSCP
5. Security features: 
a. user password protection
b. IP address filtering - list of allowed or blocked IP addresses 
c. HTTPS(SSL) login authentication

d. HTTPS(SSL) secured communications

e. Digest login authentication

f.  User access log 

g. 802.1x authentication

6. Discovery - Manufacturer shall offer a discovery program to identify all devices of his manufacture on the network.
C. Audio

1. Direction:


uni-directional

2. I/O



Line-in
3. Compression:
a. G.711 u-law/G.726 selectable 

1.) G.726 (ADPCM) 8KHz, G.711 8KHz

2.) G.726: 16Kbps, 24Kbps, 32Kbps, 40Kbps
D. Electrical
1. Power
a. Input Voltage / Current
PoE (IEEE802.3af, Class2)
b. Power Consumption:
<5.8 W
c. Ethernet: 


RJ-45 connector
E. Mechanical And Environmental
1. Material: 
a. Housing:


metal, vandal resistant
2. Dimensions (W x H):

99.0 x 52.0 (3.9 x 2.05 in.). 
3. Temperature: 


a. Operating: 


-30° C to 55° C (-22° F to 131° F)
b. Storage:  


-30° C to 60° C (-22° F to 140° F)
4. Humidity:


0 - 90%, non-condensing
5. Environmental Rating:

a. Ingress Protection



IP66, NEMA 250 type 4x
b. Mechanical (Vandal) Protection

IK10
c. Vibration, Shock, Bump, Temperature
EN50155 class T3 (Railway)
d. Electromagnetic Compatibility 

EN50121 (Railway)
e. Vibration




ISO 16750-3 (Road)

END OF SECTION
PART  3    EXECUTION
3.01 INSTALLERS
A. Contractor personnel shall comply with all applicable state and local licensing requirements.
3.02 PREPARATION

A. The network design and configuration shall be verified for compatibility and performance with the camera(s). 
B. Network configuration shall be tested and qualified by the Contractor prior to camera installation.

C. All firmware found in products shall be the latest and most up-to-date provided by the manufacturer, or of a version as specified by the provider of the Video Management Application (VMA) or Network Video Recorder (NVR). 

D. All equipment requiring users to log on using a password shall be configured with user/site-specific password/passwords. No system/product default passwords shall be allowed.
3.03 INSTALLATION
A. The Contractor shall carefully follow instructions in documentation provided by the manufacturer to insure all steps have been taken to provide a reliable, easy-to-operate system.

B. All equipment shall be tested and configured in accordance with instructions provided by the manufacturer prior to installation.

C. Before permanent installation of the system, the Contractor shall test the system in conditions simulating the final installed environment.
3.04 STORAGE

A. The 2 MP camera hardware shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.
END OF SECTION
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