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SPE-100 1CH NETWORK VIDEO ENCODER 
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SPE-100 1CH NETWORK VIDEO ENCODER
A.  This video encoder shall provide a maximum of 30 fps at NTSC, an 35 fps at PAL, with 4CIF resolution.
B.  The encoder shall support simultaneous transmission of multiple codec (H.264, MPEG-4 and MJPEG).
C. 	The encoder shall provide PoE, SD memory, and bi-directional audio support, and Ethernet transfer of 10/100Base-T.

2.03 ELECTRICAL SPECIFICATIONS
A. Input Voltage	12V DC, PoE (IEEE802.3af)
B. Power Consumption, max.	4W
	
2.04	OPERATIONAL	
A. Video In	CVBS: 1.0 Vp-p / 75Ω composite, NTSC/PAL auto-detection
B. Video Out	CVBS: 1.0 Vp-p / 75Ω composite, loop out
C. De-interlacing filter	Built in
D. Event Trigger	Motion Detection, Alarm input, Video loss
E. Alarm I/O	Input, 1 each; Output, 1 each (relay)
F. Remote Control Interface	1 each RS-485 (half duplex)
G. RS-485 Protocol	Samsung-T/E, Pelco-P/D

2.05	NETWORK
A. Ethernet	RJ-45 (10/100Base-T)
B. Video Compression	H.264, MPEG-4, MJPEG  
C. Resolution 	
	1. NTSC	704 x 480, 640 x 480, 352 x 240, 320 x 240
	2. PAL	704 x 576, 640 x 480, 352 x 288, 320 x 240
D. Max Framerate	
	1. NTSC	30fps
	2. PAL	25fps
E. Video Quality
	1. H.264, MPEG-4	Compression level, Target bitrate level control
	2. MJPEG	Quality level control


F. Bitrate Control
	1. H.264, MPEG-4	VBR or CBR
	2. MJPEG	VBR
G. Streaming	Multiple, up to 10 profiles
H. Audio I/O	1 each line in, 1 each line out
I. Audio Compression Format	G.711 u-law
J. Audio Communication	Bi-directional audio
K. IP		IPv4, IPv6			
L. Network Protocol	TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP, 
			HTTP, HTTPS, SSL, DHCP, PPPoE, FTP, SMTP, ICMP,
			IGMP,  SNMPv1, v2c, v3 (MIB-2), ARP, DNS, DDNS, 
			ONVIF
M. Security	HTTPS (SSL) login authentication, Digest login 
		authentication, IP Address filtering, User access log, 
N. Streaming Method	Unicast, Multicast
O. User Access 	10 users at Unicast 
P. Memory Slot	SD/SDHC memory slot
Q. ONVIF Conformance	Yes
R. Web Viewer
	1. Supported OS	Windows XP, Windows Vista, Windows 7, MAC OS
	2. Supported Browser	Internet Explorer 6.0 or higher, Firefox, Chrome, Safari
S. Central Management Software	NET-i Viewer

2.06	ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature	-10°C ~ +50°C (+14°F ~ +122°F)
B. Operating Humidity		20~80% RH

2.07	PHYSCIAL SPECIFICATIONS
A. Dimension	128 x 43.8 x 87.14mm (5.04 x 1.72 x 3.43")
B. Weight	391g (0.87 lb) 
C. Color	Silver 
D. Material	Metal

2.08	CERTIFICATIONS	
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.09	WARRANTY
A. 3 years, parts and labor.
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