Page 2 SPE-400 4CH Network Video Encoder 		D R A F T

SPE-1600R 4SLOT NETWORK VIDEO ENCODER RACK MOUNTED CHASSIS 
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll-free (U.S. and Canada), 24-hour technical assistance program (TAP) from the manufacturer.  The TAP shall allow for immediate technical assistance for either the dealer/installer or the end user at no charge for as long as the product is installed.

2.02	SPE-1600R 4SLOT NETWORK VIDEO ENCODER CHASSIS  (CONNECTIONS)
A.  Expansion Slots 4 Slots for SPE-400B
B.  Connector RJ-45 (10/100/1000BASE-T)


2.03 ENVIRONMENTAL SPECIFICATIONS
A. Operating Temperature 0°C ~ +40°C (+32°F ~ +104°F)
B. Operating Humidity 20% ~ 80% RH
	
2.04	ELECTRICAL
A. Input Voltage / Current AC 100-240V~, 50/60Hz, 0.5A
B. Power Consumption Max. 50W (with SPE-400B x 4)

2.05	MECHANICAL
A. Color / Material Black / Metal
B. Dimensions (WxHxD) 440.0 x 44.0 x 310.5mm (17.32" x 1.73" x 12.22")  
C. Weight 3Kg (6.61 lb)
2.06	CERTIFICATIONS	
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.07	WARRANTY
A. 3 years, parts and labor.
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