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SRD-480D HD-SDI H.264 4 CHANNEL DIGITAL VIDEO RECORDER
TECHNICAL SPECIFICATIONS							SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS 

PART 2 – PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with an explicit manufacturer warranty.


2.02	SRD-480D HD-SDI H.264 4 CHANNEL DIGITAL VIDEO RECORDER

A. The digital video recorder (DVR) shall support 4 camera channels with HD-SDI interface, 1280x720p @ 120fps or 1920x1080p @ 60fps.

B. The DVR shall be equipped with a maximum of 4 internal hard disk drives (HDD), with SATA HDD support.

C. The DVR shall offer combined HDMI and VGA video output for main display; H.264 video compression and ADPCM audio compression; and up to 4 audio inputs and 1 audio output

D. The DVR shall provide network monitoring through built-in Web viewer.

E. All operation and configuration menus shall be provided in several languages, including Korean, Japanese, Chinese, English, French, German, Spanish, Italian, Russian, Polish, Czech, Turkish, Netherlands, Portuguese, Swedish, Danish, Thai, Rumanian, Serbian, Croatian, Hungarian, Greek (22 Language)


2.03	DISPLAY
A.	Video
	1. Inputs	4 HD-SDI SMPTE292M inputs termination
	2. Resolution	1920x1080p
B.	Live
	1. Frame Rate	120fps
	2. Resolution	1920x1080p
	3. Multi Screen Display	1, 4, Sequence

2.04	PERFORMANCE
A. Operating System 	Linux, embedded
B. Recording
	1.  Compression	H.264
	2. Record Rate	1280x720p: 120fps / 1920x1080p: 60fps

	3. Mode	Manual and Event or Schedule and Event
	4. Overwrite Modes	Continuous
	5. Pre Alarm	Up to 15 sec. (1, 2, 3, 4, 5, 10 sec.)
	6. Post Alarm	Up to 60 sec. (1, 2, 3, 4, 5, 10, 15, 20, 25 30, 35, 40, 45, 50, 55, 60 sec.)
C. Search & Playback
	1. Search Mode	Date/Time, Calendar, Event Search, Thumbnail Search
	2. Playback Function		Forward (2x, 4x, 8x, 16x, 32x, 64x) *I-frame only
Forward (1x, 1/2x) *All frame
Backward (1/2x, 1x, 2x, 4x, 8x, 16x, 32x, 64x) *I-frame only
		Step Forward/Backward play at single channel (I+P frame) *All frame
D. Network
	1. Transmission Speed		Dual codec (CIF120fps / 2CIF120fps / 4CIF120fps)
		Single codec (720p, 1080p)
	2. Bandwidth Control	Selectable, Up to (15)Mbps,15M ~ 256kbps
	3. Stream	720p, 1080p (Record encoding), 4CIF / 2CIF / CIF(Dual codec) selectable
	4. Max. Remote Users	Live Monitor 10 (Search 2)
	5. Protocol Support	TCP/IP, DHCP, HTTP, PPPoE, DDNS(iPolis Only), NTP, SMTP, TLS
	6. Monitoring	Webviewer, Samsung CMS
E. Storage (Back up)
	1. Internal HDD	up to 4 SATA HDDs
	2. External HDD	SVS-5R (Only storage support), Total 16TB (Internal+ external)
	3. DVD Writer	Yes (DVD-R, CD-R support)
	4.USB 	2 USB ports
	5. File Format	AVI, EXE (Include player), VFS4 (CD/DVD Playback)
F. Security
	1. Password Protection	1 Admin, 10 Users, User can be assigned authority for function
	2. Data Authentication	Watermark

2.05 	INTERFACE
A. Monitors
	1. VGA	1920x1080p Resolution
	2. HDMI	1920x1080p Resolution
B. Audio
	1. Inputs	4 Line in
	2. Output	1 line
	3. Compression	ADPCM 
	4. Sampling Rate	16KHz
C. Alarm
	1. Inputs	Terminal 4 inputs, NO/NC
	2. Outputs	Terminal 4 relay outputs, NO/NC
	3. Remote Notification	Notification via e-mail
D. Connections
	1. Ethernet	1 RJ-45 10/100/1000 Base-T 
	2. PTZ Control Interface	RS-485
	3. PTZ Keyboard	RS-485
	4. USB	USB 2.0, 2 ports
	5. eSATA	1
	6. Application Support	Mouse, Remote controller

E. Communication Protocols
	1. Supported PTZ Cameras	Samsung-E, Samsung-T, Pelco-D, Pelco-P, 

2.06	GENERAL
A. Electrical 
	1. Input Voltage	100 ~ 240V AC ±10%, 50/60Hz
	2. Power Consumption	Max. 85W (With 1x HDD)
B. Environmental
	1. Operating Temperature	+0°C ~ +40°C (+32°F ~ +104°F)
	2. Operating Humidity	20% ~ 85%RH
C. Dimensions	445 x 88 x 412mm (17.52" x 3.46" x 16.22")
	1. Mechanical Weight 
	  (2x Hard Disks) 	Approx. 9.0Kg (19.84 lb)
	2. Rack Mount Kit	2 each
D. Languages	Korean, Japanese, Chinese, English, French, German, Spanish, Italian, Russian, Polish, Czech, Turkish, Netherlands, Portuguese, Swedish, Danish, Thai, Rumanian, Serbian, Croatian, Hungarian, Greek (22 Language)

2.07	CERTIFICATIONS
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.08	WARRANTY
A. 3 years, parts and labor.
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