
Page Page 2Page  SRD 852D CIF H.264 Digital Video Recorder
SRD-852D 8 CHANNEL CIF H.264 DIGITAL VIDEO RECORDER
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
PART 2 – PRODUCTS
2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with an explicit manufacturer warranty.
2.02	SRD-852 8 CHANNEL CIF H.264 DIGITAL VIDEO RECORDER
A.	The digital video recorder (DVR) shall support 8 channels and provide recording rates of 240 frames per second (fps) on at CIF resolution on NTSC systems and 200 fps at CIF resolution on PAL systems.
B.	The DVR shall provide 4CIF resolution recording capability.
C.	The DVR shall offer SATA HDD support with up to four internal HDD, backup to DVD Writer, and support for iPhone and android phone.
D.	All operation and configuration menus shall be provided in English, Korean, Japanese, Chinese, French, German, Spanish, Italian, Russian, Polish, Czech, Turkish, Dutch, Portuguese, Swedish, Danish, Thai, Romanian, Serbian, Croatian, Hungarian, and Greek.
2.03	DISPLAY
A. Video
1. Inputs	8 composite video 0.5–1 Vp-p, 75 ohm automatic termination
2. Resolution	704x480 NTSC
704x576 PAL
B. Live
1. Frame rate	240fps NTSC
200fps PAL
2. Resolution	704x480 NTSC
704x576 PAL
3. Multi Screen display	1, 4, 6,8, 9, 13, PIP
2.04	PERFORMANCE
A. OS Embedded	Linux
B. Recording
1. Compression	H.264
2. Record Rate NTSC	Up to 60fps @ 704x480
Up to 120fps @ 704x240
Up to 240 @ 352x240
3. Record Rate PAL	Up to 50fps @ 704x576
Up to 100fps @ 704x288
Up to 200fps @ 352x288
4. Mode NTSC	Manual, Schedule (Continuous/Event), Event (Pre/Post),
Time lapse (0.9, 1.9, 3.8, 7.5, 15, 30 fps)
5. Mode PAL	Manual, Schedule (Continuous/Event), Event(Pre/Post),
Time lapse (0.8, 1.6, 3.1, 6.2, 12.5, 25 fps)
6. Event	Video loss, Motion (level 1~10), Alarm
7. Overwrite modes	Continuous
8. Pre-alarm	Up to 5 seconds
9. Post-Alarm	Up to 6 hours (5, 10, 20, 30 seconds; 1, 3, 5, 10, 20 minutes;
1, 2, 3, 4, 5, 6 hours)
C. Search & Playback
1. Search mode	Date/time, Event, Backup, Position, Motion (all search included in
Preview function)
2. Playback function	Fast Forward/Backward, Slow Forward/Backward,
Step Forward/Backward
D. Network
1. Transmission speed	CIF 120/100fps
2. Bandwidth	Up to 8Mbps, 2, 1.5, 1 Mbps; 800, 600, 500, 400, 300, 200, 100, 50 kbps
3. Bandwidth control	Selectable
4. Stream	H.264 (CIF 120 Max.)
5. Remote users	3 Search, 10 Live Unicast, 20 Live Multicast
6. Protocol support	TCP/IP, DHCP, PPPoE, SMTP, NTP, HTTP, DDNS, RTP, RTSP
7. Monitoring	Net-I Viewer, Smart Viewer, Webviewer
E. Smart phone
1. Phone	Android, i-Phone
2. Protocol support	RTSP/RTP(UDP), CGI, HTTP
3. Transmission speed
CIF Max	Wi-Fi: 4fps (Single Channel), 4fps (Quad Channel)
3G: 4fps(Single Channel), 4fps(Quad Channel)
4. Remote users	1, Live
F. Storage
1. Internal HDD	Up to 4 SATA HDDs
2. External HDD/DVD	Not supported
3. DVD Writer (Back-up)	Yes
4. USB (Back-up)	USB 2.0, 2 ports (front)
5. File Format (Back-up)	AVI, BU( DVR player) EXE (includes player)
G. Security
1. Password Protection	1 Admin, 10 Groups, 20 Users per group. Users can be assigned
authority per function
2. Data Authentication	Watermark
2.05	INTERFACE
A. Monitors
1. VGA	1 VGA (800x600, 1024x768, 1280x1024)
2. HDMI	Not supported
3. Main Composite	1 BNC (1 Vp-p, 75 ohm)
4. Spot Composite	Analog Spot 1 BNC (1 Vp-p, 75 ohm)
5. Loop Outputs	Not supported
B. Audio
1. Inputs	4 channel line in (Built in 4 channel, RCA)
2. Output	1 channel line out (RCA)
3. Compression	ADPCM
4. Sampling rate	16KHz
C. Alarm
1. Inputs	Terminal 8 inputs (NO/NC), Terminal 1 inputs (Alarm Reset),
2. Outputs	Terminal 4 relay outputs (NO/NC)
3. Ratings	1A for 24V DC; 0.5A for 125V AC
4. Remote notification	Notification via e-mail
D. Connections
1. Ethernet	1 RJ45 10/100/1000 Base-T
2. Serial interface	RS-232/RS-485 for PTZ, Samsung System Keyboard
3. USB	USB 2.0, 2 ports
4. e-SATA	Not supported
5. Application Support	Mouse, Remote Controller
6. Protocol support	Samsung-E, Samsung-T, Pelco-D, Pelco-P, Panasonic, Phillips,
AD, Diamond, Erna, Kalatel, VCL TP, Vicon
2.06	GENERAL
A. Electrical
1. Input Voltage/Current	100 to 240 VAC ±10%; 50/60 Hz, Autoranging
2. Power consumption	Max. 60W (with 1x HDD)
B. Environmental
1. Operating Temperature	+0°C to +40°C (+32°F to +104°F)
2. Operating Humidity	 20% to 85% RH
C. Mechanical
1. Dimension	440 x 88 x 426.8mm (17.32 x 3.46 x16.8”)
2. Weight w/ hard disks	Approx. 7.5 kg (16.53 lb)
3. Rack mount kit	2 each
D. Language	Korean, Japanese, Chinese, English, French, German, Spanish,
Italian, Russian, Polish, Czech, Turkish, Dutch, Portuguese,
Swedish, Danish, Thai, Romanian, Serbian, Croatian, Hungarian,
and Greek
2.07	CERTIFICATIONS
A.	UL Listed
B.	UL Listed to Canadian safety standards
C.	CE mark
D.	FCC mark
2.08	WARRANTY
A.	3 years, parts and labor.
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