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SRM-872 8-CHANNEL MOBILE NETWORK VIDEO RECORDER
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

1.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with an explicit manufacturer warranty.

1.02	SRM-872 8-CHANNEL MOBILE NETWORK VIDEO RECORDER
A. The mobile network video recorder (NVR) shall support up to 8 network cameras and shall be compatible with ONVIF compliant network cameras. The NVR will have the throughput of 64mbps for recording and 64mbps for network transmission
[bookmark: _GoBack]B. The NVR shall support H.264 and MJPEG Multiple codec.

1.03	DISPLAY
A. N/W Camera
1. Inputs 				Up to 8 network camera support
2. Resolution			CIF, VGA, 4CIF, 1.3M, 2M, 3M
3. Protocols 	Samsung, ONVIF
B. LIVE
1. Local Display	HDMI / VGA
	2. Multi Screen Display	1 / 4 / 9 / Sequence, 8x D-zoom

1.04	PERFORMANCE	
 A. OS Embedded 			Linux
 B. Recording
1. Compression			H.264, MJPEG
2. Recording Bit Rate 		64Mbps
3. Resolution			CIF ~ 3M
4. Mode				Manual, Schedule (Continuous/Event), 
					Event (Pre/Post)
5. Event Trigger			Alarm input(8), Video loss,IP Camera event(Sensor, MD, 					Video Analytics)
6. Event Action			E-mail, Alarm out
	C. Search & Playback
	       1. Search mode			Date/time(calendar), Event log list
	       2. Playback function 		Fast Forward/Backward, Move one step up, 
						Move one step down
	       3. Playback bandwidth		64Mbps(8Ch simultaneously)
	       4. Simultaneous Playback		8CH@1280x720(1M) / 4CH@1920x1080(2M)
4CH 80fps@2048x1536(3M) / 1CH 60fps@1920x1080(2M)
	       5. Resolution			CIF ~ 3M
	       6. Playback Function		Fast forward, backward, Move one step up/ down

	D. Storage
	         1. Built-in	HDD			2.5” HDD 1ea(SSD Compatible)
2. Max. internal HDD 		1ea, Max. 1TB(Hot swap)
	         3. Flash Memory 			Micro SD 1ea, Max. 32GB

	E. Back up
	      1. File back up(Via Web)		[GUI] : BU / Exe, [Network]:JPEG / AVI
	      2. Function				Single channel play, date-time / Title display
	F. Sensor			
	      1. I/O				8 / 4(NO / NC selectable)
	G. Audio
	      1. Inputs				8CH(Network)
	      2. Compression			G.711, G.726
	      3. Audio Communication		2-way

H. Network
	       1. Interface 			RJ-45, Gigabit Ethernet x 12ea(Total)
						IP CAM data in / Power out : 8ea, Control boc] : 1ea
Network : 1ea, IO box 1 : 1ea, IO box 2 : 1ea
	       2. Transmission speed 		Total Throughput Bandwidth Max : 64Mbps
						Transmission Bandwidth Max 	  : 64Mbps
	       3. Remote users 			3 Search, 10 Live Unicast, 20 Live Multicast
4. Protocol support 			TCP/IP, DHCP, PPPoE, SMTP, NTP, HTTP, DDNS,
RTP, RTSP
	       5. Viewer Software 			Type : Webviewer, SmartViewer auto, iPOLIS auto
						CMS support : SDK
	       6. Security				Password, Watermark
	       7. Smart Phone			OS : Android, iOS
						Protocol Support : RTP, RTSP, HTTP, CGI
	       8. IP				IPv4 / IPv6
	       9. Language			English, French, German, Spanish, Italian, Korean,
Russian, Swedish, Denish, Portuguese, Czech, Polish,	 Turkish, Rumanian, Serbian, Dutch, Croatian,
Hungarian, Greek, Finnish, Norwegian
	      10. Web Browser			IE 7.x ~ IE 9.x, IE 10
	      11. OS				Window : XP SP2 or above, Vista, 7, 8 /
Mac OS : OSX 10.4.8 or above
	
	F. Function				
	      1. Power Management		Shutdown Delay : 1 min ~ 30 min(User selectable)
	
1.05 	INDICATR / INTERFACE
	A. Front					
	        1. LED Indicator			Power 1, Error 1, Record 1 
	B. Connections
	        1. HDMI / VGA 			1ea
	        2. Audio 				Out 2ea(Total), Main unit : Phone jack 1ea, 
Control box : RCA 1ea
	        3. Ethernet				RJ-45 Gigabit Ethernet 12ea (Total)
Network : 1ea, Control box : 2ea, I/O box : 1ea, 
PoE : 8ea
	        4. Alarm				In / Out - 8ea (Terminal block, NO / NC selectable)
	        5. USB				Front 3ea
	        6. GPS				MCX 1ea
	        7. Power Cord			Square 4pin connector 1ea

1.06	SYSTEM
	A. Log
	        1. Log List			Max. 20000 (System log, Event log, Back up log each)

1.07 	GENERAL
	A. Electrical
	         1. Input Voltage	 		12 ~ 24V AC
      	          2. Power consumption 		Total : max. 89W, Main unit : max. 25W
	Camera : Max. 64W (Max. 8W per channel, IEEE 802.3af class 2)
B. Environmental
	  1. Operating Temperature	-25°C ~ +50°C (-13°F ~ +122°F)
	  2. Operating Humidity	20% ~ 85% RH
C. Mechanical
	        1. Dimensions(WxHxD)		Main unit : 225.5 x 59.0 x 311.4mm 
(8.88" x 2.32" x 12.26") (1 DIN, Without bracket)
Control box : 121.0 x 32.0 x 75.0mm 
(4.76" x 1.26" x 2.95")
			I/O box : 155.0 x 44.0 x 70.0mm 
			(6.1" x 1.73" x 2.76")
	        2. Weight(1 x Hard Disks)		Main unit : 2.16Kg (4.76 lb) (Without HDD)
			Control box : 0.18Kg (0.4 lb),
			I/O box : 0.35Kg (0.77 lb)
D. Approvals
	  1. EMC / Safety	CE, FCC (Class A), cUL, e-Mark
	  2. EMC(Railway)	EN50121-3-2
	  3. Shock / Vibration (Railway)	EN61373
	  4. Safety(Railway)	EN50155
	  5. EMC(Railway)	EN50121-4
	  6. Shock(Functional Test)	MIL STD-810F method 516.5 procedure I
	  7. Vibration	MIL STD-810F method 514.5
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