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SRN-1000 64-CHANNEL NETWORK VIDEO RECORDER
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 – PRODUCTS

2.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with an explicit manufacturer warranty.

2.02	SRN-1000 64-CHANNEL NETWORK VIDEO RECORDER
A. The network video recorder (NVR) shall support up to 64 network cameras and shall be compatible with OVIF compliant network cameras. The NVR will have the throughput of 100mbps total.
B. The NVR shall support H.264, MPEG4 and MJPEG Multiple codec.
C. The NVR shall support the iPolis mobile viewer for iPhone and Android phone
D. All operation and configuration menus shall be provided in 22 languages including Korean,
Japanese, Chinese, English, French, German, Spanish, Italian, Russian, Polish, Czech,   Turkish, Dutch, Portuguese, Swedish, Danish, Thai, Romanian, Serbian, Croatian, Hungarian and Greek.

2.03	DISPLAY
A. N/W Camera
1. Inputs 				up to 64 network camera support
2. Resolution			CIF ~ 5F
3. Protocols 	Samsung, ONVIF(Axis, Sony, Panasonic)
B. LIVE
1. Multi Screen display	 1, 4, 9, 16, Sequence

2.04	PERFORMANCE	
 A. OS Embedded 			Linux
 B. Recording
1. Compression			H.264, MPEG4, MJPEG
2. Recording Bit Rate 		100Mbps
3. Mode				Manual, Schedule (Continuous/Event), 
					Event (Pre/Post)
	C. Search & Playback
	       1. Search mode			Date/time, Event
						(all search included in Preview)
	       2. Playback function 		Fast Forward/Backward, Move one step up, 
						Move one step down
	D. Network
	       1. Ethernet 				RJ-45, Gigabit Ethernet x2
	       2. Transmission speed 		Up to 64Mb
	       3. Remote users 			3 Search, 10 Live Unicast, 20 Live Multicast
	       4. Protocol support 			TCP/IP, UDP/IP, RTP(TCP), RTP(UDP), RTSP, NTP, 							HTTP, DHCP, PPPoE, SMTP, ICMP, IGMP, ARP, DNS, 							DDNS, UPnP, ONVIF
	       5. Monitoring 			Net-I Viewer, Webviewer
	E. Storage
	         1. Internal HDD 			Up to 8 SATA HDDs
	         2. External HDD 			eSATA interface(2 port)
	         3. File Format (Back-up) 		JPEG, AVI
	
2.05 	INTERFACE
	A. Audio
	         1. Inputs 				64CH (Network)
	         2. Compression 			G.711,  726
	B. Alarm
	         1. Inputs				 Terminal 16 inputs (NO/NC)
	         2. Outputs 			 Terminal 4 relay outputs (NO/NC), Terminal 1 reset    
	C. Connections
	        1. Ethernet 			2 RJ-45 10/100/1000 Base-T
	        2. e-SATA 				2 ports

2.06 	GENERAL
	A. Electrical
	         1. Input Voltage/Current 		100 ~ 240V AC ±10%, 50/60Hz, 4 ~ 1.5A
         2. Power consumption 	Max. 45W (154 BTU with 1 HDD),
			Max. 170W(580 BTU with 8 HDD)
B. Environmental
	  1. Operating Temperature	+0°C ~ +40°C (+32°F ~ +104°F)
	  2. Operating Humidity	20% ~ 85% RH
C. Mechanical
	  1. Dimensions(WxHxD)	440.0 x 88.0 x 426.8mm(17.32” x 3.46” x 16.80”)
	  2. Weight(1 x Hard Disks)	Approx. 6.2Kg(13.67lb)
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