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SRN-472S 4-CHANNEL NETWORK VIDEO RECORDER WITH POE SWITCH
TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

1.01	GENERAL
A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
[bookmark: _GoBack]C.	All systems and components shall be provided with an explicit manufacturer warranty.

1.02	SRN-472S 4-CHANNEL NETWORK VIDEO RECORDER WITH POE SWITCH
A. The network video recorder (NVR) shall support up to 4 network cameras and shall be compatible with ONVIF compliant network cameras. The NVR will have the throughput of 32mbps for recording and 32mbps for network transmission
B. The NVR shall support H.264 and MJPEG Multiple codec.
C. The NVR shall support the iPolis mobile viewer for iPhone and Android phone

1.03	DISPLAY
A. N/W Camera
1. Inputs 				Up to 4 network camera support
2. Resolution			CIF ~ 5M
3. Protocols 	Samsung, ONVIF
B. LIVE
1. Local Display	HDMI / VGA
	2. Multi Screen Display	Local monitor : 1, 4, Auto sequence 
		Web : 1, 4, Auto sequence

1.04	PERFORMANCE	
 A. OS Embedded 			Linux

 B. Recording
1. Compression			H.264, MJPEG
2. Recording Bit Rate 		Max. 32Mbps (2M 4CH real-time recording)
3. Mode				Normal, Scheduled, Event (Pre/Post)
4. Event Trigger			Alarm input(4), Video loss, Camera event
 					(Sensor, MD, Video analytics) 
5. Event Action			E-mail, PTZ preset, Alarm out, Buzzer, Monitor out
6. Resolution			CIF ~ 5M
	C. Search & Playback
	       1. Playback bandwidth		32Mbps(4Ch simultaneously)
	       2. Mode				Date & Time (Calendar) / Event log list
	       3. Simultaneous Playback		4CH(Local monitor, CMS), 4CH(Web,CMS)
	       4. Resolution			CIF ~ 5M
	       5. Playback Function		Fast forward, backward, Move one step up/ down
	D. Network
	       1. Transmission speed 		Min. 32Mbps
	       2. Remote users 			3 Search, 10 Live Unicast, 20 Live Multicast
	       3. Protocol support 			TCP/IP, UDP/IP, RTP (UDP), RTP (TCP), RTSP, NTP, 							HTTP, DHCP (Server, Client), PPPoE, SMTP, ICMP, 
I						GMP, ARP, DNS, DDNS, uPnP, HTTPS, SNMP, 
						ONVIF (Profile-S)
	       4. Viewer Software 			Type : SSM, Webviewer, SmartViewer
						CMS support : Support SDK / CGI
	       5. DDNS				Samsung Ipolis, DDNS
	       6. IP				IPv4/v6
	       7. Security				IP address Filtering, User access log, 802.1x 								authentication, Encryption
	       8. Language			English, French, German, Italian, Spanish, Russian, 							Turkish, Polish, Dutch, Swedish, Czech, Portuguese, 							 Danish, Rumanian, Serbian, Croatian, Hungarian, 							Greek, 	Norwegian, Finnish, Korean, Chinese, Japanese, 						Thai 
	       9. OS				Supported OS : Window XP (service pack 2 or above), 							Vista, 7, 8, Mac OS X (10.7 or above) 
	       10. Web Browser			[Internet Explorer] : ver.8 ~ 11, [Firefox] : ver.19.x or 							above [Chrome] : ver.26.x or above, [Safari] : ver.6.0.3 							or above (OSX 10.6 or above) 
	       11 Smart Phone			Platform : Android, IOS
						Max. Remote Users : Live 4, Playback 1 
	E. Storage
	         1. Built-in				1ea
2. Internal HDD 			2ea (Fixed)
	         3. Capacity			internal max. 8TB
	F. Back up				
	         1. File Back up			[USB] : BU/Exe, [Web, CMS] : JPEG, AVI
	         2. Function			Single channel play, Date-time/title display
	G. Sensor				4 / 3 (NO/NC selectable)
	H. Audio				Input : 4CH(Network), compression : G.711, G.726
						Audio Communication : 2-Way
	
1.05 	INTERFACE
	A. Front					
	        1. Indicator				Power status LED 1ea, HDD action LED 1ea, Alarm 							status LED 1ea, Record status LED 1ea, Network action 							LED 1ea, Back up LED 1ea
	         2. USB				2ea
	B. Alarm
	         1. Inputs				Terminal 4 inputs (Terminal block)
	         2. Outputs 			Terminal 3 outputs (Terminal block)
	C. Connections
	        1. Ethernet 			2ea(100Mbps) + PoE 4ea(10/100Mbps)
	        2. Audio 				Out 1ea(RCA, Line)
	        3. HDMI/VGA			1ea / 1ea
	        4. Power cord			1ea AC inlet
1.06	FUNCTIONS
	A. Camera Setup			
	        1. Register				PnP mode, Manual mode
	        2. Setup Items			 IP Address, Add Profile Edit, Bitrate, Compression, 							GOP, Quality, Video Setup 
						(MD, VA, ABF, Brightness/Contrast, Flip/Mirror, IRIS, 							WDR, D&N, SSNR, Shutter)
	B. PTZ					
	        1. Control				Via GUI, Webviewer
	        2. Preset				255
	        3. System Control			Mouse, IR Remocon

1.07	SYSTEM
	        1. Log				Log list : System log(Max. 20000)
							    Event log(Max. 20000)

1.08 	GENERAL
	A. Electrical
	         1. Input Voltage/Current 		100 ~ 240V AC / 3.5A 50Hz/60Hz
         2. NVR Power consumption 	Max 30W(With 1TB HDD 1ea)
	  3. Camera Power Output	15.4W per Channel, Total 61.6W(PoE, IEEE 802.3af)
B. Environmental
	  1. Operating Temperature	+0°C ~ +40°C (+32°F ~ +104°F)
	  2. Operating Humidity	20% ~ 85% RH
C. Mechanical
	  1. Dimensions(WxHxD)	370.0 x 44.0 x 320.0mm(14.57” x 1.73” x 12.6”)(1U)
	  2. Weight(1 x Hard Disks)	Approx. 2.73Kg(6.02lb) without HDD
	  3. Color / Material	Black / Metal
D. Approvals
	  1. Safety	UL, KC
	  2. EMC	CE, FCC, KCC, CCC, Gost-R


SRN-472S  A&E 2014
