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MODEL : 2M 4.3배 경량 방폭 네트워크 PTZ 카메라 (TNU-L2040E)


1. 개 요
TNU-L2040E는 자이로 센서를 적용한 4.3배 2M 경량 방폭 네트워크 PTZ 카메라 입니다

2. 제 원 
1) 촬상 소자 : 1/2.8” CMOS
2) 해상도 : 1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 800 x 448, 720 x 576, 720 x 480,640 x 480, 640 x 360, 320 x 240
3) 초점거리 :  2.8 ~ 12mm (4.3배) 줌 렌즈, 최대구경비 F1.4
4) 최소 지근거리 :  1.5m(Wide), 2.5m(Tele)
5) 최저조도 컬러 :  Color : 0.015 Lux (1/30 sec, F1.4), B/W: 0.0015 Lux (1/30 sec, F1.4)
6) 방폭기능 : 내압 : Ex db IIC T6 Gb (IECEx/ATEX/KCs), 분진 : Ex tb IIIC T85°C Db(IECEx/ATEX/KCs)
           사용 가능 지역 : Zone 1, 2 , 21, 22, 재질 : 스테인레스(SUS316L Polished), IP68
7) 화각 : H: 119.5°(Wide) ~ 27.9°(Tele)
8) 팬/틸트 범위 :  0°~350° / 0°~90°
9) 팬/틸트 속도 :  0.1°~60°/sec
10) 프리셋 정확도 :  +0.2° / Yes (E / W/ S / N / NE / NW / SE / SW)
11) 영상 흔들림 보정 지원(자이로센서 내장)
12) 지능형분석 : Tampering, Loitering, Directional detection, Fog detection, Virtual Line, Enter/Exit, Appear/Disappear, Audio detection, Face detection, Motion detection, Sound classification
13) Edge Storage  : Micro SD/SDHC/SDXC 2 slots (up to 512 GB) - Continuous recording (1st slot to 2nd slot) Motion images recorded in the SD/SDHC/SDXC memory card can be downloaded. NAS (Network Attached Storage), Local PC for instant recording
14) 알람 I/O : 입력 1개 / 출력 1개
15) 동작 온/습도 : -30°C~+55°C (-22°F~+131°F) / 90% RH 이하
16)전원 / 소비 전력  :  DC12V, PoE(IEEE802.3af, Class3)/ DC12V: 최대. 8.6W, PoE : 최대. 9.6W
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