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MODEL : Wisenet7 AI 2M 렌즈분리형 카메라 (XNB-6002)

1. 개 요
XNB-6002은 최신 Wisenet7 탑재 2M 해상도의 렌즈분리형 카메라 최적의 이미지를 제공합니다.  
2. 제 원 
1) 촬상소자     : 1/2.8형 CMOS 
2) 최저조도     :  SLA-T1080FA, 1.6mm fixed, F1.6, H 187, 컬러 0.03Lux(F1.6, 1/30초)
SLA-T2480A , 2.4mm fixed, F2.0, H 138/V73, 컬러 0.045Lux(F2.0, 1/30초)
SLA-T2480VA , 2.4mm fixed, F2.0, H 138/V73, 컬러 0.045Lux(F2.0, 1/30초)
                  SLA-T4680A , 4mm fixed, F2.5, H73/V39, 컬러 0.06Lux(F2.5, 1/30초), 
SLA-T4680VA , 4mm fixed, F2.5,H73/V39/D85, 컬러 0.06Lux(F2.5, 1/30초)
3) 보정기능     : Day&night(Electrical)/extreme WDR /HLC/BLC/ SSNR V/WiseNR
4) 영상흔들림   : 내장
5) 지능형 
- Analytic events : - Defocus/Motion/Tampering/Fog/Audio/ Face detection, Sound classification, 
Virtual area(Loitering/Intrusion/Enter/Exit/Appear/Disappear),  Virtual line(Crossing/Direction)
 - Business Intelligence :People counting, Queue management, Heatmap
 - Alarm Triggers :Analytics, Network disconnect, Alarm input, App event, Time schedule
6) 알람 입출력  : I/O 포트 각1개
7) 오디오       : 선택가능(마이크/라인입력)
	8) 비디오 압축 : H.265/H.264: Main/High, MJPEG, 유니캐스트(최대 20명) / 멀티캐스트
멀티 스트리밍(최대 10개 프로파일) 


9) 보안        : HTTPS(SSL) Login Authentication, Digest Login Authentication, IP Address Filtering
User access log, 802.1X Authentication(EAP-TLS, EAP-LEAP, EAP-PEAP MSCHAPv2), 
Device Certificate(Hanwha Techwin Root CA, pre-installed), Secure by default certificate,
HTPM (Hanwha Trusted platform module),Secure OS/Boot/Storage, Verify firmware forgery,
[bookmark: _GoBack]TPM 2.0 with FIPS 140-2 level2
10) Edge Storage    : Micro SD/SDHC/SDXC 1slot Max. 1TB
11) 응용 인터페이스  : ONVIF Profile S/G/T, SUNAPI(HTTP API), Wisenet open platform
12) 동작환경    : -10°C ~ +55°C / Less than 90% RH, 
13) 전원        : 10.5W(PoE), 8.6W(DC12V) 
14) 외관        : 사이즈 : 131.1(W)x33.5(H)x86(D)mm / 무게 : 0.42kg
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