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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com
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PART  1  PRODUCTS
1.01 EQUIPMENT
A. Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
B. [bookmark: _Toc173721624]Model: XNO-6120R
C. Alternates: None
1.02 GENERAL DESCRIPTION
A. Video Compression and Transmission – The camera shall have the following properties relating to the video signals it produces.
1. H.265, H.264 and MJPEG compression, each derived from a dedicated encoder and capable of being streamed independently and simultaneously
a. H.265 and H.264 –60 fps at all resolutions
b. MJPEG – frame rates up to 30 fps
2. The camera shall be able to configure up to 10 independent video stream profiles with differing encoding, quality, frame rate, resolution, and bit rate settings.
3. Resolution selections
a. 1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 800 x 448, 720 x 576, 720 x 480, 640 x 480, 640 x 360, 320 x 240
4. Simultaneous unicast access by up to 20 users
5. Multicast or unicast capable
6. Dynamic DNS (DDNS) support.
7. Smart Codec, Dynamic GOV and Dynamic FPS to efficiently manage bitrate of the video stream.
B. Camera – The camera device shall have the following physical and performance properties.
1. True day/night operation with removable IR cut filter
a. Low light level operation to 0.03 lux (color) and 0 lux (black and white)
2. Integral IR illumination, providing effective visibility of 70m (229.66ft)
3. 2D and 3D digital noise reduction
4. 32 privacy masking regions utilizing a polygon with 6 different coloring as below.
a. Grey / Green / Red / Blue / Black / White
b. Mosaic
5. True WDR up to 150dB
6. Hallway view with rotatable lens
C. Intelligence and Analytics – The camera shall have a suite of integral intelligent operations and analytic functions to include.
1. Motion detection with eight definable detection areas, minimum / maximum object size definition and a learning algorithm that ignores false alarms such as trees and waves on water.
2. Detection of logical events of specified conditions from the camera’s video and audio input
a. camera tamper (scene change)
b. loitering
c. directional detection
d. defocus detection
e. fog detection
f. virtual line
g. enter/exit
h. appear/disappear
i. audio detection
j. face detection
k. motion detection with link to other cameras
l. sound classification
D. Interoperability – The camera shall be ONVIF Profile S and G compliant.
E. The camera shall possess the following further characteristics.
1. Built-in web server, accessed via standard browsers including Internet Explorer, MS Edge, Firefox, Chrome & Safari
2. Two slots for micro SD/SDHC/SDXC memory card and NAS recording options, with configurable pre-alarm and post-alarm recording intervals. Maximum capacity for each slot is 512GB.
3. Bi-directional audio
4. Alarms and notifications
a. alarm notification triggers
1) alarm input
2) motion detection
3) intelligent audio and video analytics
4) network disconnection
b. available notification means upon trigger
1) file upload via FTP and e-mail
2) notification via e-mail
3) record to local storage (SD/SDHC/SDXC card)
4) NAS recording
5) external output
6) preset
5. Pixel Counter available in the plug-in web viewer.
6. POE capable
1.03 CAMERA SOFTWARE
A. The camera shall have a built in web server which supports browser-based configuration using Internet Explorer, MS Edge, Google Chrome, Mozilla Firefox, and Apple Safari, for which web viewer plug-ins are available, from a PC or Mac.
B. The web viewer shall provide a monitoring screen which displays live camera video and simultaneously provides same-screen access to the following functions.
1. Live view window size
2. Resolution setting
3. Image (snapshot) capture
4. Manual recording to SD or NAS
5. Audio/microphone control
6. Access Playback and Setup menus
C. The web viewer shall provide a playback screen which provides access to the following functions.
1. Search date and time range
2. Search event type
3. Play an event video
4. Set resolution
5. Play audio if present
6. Generate a backup copy of saved video data
D. The web viewer shall provide a setup screen which provides access to the following configuration settings and functions in the camera.
1. Digital video profile to include compression type, maximum or target bit rate, frame rate, multicast parameters, crop encoding area
2. User profile to include password, access level, authentication
3. Date and time
4. Network settings and IP version
a. DDNS
b. SSL, including certificate management
c. 802.1x authentication
d. Quality of Service settings
e. SNMP to include version selection and settings
f. Auto configuration
5. Video setup to include flip and mirror mode, hallway view mode, video type, privacy zone
6. Audio setup to include source, audio codec type, gain, and bit rate
7. Camera settings to include image preset, sensor frame capture, dynamic range, white balance, back light, exposure, day/night operation, on-screen display, sharpness, contrast, color level, lens distortion correction.
8. Event detection setup to include notification parameters, recording rules, time schedule, tamper protection, motion detection, event triggers
9. System function to include reboot, upgrade, check system and event logs, application (SDK) management
10. View profile information
E. Minimum client requirements
1. Acceptable Operating Systems: Windows 7 / 8.1 / 10, MAC OS X 10.10~10.12
2. Acceptable browsers: Microsoft Internet Explorer and Edge, Mozilla Firefox, Google Chrome, Apple Safari
1.04 DETAILED SPECIFICATIONS
A. Video
1. Imager
a. Sensor: 1/2.8" 2 MP CMOS
1) pixels per sensor: 1945 (H) x 1109 (V) total, 1945 (H) x 1097 (V) effective
2) scanning: progressive
b. Minimum illumination
1) Color mode: 0.03 Lux (F1.6, 1/30 sec)
2) Black & white mode: 0 Lux (IR LED On)
c. Signal to noise ratio: 50dB
d. Video out
1) CVBS: 1.0 Vp-p / 75 ohms Composite, 720x480(NTSC), 720x576(P)
2) USB: micro USB type B, 1280x720
e. The following features with control settings shall be available
1) Camera Title: Off / On (Displayed up to 85 characters)
a) W/W: English / Numeric / Special characters
b) China: English / Numeric / Special / Chinese characters
c) Common: Multi-line (Max. 5), Color (Grey/Green/Red/Blue/Black/White), Transparency, Auto scale by resolution
2) Day/night setting: Auto (ICR) / Color / BW / External / Schedule
3) Backlight compensation (BLC): Off / BLC / HLC (masking, dimming) / WDR
4) WDR: 150dB
5) Contrast Enhancement: Off / On
6) Digital Noise Reduction (DNR): Off / On (2D + 3D noise filter)
7) Digital Image Stabilization: Off / On
8) Defog: Off / On
9) Motion Detection: Off / On (8ea, 8 point polygonal zones) Link to other cameras
10) Privacy Masking: Off / On (32ea polygonal zones)
11) Gain Control: Off / Low / Middle / High
12) White Balance: ATW / AWC / Manual / Indoor / Outdoor (including Mercury and Sodium light)
13) LDC: Off / On (5 levels with min / max)
14) Electronic shutter speed: min, max, anti-flicker (2 ~ 1/2,000 sec)
15) Presets: 300ea
16) Image flip: Off / On
17) Image mirror: Off / On
18) Hallway view: Off / On (90°, 270°)
19) Video & Audio Analytics: tampering, loitering, directional detection, defocus detection, fog detection, virtual line, enter / exit, (Dis)Appear, audio detection, face detection, motion detection, sound classification
20) Alarm I/O: Input 1 / Output 1
21) Alarm Triggers: alarm input, motion detection, video & audio analytics, network disconnection
22) Alarm Events: File upload via FTP and E-mail, local storage recording at event, notification via E-mail, external output, preset
23) Pixel Counter: Available in the plug-in viewer.
f. Lens: 5.2 ~ 62.4 mm (Optical 12x)
1) Max. Aperture Ratio: F1.6 (Wide) ~ F3.0 (Tele)
2) Angle of View: H: 54.58° ~ 5.30° / V: 32.19° ~ 3.00° / D: 61.40° ~ 6.06°
3) Min. Object Distance: 1.5 m (4.92 ft.)
4) Focus Control: Auto, Manual, One shot auto focus
5) Lens Type: DC auto iris 
6) Mount Type: Board-in Type
2. Video Streams
a. The camera shall be able to produce 10 video profiles, each of which may have the following properties.
1) Encoding type.
a) H.265
b) H.264
c) MJPEG
2) Resolution: 1920 x 1080, 1280 x 1024, 1280 x 960, 1280 x 720, 1024 x 768, 800 x 600, 800 x 448, 720 x 576, 720 x 480, 640 x 480, 640 x 360, 320 x 240
3) Maximum frame rate
a) H.265 and H.264: Max. 60 fps at all resolutions
b) MJPEG: Max. 30 fps
4) Smart Codec: Manual mode, WiseStream, Dynamic GOV, Dynamic FPS
5) Bit rate control method
a) H.265 and H.264
i. target bitrate level control 
ii. constant bit rate (CBR) or variable bit rate (VBR)
b) MJPEG
i. target bitrate level control
ii. variable bit rate (VBR)
3. Number of multi-streaming profiles: 10 maximum
4. Simultaneous users (total): 20 maximum (unicast)
5. Storage and Recording
a. The camera shall have onboard SD card storage.
1) Card type: Micro SD/SDHC/SDXC
2) Capacity: Up to 512 GB
3) No. of slots: 2 (available for continuous recording)
4) Image content on the card shall have the ability to be downloaded to a selected destination.
b. NAS
c. Local PC for instant recording
6. Interoperability - Video streams shall be capable of supporting ONVIF protocol, profiles S and G.
7. Single Images - The camera shall support jpg file image screenshot and export.
B. Network
1. Connectivity: 10/100 Base-T Ethernet via RJ-45 connector
2. Protocols supported:
a. Transmission Control Protocol (TCP), Internet Protocol (IP) v4 and v6, User Datagram Protocol (UDP)
b. Configuration: Dynamic Host Configuration Protocol (DHCP)
c. Web services: Hypertext Transfer Protocol (HTTP), Secure HTTP (HTTPS)
d. Network services: Address Resolution Protocol (ARP), Bonjour, Domain Name System (DNS), Internet Control Message Protocol (ICMP), Network Time Protocol (NTP), Protocol Independent Multicast-Sparse Mode (PIM-SM), Simple Network Management Protocol (SNMP v1/2c/3 – MIB-2), Universal Plug and Play (UPnP)
e. Media: Real-Time Transport Protocol (RTP), Real-Time Control Protocol, Real-Time Streaming Protocol (RTSP)
f. Multicast: Internet Group Management Protocol (IGMP)
g. Notifications: File Transfer Protocol (FTP), Simple Mail Transfer Protocol (SMTP)
h. Remote Access: Point-to-Point Protocol over Ethernet) (PPPoE)
3. DDNS – The camera shall support DDNS services offered by the Manufacturer and other publicly available service offerings.
4. Quality of Service (QoS) – Layer 3 DSCP
5. Security features
a. user password protection
b. IP address filtering - list of allowed or blocked IP addresses 
c. HTTPS(SSL) login authentication
d. HTTPS(SSL) secured communications
e. Digest login authentication
f. User access log
g. 802.1x authentication
6. Discovery - Manufacturer shall offer a discovery program to identify all devices of his manufacture on the network.
7. Configuration – Manufacturer shall offer a configuration program that remotely allows users to change settings on multiple cameras simultaneously.
C. Audio
1. Direction: Bi-directional
2. Audio In
a. Selectable (MIC in / line in)
b. Supply voltage: 2.5V DC (4mA)
c. Input Impedance: approx. 2K Ohm
3. Compression
a. G.711 u-law/G.726 selectable
1) G.726 (ADPCM) 8KHz, G.711 8KHz
2) G.726: 16Kbps, 24Kbps, 32Kbps, 40Kbps
3) AAC-LC: 48Kbps at 8/16/32/48 kHz
D. Electrical
1. Power
a. Input Voltage / Current: PoE (IEEE802.3af Class 3), 12V DC, 24V AC
b. Power Consumption: <12.95 W (PoE), <12.5 W (12V DC), <14.5 W (24V AC)
E. Mechanical And Environmental
1. Material
a. Housing: Aluminum
2. Dimensions (W x H): 91.0 x 368.6 mm (3.58 x 14.51 in.)
3. Weight: 2.18Kg (4.81 lb.)
4. Temperature
a. Operating: -40° C to 55° C (-40° F to 131° F)
b. Storage: -50° C to 60° C (-58° F to 140° F)
5. Humidity: 0 - 90%, non-condensing
6. Environmental Rating
a. Mechanical (Impact) Protection: IK10
7. Ingress Protection: IP67, IP66, NEMA 4X
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