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[bookmark: _Toc334350683]Hanwha Vision is a global leading supplier of solutions for IP and analog video surveillance. Building on the company's history of innovation, Hanwha Vision is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-effectiveness. Hanwha Vision is committed to the continued development of innovative systems products for professional security applications.

For additional information, https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com

[bookmark: _Toc334350689]
 PRODUCTS
EQUIPMENT
Manufacturer: Hanwha Vision (https://www.hanwhavision.com/en/, https://hanwhavisionamerica.com)
Model: XNV-A9085R
Alternates: XNV-A8085R
GENERAL DESCRIPTION
Video Compression and Transmission – The camera shall have the following properties relating to the video signals it produces.
H.265, H.264 and MJPEG compression, each derived from a dedicated encoder and capable of being streamed independently and simultaneously. (See detailed specifications)
The camera shall be able to configure various resolution selections. (See detailed specifications)
The camera shall be able to configure up to 10 independent video stream profiles with differing encoding, quality, frame rate, resolution, and bit rate settings
The camera shall support unicast video streaming up to 20 users.
The camera shall support multiple streaming up to 5 profiles and 3 virtual channels.
The camera shall support multicast video streaming.
The camera shall be able to configure Dynamic DNS (DDNS). DDNS shall be provided with no additional cost by the manufacturer.
[bookmark: _Hlk197931251][bookmark: _Hlk197932097]The camera shall provide WiseStream based on AI engine to efficiently manage bit rate of the video stream and reduce storage.
The camera shall provide WiseNRⅡ, an AI-based feature to reduce noise and blur on image.
Camera – The camera device shall have the following physical and performance properties.
[bookmark: _Hlk197931280]True day/night operation with removable IR cut filter. The IR function shall provide manual power adjustment, automatic mode based on objects in the center of the screen, and automatic mode based on objects anywhere in the scene.
[bookmark: _Hlk197931300]The camera shall be able to produce clear images in high-contrast scenes with multi-exposure wide dynamic range up to 120dB. The WDR function shall include the following modes and options: On / Off, Automatic mode, Automatic mode based on low light, Automatic mode based on Black/White mode.  The WDR function shall provide 3 level adjustments.
The camera shall support digital noise reduction using both 2D and 3D noise reduction technology.
The camera shall be able to configure privacy masking areas with polygonal zones.
[bookmark: _Hlk197931315]The camera shall support mobile applications (iOS, Android) for remote viewing angle adjustment, rotation and focus control during installation.
The camera shall have a dual NPU capable of running all AI & analytics functions fully on one NPU while the other is available for ISP functions, including AI-based noise reduction, WDR, & low light image enhancements.
Intelligence and Analytics – The camera shall have a suite of intelligent analytic functions.
Classified object type: Person / Face / Vehicle / License plate
Attributes: Person (Gender, Clothing top/bottom color, Bag), Face (Age, Gender, Mask, Glasses), Vehicle (Type: car / bus / truck / motorcycle / bicycle, Color)
BestShot supported
Re-ID (Person) supported
Analytics events based on AI engine: Motion detection, Object detection, Virtual line(Crossing / Direction), Virtual area(Loitering / Intrusion / Enter / Exit / Appear / Disappear), Slip & Fall detection, Face mask detection, Social distancing detection
Analytics events: Defocus detection, Tampering, Shock detection, Audio detection
[bookmark: _Hlk197931375][bookmark: _Hlk197932618]Business Intelligence: People / Vehicle / Crowd counting, Queue management, Heatmap based on AI engine
The camera shall provide configurable Dynamic Privacy Masking feature with selectable mosaic or color masking.  Mosaic masking shall provide multiple pixilation options while color masking shall provide 8 color options.  Masking shall be available for any AI-based object type.  Masking shall be available at full resolution/frame rate on a selected channel, allowing a VMS to record both the original and masked video.
Interoperability
The camera shall be ONVIF Profile S, G, T and M compliant.
The camera shall be compatible with the Hanwha Vision Cloud Portal, including OnCloud VMS, HealthPro, and SightMind, utilizing the provided CloudConnector Open Platform application.
The camera shall be compatible with Hanwha Vision AI packs, utilizing Open Platform, to add additional AI functions.
Additional Features
Micro SD/SDHC/SDXC memory slot with configurable pre-alarm and post-alarm recording intervals
NAS recording option with configurable pre-alarm and post-alarm recording intervals
Alarm triggers and notifications
[bookmark: _Hlk197931432]Impact protection (IK10), Water & Dust protection (IP52)
Support Wisepower (Power monitoring & ECO mode)
The camera uses recycled plastic in construction
Device certificate (Hanwha Vision Root CA), Secure storage (Secure element with FIPS 140-3 level 3/CC EAL6+ certified), S-BOM
The camera shall feature an admin session timeout to prevent a webpage user from leaving access to the camera for longer than a specified period.
DETAILED SPECIFICATIONS
[bookmark: _Toc173721624]Video
Imaging device: 1/1.8" CMOS
Resolution: 3840x2160, 3328x1872, 3072x1728, 2592x1944, 2688x1512, 2560x1440, 1920x1080, 1600x1200, 1280x960, 1280x720, 1024x768, 800x600, 640x480, 640x360, 320x240, 320x180
Maximum Framerate
H.265/H.264: Max. 30fps(60Hz) / 25fps(50Hz)
MJPEG: Max. 30fps (at 8MP Max. 5fps)
Minimum Illumination
Color: 0.04Lux (F1.3, 1/30sec, 30IRE)
B/W: 0.004Lux (F1.3, 1/30sec, 30IRE), 0Lux(IR LED on)
Video Out (for Installation): Micro USB Type C
Lens
Focal length: 4.4 ~ 9.3mm (2.1x) motorized varifocal
Max. Aperture Ratio: F1.3(Wide) ~ F2.15(Tele)
Field of View
H:113°(Wide) ~ 47°(Tele)
V:58°(Wide) ~ 26°(Tele)
D:138°(Wide) ~ 54°(Tele)
Min. Object Distance: 0.5m (1.64ft)
Focus Control: Simple focus, manual
Lens Type: P-Iris(IR corrected)
Pan & Tilt & Rotate
Range: 0°~360° / 0°~85°/ 0°~355°
Operational Functions
Camera Title: Displayed up to 85 characters
Day/Night: Auto (ICR)
Backlight Compensation: BLC / HLC / WDR / SSDR
WDR(Wide Dynamic Range): extremeWDR 120dB
Digital Noise Reduction: SSNRⅤ, WiseNRⅡ(AI-based)
Digital Image Stabilization: Supported (built-in gyro sensor)
Defog: Supported
Motion Detection: 8 zones, each with 8-point polygonal shape
Privacy Masking
32 zones, each with 8-point polygonal shape
Color: gray/green/red/blue/black/white/purple/yellow
Mosaic
Dynamic Privacy Mask(Based on AI engine)
Color: gray/green/red/blue/black/white/purple/yellow
Mosaic
Gain Control: Off / Max Gain / Manual
White Balance: ATW / Narrow ATW / AWC / Manual / Indoor / Outdoor
Lens Distortion Correction: Supported (Fill / Stretch mode)
Electronic Shutter Speed
Min / Max / Anti-flicker (2 ~ 1/30,000sec)
Prefer shutter control (based on AI engine)
Video Rotation: Flip, Mirror, Hallway view (90° / 270°)
Analytics
Classified object type: Person / Face / Vehicle / License plate
Attributes: Person (Gender, Clothing top/bottom color, Bag), Face (Age, Gender, Mask, Glasses), Vehicle (Type: car / bus / truck / motorcycle / bicycle, Color)
BestShot supported
Re-ID (Person) supported
AI-based analytics events: Motion detection, Object detection, Virtual line(Crossing / Direction), Virtual area(Loitering / Intrusion / Enter / Exit / Appear / Disappear), Slip & Fall detection, Face mask detection, Social distancing detection
Analytics events: Defocus detection, Tampering, Shock detection, Audio detection
Business Intelligence: People / Vehicle / Crowd counting, Queue management, Heatmap based on AI engine
Alarm I/O
2 configurable I/O ports, DC 12V output(Max. 50mA)
Support extra alarm I/O via optional I/O box
Alarm Triggers: Analytics, Network disconnection, Alarm input, Time schedule, MQTT subscription, Day/Night Storage disruption, Case tampering
Alarm Events (When alarm trigger occurred)
File upload
image: e-mail/FTP/SFTP
video clip: FTP/SFTP
Notification: e-mail
Recording: SD/SDHC/SDXC or NAS recording at event triggers
Alarm output
Handover: PTZ preset, Send message by HTTP / HTTPS / TCP
Audio clip playback
MQTT: publication
Audio in: Selectable (mic in / line in)
Audio out: Line out
Light Type: IR LED (850nm)
[bookmark: _Hlk137643969]IR Viewable Length: WiseIR
[bookmark: _Hlk197931852]PoE+: 50m(164.04ft)
PoE: 30m(98.43ft)
Edge Storage
Micro SD/SDHC/SDXC 2TB (1TB x 2 slots), NAS support
Memory: 4GB RAM, 8GB eMMC
Webpage Language: English, Korean, Simplified Chinese, Traditional Chinese, French, Italian, Spanish, German, Japanese, Russian, Portuguese, Czech, Polish, Turkish, Dutch, Hungarian, Greek
Network
Ethernet: Metal shielded RJ-45 (10/100/1000 BASE-T)
Video compression
H.265/H.264: Main / Baseline / High
MJPEG
Audio Compression
G.711(PCM): 8kHz(64Kbps)
G.726(ADPCM): 8kHz(16/24/32/40Kbps)
AAC-LC: 16kHz(48Kbps)
OPUS: 48kHz(64Kbps)
Smart Codec: WiseStream (Based on AI engine)
Bitrate Control
H.265 / H.264: CBR or VBR
MJPEG: VBR
Streaming
Unicast(20 users) / Multicast
Multiple streaming (Up to 5 profiles, 3 virtual channel support)
Profile set: Max. 10 profiles
Application Programming Interface
ONVIF Profiles S, G, T, M
SUNAPI (HTTP API)
Hanwha Vision Open Platform
Protocol
Network: IPv4, IPv6, TCP/IP, UDP/IP
Streaming: RTP(UDP), RTP(TCP), RTCP, RTSP, SRTP
Services: NTP, HTTP, HTTPS, SSL/TLS, DHCP, DNS, DDNS
File Transfer: FTP/SFTP, SMTP(StartTLS)
Management: SNMPv1/v2c/v3(MIB-2), IGMP, UPnP, Bonjour, LLDP
Other: ICMP, ARP, QoS, CDP, MQTT, Syslog
DDNS – The camera shall support DDNS services offered by the manufacturer and others publicly available service offerings
QoS – Layer 3 DSCP
Security Feature
OS / Firmware Protect: Encrypted Firmware, Secure boot, Signed Firmware
User authentication: Digest Authentication, Prevent brute-force attack
Network authentication: IEEE 802.1X (EAP-TLS, EAP-LEAP, EAP-PEAP, MSCHAPv2)
Secure Communication: HTTPS, SRTP, WSS (WebSocket Secure)
Access Control: IP-based access control, MAC-based access control, Auto logout
Data Protect: Encryption Credentials, Encrypt compress for live recording file export
Audit: Access / System / Event Log management
Device ID: Device certificate (Hanwha Vision Root CA)
Secure Storage: Secure element, SD card partition encrypt
[bookmark: _Hlk197931491][bookmark: _Hlk197931906]Security Certificate: ETSI EN 303 645, Secure element (FIPS 140-3 level 3, CC EAL6+)
The device shall not provide a manufacturer default password. Default password change shall be required to access the camera.
A minimal level of password complexity shall be required by the camera.
The camera shall not have a manufacturer back-door password.
The manufacturer shall provide a tool that provides the ability to make password changes to multiple cameras at the same time. 
[bookmark: _Hlk197931509]Network filtering – The camera shall allow a list of allowed or blocked IP addresses/subnet mask and/or MAC addresses to be entered to restrict access to the device.
Discovery – The manufacturer shall offer a discovery program to identify all their devices on the network. 
Configuration – The manufacturer shall offer a configuration program that remotely allows users to change settings on multiple cameras simultaneously.
Firmware upgrade – The manufacturer shall offer a program capable of upgrading multiple cameras at the same time (not requiring access to individual cameras).
Camera backup setting – The manufacturer shall provide a program that provides the ability to save multiple camera settings to a file and restore these camera settings if needed.
Reporting – The manufacturer shall provide a tool that can generate a report including thumbnail view, MAC address, IP address, serial number and other camera settings.
Environmental & Electrical
[bookmark: _Hlk148096344]Temperature
-50°C to +60°C (-58°F to +140°F)
Startup should be done at above -30°C (-22°F)
+74°C (+165°F)(Max) based on NEMA-TS 2(2.2.7)
Humidity
Operating Condition
0 ~ 100% RH(Condensing)
Humidity control with AIR vent
Storage Condition
0 ~ 100% RH(Condensing)
EPA(Effective Projected Area): 0.017㎡
Certification: IP66/IP67/IP6K9K, NEMA4X, IK11, NEMA-TS 2(2.2.7.2-8, 2.2.8, 2.2.9)
Input Voltage
PoE+ (IEEE802.3at type 2, class 4)
PoE (IEEE802.3af, class 3)
12V DC
Power Consumption
PoE+: Max. 14.2W, typical 9.4W
PoE: Max. 12.9W, typical 8.3W
12V DC: Max. 9.5W, typical 14.5W
Support Wisepower: Power monitoring (Max./Current/Avg.)
Mechanical
Color: White
Material: Aluminum
Bubble: Hard-coated dome
RAL Code: RAL9003
Dimensions (Width x Height): ø180 x 125mm (ø7.09 x 4.92")
Weight: 1.860Kg(4.10lb)
Compatible Conduit hole / Gang box
Conduit: 19.1mm(3/4") (M25)
Gang box: Single, double, 4" octagon, 4" square
Certifications & Standards
EMC 
FCC 47 CFR Part 15 Subpart B Class A
ICES-3(A)/NMB-3(A)
CE/UKCA: EN 55032 Class A, EN 50130-4, EN 61000-3-2, EN 61000-3-3
VCCI CISPR 32 Class A
RCM AS/NZS CISPR 32 Class A
KS C 9832 Class A, KS C9835
Safety
UL 62368-1, CAN/CSA C22.2 NO.62638-1
IEC/EN 62471
Environment
IEC/EN 63000
IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA-TS 2(2.2.7.2-8, 2.2.8, 2.2.9)
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Compatible Models
Hanging Adaptor: SBP-180HMW1
Back Box: SBV-180BW, SBV-180WW
Ceiling Mount(Assy): SBP-150CMI, SBP-300CMI, SBP-300CMW1, SBP-900CMW, SBP-300CMTW, SBP-300CMTS
Ceiling Mount(Single Unit): SBP-180CMB, SBP-140CMB, SBP-180CMS, SBP-900CMP, SBP-300CMP, SBP-150CMP, SBP-C15P, SBP-C15H
Wall Mount: SBP-400WMW, SBP-250WMW, SBP-300WMW, SBP-300WMW1
Pole Mount: SBD-180PMW, SBP-300PMW2
[bookmark: _Hlk214039527]In-ceiling Mount: SHD-1370FPW, SHD-1350FPW
Corner Mount: SBP-156KMsdaW, SBP-300KMW, SBD-180KMA
Parapet Mount: SBP-156LMW1, SBP-300LMW
Cabinet: SBP-150NBW, SBP-300NBW
Interface Box: SPM-4210
Other Compatible Models: SBP-VAN85W, SBP-115PFA
DORI Distance
Detect (25PPM / 8PPF): Wide 50.8m(166.77ft) / Tele 176.6m(579.49ft)
Observe (63PPM / 19PPF): Wide 20.3m(66.71ft) / Tele 70.7m(231.80ft) 
Recognize (125PPM / 38PPF): Wide 10.2m(33.35ft) / Tele 35.3m(115.90ft)
Identify (250PPM / 76PPF): Wide 5.1m(16.68ft) / Tele 17.7m(57.95ft)
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